;/****************************************************************************
; * Copyright 2009 Atheros Communications Inc., all rights reserved.          *
; *                                                                           *
; * Copyright (c) 2011 Qualcomm Atheros, Inc.                                 *
; * All Rights Reserved.                                                      *
; * Qualcomm Atheros Confidential and Proprietary.                            *
; *                                                                           *
; * INF file for Atheros reference designs                                    *
; ****************************************************************************/

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHEROS%
CatalogFile = athwb.cat
DriverVer   = 10/17/2013,10.0.0.270

[Manufacturer]
%ATHEROS%     = Atheros, NTX86.6.2
%GIGABYTE%    = Gigabyte, NTX86.6.2

[ControlFlags]
ExcludeFromSelect = *
;
; OS 6.2 Manufacturer section
;
[Atheros.NTX86.6.2]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
;legacy HW Entries
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_FF19
%ATHR.DeviceDesc.ospsim%   = ATHR_DEV_OS61_OSPEMU.ndi,   PCI\VEN_168C&DEV_FE30
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_ABCD
%ATHR.DeviceDesc.osprey%   = ATHR_DEV_OS61_OSPREY.ndi,   PCI\VEN_168C&DEV_0030
%ATHR.DeviceDesc.9580%     = ATHR_DEV_OS61_9580.ndi,     PCI\VEN_168C&DEV_0033
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_9485.ndi,     PCI\VEN_168C&DEV_0032&SUBSYS_3118168C
%ATHR.DeviceDesc.1111%     = ATHR_DEV_OS61_1111.ndi,     PCI\VEN_168C&DEV_0037&SUBSYS_3118168C
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119.ndi,     PCI\VEN_168C&DEV_0032&SUBSYS_3119168C
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119.ndi,     PCI\VEN_168C&DEV_0032&SUBSYS_3122168C
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_3112168C
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_3113168C
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_3114168C
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_3116168C
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_ABCD&SUBSYS_00000000
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946x.ndi,     PCI\VEN_168C&DEV_0034&SUBSYS_3117168C
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956x.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_3025168C
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956x.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_3026168C
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_3027168C.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_3027168C
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_3028.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_3028168C
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956x.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_302B168C
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_3027168C.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_302C168C
%ATHR.DeviceDesc.1030%     = ATHR_DEV_OS61_1030.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1030168C
%ATHR.DeviceDesc.2030%     = ATHR_DEV_OS61_2030.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2030168C
%ATHR.DeviceDesc.1031%     = ATHR_DEV_OS61_1031.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1031168C
%ATHR.DeviceDesc.2031%     = ATHR_DEV_OS61_2031.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2031168C
%ATHR.DeviceDesc.1041%     = ATHR_DEV_OS61_1041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1041168C
%ATHR.DeviceDesc.2041%     = ATHR_DEV_OS61_2041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2041168C
%ATHR.DeviceDesc.1042%     = ATHR_DEV_OS61_1042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1042168C
%ATHR.DeviceDesc.2042%     = ATHR_DEV_OS61_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2042168C
%ATHR.DeviceDesc.1051%     = ATHR_DEV_OS61_1051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1051168C
%ATHR.DeviceDesc.2051%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2051168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_1052.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_1052168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_2052.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_2052168C
%ATHR.DeviceDesc.1053%     = ATHR_DEV_OS61_1053.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1053168C
%ATHR.DeviceDesc.2053%     = ATHR_DEV_OS61_2053.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2053168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_1054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_1054168C
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_2054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_2054168C
%ATHR.DeviceDesc.1062%     = ATHR_DEV_OS61_1062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1062168C
%ATHR.DeviceDesc.2062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2062168C
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_1063.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1063168C
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_2063.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2063168C
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3062168C
%ATHR.DeviceDesc.3063%     = ATHR_DEV_OS61_2063.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3063168C
%ATHR.DeviceDesc.3061%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3061168C
%ATHR.DeviceDesc.3065%     = ATHR_DEV_OS61_2052.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3065168C
%ATHR.DeviceDesc.2061%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2061168C
%ATHR.DeviceDesc.1061%     = ATHR_DEV_OS61_1051.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1061168C
%ATHR.DeviceDesc.2065%     = ATHR_DEV_OS61_2052.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_2065168C
%ATHR.DeviceDesc.1065%     = ATHR_DEV_OS61_1052.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1065168C
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3067168C
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_3064.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_3064168C
%ATHR.DeviceDesc.2055%     = ATHR_DEV_OS61_2055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_2055168C
%ATHR.DeviceDesc.2055%     = ATHR_DEV_OS61_1055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_1055168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1025168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1026168C
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_2026168C
%ATHR.DeviceDesc.1071%     = ATHR_DEV_OS61_1071.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_1071168C
%ATHR.DeviceDesc.1071%     = ATHR_DEV_OS61_1071.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_2071168C
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_1072168C
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_2072168C
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_3072168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3091168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3092168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3093168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3094168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3095168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3096168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3097168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3098168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_3099168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309A168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309B168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309C168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_309D168C.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309D168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_309F168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2091168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2092168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091PB.ndi,   PCI\VEN_168C&DEV_0029&SUBSYS_2093168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2094168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2096168C
%ATHR.DeviceDesc.2091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_0029&SUBSYS_2098168C
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30A1168C
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30A2168C
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AB168C
%ATHR.DeviceDesc.30AD%     = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AD168C
%ATHR.DeviceDesc.30AE%     = ATHR_DEV_OS61_30AA.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AE168C
%ATHR.DeviceDesc.30AF%     = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_30AF168C
%ATHR.DeviceDesc.30B0%     = ATHR_DEV_OS61_30B0.ndi,     PCI\VEN_168C&DEV_002E&SUBSYS_30B0168C
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_30A3168C
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_002C&SUBSYS_30A7168C
%ATHR.DeviceDesc.2099%     = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002D&SUBSYS_2099168C
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_30A4.ndi,     PCI\VEN_168C&DEV_002E&SUBSYS_30A4168C
; Customer X
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_A527167D
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_7125144F.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_04291468
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_04301468
%ATHR.DeviceDesc.2055%     = ATHR_DEV_OS61_2055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_720B1799
%ATHR.DeviceDesc.2055%     = ATHR_DEV_OS61_2055.ndi,     PCI\VEN_168C&DEV_001D&SUBSYS_B2031113
; Foxconn
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_04221468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04221468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_04221468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04171468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_04221468.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_04181468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_04221468.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_04201468
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_E023105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E023105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_E036105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E036105B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_E029105B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_E029105B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_E029105B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_1029105B
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_E033105Bw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_E033105B
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_E064105B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_661711AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E062105B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_661811AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E063105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_S30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E070105B
%ATHR.DeviceDesc.311711AD% = ATHR_DEV_OS61_1186788.ndi,  PCI\VEN_168C&DEV_0034&SUBSYS_E07D105B
; Apple
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_008F106B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_008F106B
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_009A106B
; Linksys
%ATHR.DeviceDesc.1737_g%   = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_00531737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_00431737
%ATHR.DeviceDesc.0044%     = ATHR_DEV_OS61_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_00441737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00351731
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00351737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00171737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00251737
%ATHR.DeviceDesc.1737_bg%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1026168C
%ATHR.DeviceDesc.1737_abg% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_00361737
; Siemens
%ATHR.DeviceDesc.800118CB% = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_800118CB
%ATHR.DeviceDesc.3070%     = ATHR_DEV_OS61_1042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_307002FA
%ATHR.DeviceDesc.3071%     = ATHR_DEV_OS61_1042.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_307102FA
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_662111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_662111AD
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_662211AD.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_662211AD
;Accton
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_75191113
; AMD
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091amd.ndi,  PCI\VEN_168C&DEV_002A&SUBSYS_1130168C
; Netgear
%ATHR.DeviceDesc.90001385% = ATHR_DEV_OS61_90001385.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_90001385
%ATHR.DeviceDesc.4B001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4B001385
%ATHR.DeviceDesc.4B001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5B001385
%ATHR.DeviceDesc.5D001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5D001385
%ATHR.DeviceDesc.4D001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4D001385
%ATHR.DeviceDesc.4F001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_4F001385
%ATHR.DeviceDesc.5E001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5E001385
%ATHR.DeviceDesc.4D001385% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_5A001385
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_46101385
; OQO
%ATHR.DeviceDesc.2062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1602196f
%ATHR.DeviceDesc.2062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_1603196f
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_1604196f
;Lenovo Japan
%ATHR.DeviceDesc.5013%     = ATHR_DEV_OS61_5013.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0034168c
%ATHR.DeviceDesc.6013%     = ATHR_DEV_OS61_6013.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_0035168c
%ATHR.DeviceDesc.3013%     = ATHR_DEV_OS61_3013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_05891014
%ATHR.DeviceDesc.4013%     = ATHR_DEV_OS61_4013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_058A1014
%ATHR.DeviceDesc.2013%     = ATHR_DEV_OS61_2013.ndi,     PCI\VEN_168C&DEV_1014&SUBSYS_057E1014
%ATHR.DeviceDesc.1013%     = ATHR_DEV_OS61_1013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_04081468
%ATHR.DeviceDesc.0032168c% = ATHR_DEV_OS61_0032168c.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_0032168c
%ATHR.DeviceDesc.0033168c% = ATHR_DEV_OS61_0033168c.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_0033168c
%ATHR.DeviceDesc.0036%     = ATHR_DEV_OS61_0036.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_0036168c
%ATHR.DeviceDesc.0037%     = ATHR_DEV_OS61_0037.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0037168c
; Lenovo China
%ATHR.DeviceDesc.309917AA% = ATHR_DEV_OS61_309917AA.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309917AA
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_316417AA.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_316417AA
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_309D17AA.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309D17AA
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A117AA.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_30A117AA
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A117AAw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_31A117AA
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_30A417AA.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_30A417AA
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_30A417AAw.ndi,PCI\VEN_168C&DEV_002E&SUBSYS_31A417AA
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30A117AAw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_30AB185F
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_311817AA.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_311817AA
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_321817AA.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_321817AA
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_321917AA.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_321917AA
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_311417AA.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_311417AA
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_321417AA.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_321417AA
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_00911969.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_00911969
%ATHR.DeviceDesc.302617AA% = ATHR_DEV_OS61_302617AA.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_302617AA
%ATHR.DeviceDesc.302617AA% = ATHR_DEV_OS61_302617AA.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_402617AA
; QCA Killer
%ATHR.DeviceDesc.k1202%    = ATHR_DEV_OS61_K1202.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_20031A56
%ATHR.DeviceDesc.k1103%    = ATHR_DEV_OS61_K110x.ndi,    PCI\VEN_168C&DEV_0030&SUBSYS_20011A56
%ATHR.DeviceDesc.k1102%    = ATHR_DEV_OS61_K110x.ndi,    PCI\VEN_168C&DEV_0030&SUBSYS_20001A56
; IBM
%ATHR.DeviceDesc.0033168c% = ATHR_DEV_OS61_03841014.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_03841014
; Samsung
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7101144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7114144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_S001A.ndi,    PCI\VEN_168C&DEV_001A&SUBSYS_7115144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_7131144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_7130144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_S001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7108144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_S001B.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_7116144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_E00B105B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_S3067b.ndi,   PCI\VEN_168C&DEV_001C&SUBSYS_E00C105B
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_S3067.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_E00E105B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_E00F105B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_E010105B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091SF.ndi,   PCI\VEN_168C&DEV_002A&SUBSYS_7161144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7167144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E025105B
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_30A1w.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E032105B
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30A1w.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7178144F
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30A1w.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_30B2185F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7187144F
%ATHR.DeviceDesc.30B0%     = ATHR_DEV_OS61_30B07189.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_7189144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_4101144D
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1a.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_4114144D
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30A1w.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_4102144D
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30A1w.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_4103144D
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30A1w.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_4104144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_4105144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_4106144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_410D144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_410E144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_410F144D
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_4107144D.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_4107144D
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_4107144D.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_4108144D
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_4107144D.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_4109144D
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_4107144D.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_410A144D
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_4107144D.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_410B144D
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_4107144D.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_410C144D
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_9485s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_4115144D
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_9485s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_4116144D
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_9485s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_4117144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_4110144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_4111144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_4112144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_4113144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_C0F9144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_C0E8144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_C0E6144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_411F144D
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946xs.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_4120144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_C706144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_C680144D
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119s.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_C708144D
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956xs.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_411A144D
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956xs.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_411B144D
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956xs.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_411C144D
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956xs.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_411D144D
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956xs.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_411E144D
; Option
%ATHR.DeviceDesc.00231931% = ATHR_DEV_OS61_30A1op.ndi,   PCI\VEN_168C&DEV_002B&SUBSYS_00231931
; D-Link
%ATHR.DeviceDesc.DWA642%   = ATHR_DEV_OS61_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A6A1186
%ATHR.DeviceDesc.DWA645%   = ATHR_DEV_OS61_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A0907D1
%ATHR.DeviceDesc.DWA645%   = ATHR_DEV_OS61_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A761186
%ATHR.DeviceDesc.DWA645%   = ATHR_DEV_OS61_3A7B1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A791186
%ATHR.DeviceDesc.DWA542%   = ATHR_DEV_OS61_3A691186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A691186
%ATHR.DeviceDesc.DWA547%   = ATHR_DEV_OS61_3A6D1186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A6B1186
%ATHR.DeviceDesc.DWA547%   = ATHR_DEV_OS61_3A7A1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A781186
%ATHR.DeviceDesc.DWA652%   = ATHR_DEV_OS61_1186.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_3A6E1186
%ATHR.DeviceDesc.DWA652%   = ATHR_DEV_OS61_3A7B1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A7B1186
%ATHR.DeviceDesc.DWA552%   = ATHR_DEV_OS61_3A6D1186.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_3A6D1186
%ATHR.DeviceDesc.DWA552%   = ATHR_DEV_OS61_3A7A1186.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_3A7A1186
%ATHR.DeviceDesc.DWA643%   = ATHR_DEV_OS61_3A6F1186.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_3A6F1186
%ATHR.DeviceDesc.DWA556%   = ATHR_DEV_OS61_3A701186.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_3A701186
%ATHR.DeviceDesc.G650%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A121186
%ATHR.DeviceDesc.G520X%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_32031186
%ATHR.DeviceDesc.G520%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A131186
%ATHR.DeviceDesc.AG520%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A081186
%ATHR.DeviceDesc.AG530%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A141186
%ATHR.DeviceDesc.G630%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A151186
%ATHR.DeviceDesc.G510%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A161186
%ATHR.DeviceDesc.AG650%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A071186
%ATHR.DeviceDesc.AG660%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A631186
%ATHR.DeviceDesc.G680%     = ATHR_DEV_OS61_3A171186.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_3A171186
%ATHR.DeviceDesc.G550%     = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A181186
%ATHR.DeviceDesc.AG660B%   = ATHR_DEV_OS61_3A171186.ndi, PCI\VEN_168C&DEV_001B&SUBSYS_3A191186
%ATHR.DeviceDesc.AG530B%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_3A221186
%ATHR.DeviceDesc.G650P%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A241186
%ATHR.DeviceDesc.G520P%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A231186
%ATHR.DeviceDesc.WDA1320%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3A1D1186
%ATHR.DeviceDesc.WDA2320%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A1B1186
%ATHR.DeviceDesc.DWA520%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A731186
%ATHR.DeviceDesc.DWA620%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A741186
%ATHR.DeviceDesc.CWNA2330% = ATHR_DEV_OS61_3A171186.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_3A1A1186
%ATHR.DeviceDesc.CWNA1330% = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3A1C1186
%ATHR.DeviceDesc.CWNA1330% = ATHR_DEV_OS61_3A171186.ndi, PCI\VEN_168C&DEV_001A&SUBSYS_3A1C1186
%ATHR.DeviceDesc.CG650%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_32021186
%ATHR.DeviceDesc.CG630%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_3B081186
%ATHR.DeviceDesc.CG630%    = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_3B081186
; Alpha/ATKK
%ATIWC.DeviceDesc.ATICB%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_12041259
%ATIWC.DeviceDesc.ATIPC%   = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_12031259
%ATHR.DeviceDesc.DWA566%   = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_3A7E1186
%ATHR.DeviceDesc.TEW726%   = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_3ABE1948
; Motion Computing
%ATHR.DeviceDesc.3061%     = ATHR_DEV_OS61_7111144F.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_7111144F
; Azurewave
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_10341A3B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10261A3B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10601A3B
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_10241A3B.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_10241A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_10671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10671A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_10711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10711A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_10711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10811A3B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_10891A3B
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_1D891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_1D891A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_10671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_10901A3B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_20371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_11061A3B
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_1A671A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1A671A3B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_1A891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_1A891A3B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_11121A3B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_11121A3B
%ATHR.DeviceDesc.30A7%     = ATHR_DEV_OS61_11121A3B.ndi, PCI\VEN_168C&DEV_002C&SUBSYS_1A121A3B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_10261A3B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_10331A3B
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_20361A3B
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB2C37.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_2C371A3B
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_11211A3B.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_11211A3B
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_1A211A3B.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_1A211A3B
%ATHR.DeviceDesc.2A371A3B% = ATHR_DEV_OS61_2A371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_2A371A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_2C971A3B_2.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_2C971A3B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_11861A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_CUS198.ndi,   PCI\VEN_168C&DEV_0032&SUBSYS_20861A3B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_1F861A3B
%ATHR.DeviceDesc.11951A3B% = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_11951A3B
%ATHR.DeviceDesc.11951A3B% = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_1F951A3B
%ATHR.DeviceDesc.21001A3B% = ATHR_DEV_OS61_2C971A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_21001A3B
%ATHR.DeviceDesc.11951A3B% = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0037&SUBSYS_11951A3B
%ATHR.DeviceDesc.11951A3B% = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0037&SUBSYS_1F951A3B
%ATHR.DeviceDesc.21001A3B% = ATHR_DEV_OS61_2C971A3B.ndi, PCI\VEN_168C&DEV_0037&SUBSYS_21001A3B
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_651311AD.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_11731A3B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_118C1A3B1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_118C1A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_209C1A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_209C1A3B
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_21101A3B.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_21101A3B
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_850E1043.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_211C1A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_CUS198_1.ndi,   PCI\VEN_168C&DEV_0032&SUBSYS_12371A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_CUS198_1.ndi,   PCI\VEN_168C&DEV_0032&SUBSYS_21261A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_20971A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_20971A3B
; Huawei
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5003485
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5013485
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_663111AD.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A5023485
; Panasonic
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_1C711A3B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1C711A3B
; QMI    
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_01121A32                        
%ATHR.DeviceDesc.3065%     = ATHR_DEV_OS61_01001A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01001A32
%ATHR.DeviceDesc.3063%     = ATHR_DEV_OS61_01001A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_02001A32
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_05021A32
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03011A32
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_05041A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_21081A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01051A32 
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_2A97103C
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01121A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01121A32
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_05071A32
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_03091A32.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_03091A32
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_03051A32w.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_23001A32
; Arcadyan
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_01051A32.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_C6011113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_D8111113.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_D8111113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_F6111113
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_C8231113
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_C8221113
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_D8221113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_03051A32w.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_98111113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A0111113
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_9485.ndi,     PCI\VEN_168C&DEV_0032&SUBSYS_F8421113
; Askey/Compal
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7168144F
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_2C971A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_40011C56
; LiteOn
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_630311AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_631311AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_6313.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_633311AD
%ATHR.DeviceDesc.2061%     = ATHR_DEV_OS61_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_530111AD
%ATHR.DeviceDesc.2062%     = ATHR_DEV_OS61_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_540111AD
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_661311AD
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_660311AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_654211AD
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_665111AD
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_651311AD.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_651311AD
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_652311AD.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_652311AD
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_30A417AAw.ndi,PCI\VEN_168C&DEV_002E&SUBSYS_660711AD
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_11861A3B.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_662711AD
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_2C971A3B_2.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_662811AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_321417AAA.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_663111AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_664111AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_664111AD
%ATHR.DeviceDesc.661811AD% = ATHR_DEV_OS61_661811AD.ndi, PCI\VEN_168C&DEV_0037&SUBSYS_661811AD
%ATHR.DeviceDesc.661711AD% = ATHR_DEV_OS61_661711AD.ndi, PCI\VEN_168C&DEV_0037&SUBSYS_661711AD
%ATHR.DeviceDesc.E059105B% = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_665111AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_CUS217.ndi,   PCI\VEN_168C&DEV_0034&SUBSYS_666111AD
%ATHR.DeviceDesc.H3119%    = ATHR_DEV_OS61_661711ADPCIE_1_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_664711AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956x.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_062211AD
%ATHR.DeviceDesc.311711AD% = ATHR_DEV_OS61_1186788.ndi,  PCI\VEN_168C&DEV_0034&SUBSYS_080211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_21301A3B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_065211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_067211AD_PCIE_1_1.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_067211AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_081211AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_081211AD
; Acer
%ATHR.DeviceDesc.E006105B% = ATHR_DEV_OS61_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_660011AD 
%ATHR.DeviceDesc.E006105B% = ATHR_DEV_OS61_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E006105B
%ATHR.DeviceDesc.E006105B% = ATHR_DEV_OS61_E006105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03031A32
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_OS61_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E01F105B
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_OS61_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_663211AD
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_OS61_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_03061A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_01081A32   
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04281468
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E008105B
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E00D105B
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_663111AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_635311AD
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_04281468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_660311AD
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E016105B
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E022105B
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_OS61_E01F105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_309D185F
%ATHR.DeviceDesc.E031105B% = ATHR_DEV_OS61_E031105Bw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_E031105B
%ATHR.DeviceDesc.660311AD% = ATHR_DEV_OS61_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_660311AD
%ATHR.DeviceDesc.660311AD% = ATHR_DEV_OS61_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_23091A32
%ATHR.DeviceDesc.660311AD% = ATHR_DEV_OS61_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_E034105B
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_23051A32
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_E035105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E035105B
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_E035105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_664111AD
%ATHR.DeviceDesc.663111AD% = ATHR_DEV_OS61_E035105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_63051A32
%ATHR.DeviceDesc.E01F105B% = ATHR_DEV_OS61_664211AD.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_664211AD
%ATHR.DeviceDesc.660311AD% = ATHR_DEV_OS61_660311AD.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_30B4185F
%ATHR.DeviceDesc.655211AD% = ATHR_DEV_OS61_655211AD.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_655211AD
%ATHR.DeviceDesc.661711AD% = ATHR_DEV_OS61_661711AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_661711AD
%ATHR.DeviceDesc.661711AD% = ATHR_DEV_OS61_661711AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E047105B
%ATHR.DeviceDesc.E04A105B% = ATHR_DEV_OS61_E04A105B.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_E04A105B
%ATHR.DeviceDesc.661811AD% = ATHR_DEV_OS61_661811AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_661811AD
%ATHR.DeviceDesc.661811AD% = ATHR_DEV_OS61_661811AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E04D105B
%ATHR.DeviceDesc.E051105B% = ATHR_DEV_OS61_661811AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E051105B
%ATHR.DeviceDesc.661711AD% = ATHR_DEV_OS61_661711AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_A118185F
%ATHR.DeviceDesc.661711AD% = ATHR_DEV_OS61_661711AD.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_663711AD
%ATHR.DeviceDesc.661711AD% = ATHR_DEV_OS61_661711AD.ndi, PCI\VEN_168C&DEV_0037&SUBSYS_663711AD
%ATHR.DeviceDesc.311711AD% = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_662111AD
%ATHR.DeviceDesc.311711AD% = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_E052105B
%ATHR.DeviceDesc.E059105B% = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_E059105B
%ATHR.DeviceDesc.E059105B% = ATHR_DEV_OS61_311711AD.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_E058105B
%ATHR.DeviceDesc.E068105B% = ATHR_DEV_OS61_ACER956x.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_E068105B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER956x.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_A119185F
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER956x.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_063211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER956x.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_667111AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER_956x_CH2.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_064211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_A120185F.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_A120185F
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_ACER_956x_CH2.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_E07F105B
; Toshiba
%ATHR.DeviceDesc.2041%     = ATHR_DEV_OS61_2041.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7064144F
%ATHR.DeviceDesc.2042%     = ATHR_DEV_OS61_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7065144F
%ATHR.DeviceDesc.2051%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7084144F
%ATHR.DeviceDesc.2051%     = ATHR_DEV_OS61_2051.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_7088144F
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_7092144F
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_2054.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_7094144F
%ATHR.DeviceDesc.3063%     = ATHR_DEV_OS61_2063.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7096144F
%ATHR.DeviceDesc.3065%     = ATHR_DEV_OS61_2052.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7106144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7128144f
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_04271468
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_001B.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_04251468
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_04261468
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_7125144F.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_7125144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_042A1468
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E004105B
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E009105B
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7136144F
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7154144F
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7141144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_41051A32
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43011A32  
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43031A32
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E012105B
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E013105B
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E015105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E014105B
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7158144F
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7156144F
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7157144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7159144F
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_632311AD
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_662011AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_650211AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_653211AD
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_661011AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_651211AD
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_652211AD
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_661111AD
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7163144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_661211AD
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_660111AD
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7163144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_7163144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7164144F
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7163144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E019105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E01A105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_43051A32
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7163144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_43061A32
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_001C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_A6011113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E6111113
%ATHR.DeviceDesc.7141144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E6221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_D6221113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E8111113
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_7163144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_F8221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_A8221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_B8221113
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_45071A32
%ATHR.DeviceDesc.7136144F% = ATHR_DEV_OS61_7136144F.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_65071A32
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_T30A4.ndi,    PCI\VEN_168C&DEV_002E&SUBSYS_43091A32
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_7173144Fw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_7173144F
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_7173144Fw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_661311AD
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_7173144Fw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_10001B14
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_7188144F
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_938x.ndi,     PCI\VEN_168C&DEV_0030&SUBSYS_650311AD
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_7173144Fw.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_EE321113
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_9485.ndi,     PCI\VEN_168C&DEV_0032&SUBSYS_660711AD
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_T3119.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_660811AD
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_9485.ndi,     PCI\VEN_168C&DEV_0032&SUBSYS_7192144F
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_T3119.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_7193144F
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_9485.ndi,     PCI\VEN_168C&DEV_0032&SUBSYS_B8411113
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_T3119.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_B8421113
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_9485.ndi,     PCI\VEN_168C&DEV_0032&SUBSYS_43181A32
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_T30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_7194144F
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_T946x.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_7055144F
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_T946x.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_661111AD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_T946x.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_2C001B9A
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_061211AD.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_061211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_7202144F.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_7202144F
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_28101B9A.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_28101B9A
; Sony
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_E007105B.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E007105B
%ATHR.DeviceDesc.04231468% = ATHR_DEV_OS61_E000105B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E000105B
%ATHR.DeviceDesc.04231468% = ATHR_DEV_OS61_E002105B.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_E002105B
%ATHR.DeviceDesc.04061468% = ATHR_DEV_OS61_04061468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04061468
%ATHR.DeviceDesc.04071468% = ATHR_DEV_OS61_04061468.ndi, PCI\VEN_168C&DEV_0013&SUBSYS_04071468 
%ATHR.DeviceDesc.04231468% = ATHR_DEV_OS61_04231468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_04231468 
%ATHR.DeviceDesc.04231468% = ATHR_DEV_OS61_04231468.ndi, PCI\VEN_168C&DEV_001C&SUBSYS_0423168C
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_S30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_E017105B
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_SS30A1.ndi,   PCI\VEN_168C&DEV_002E&SUBSYS_E030105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_S30A1w.ndi,   PCI\VEN_168C&DEV_002B&SUBSYS_E037105B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_S3119.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_E044105B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956x.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_E069105B
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_3117104D.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_3117104D
; HP Desktop
%ATHR.DeviceDesc.2A5F103C% = ATHR_DEV_OS61_2A5F103C.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_2A5F103C
%ATHR.DeviceDesc.500011AD% = ATHR_DEV_OS61_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_500011AD
%ATHR.DeviceDesc.500111AD% = ATHR_DEV_OS61_11AD.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_500111AD
%ATHR.DeviceDesc.1000168c% = ATHR_DEV_OS61_1000168C.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1000168C
%ATHR.DeviceDesc.1000168c% = ATHR_DEV_OS61_1001168C.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_1001168C
; HP LT
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30ABLT.ndi,   PCI\VEN_168C&DEV_002B&SUBSYS_30AB1895
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_30A1LT.ndi,   PCI\VEN_168C&DEV_002B&SUBSYS_30A11895
; HP laptop
%ATHR.DeviceDesc.H3067%    = ATHR_DEV_OS61_H001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_303F103C
%ATHR.DeviceDesc.H3067%    = ATHR_DEV_OS61_H001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_3040103C
%ATHR.DeviceDesc.H3067%    = ATHR_DEV_OS61_H001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_137A103C
%ATHR.DeviceDesc.H3067%    = ATHR_DEV_OS61_H001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_137B103C
%ATHR.DeviceDesc.H2063%    = ATHR_DEV_OS61_H2063.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_1385103C
%ATHR.DeviceDesc.H2063%    = ATHR_DEV_OS61_H2063.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_1386103C
%ATHR.DeviceDesc.H3096%    = ATHR_DEV_OS61_H002A.ndi,    PCI\VEN_168C&DEV_002A&SUBSYS_1381103C
%ATHR.DeviceDesc.H3096%    = ATHR_DEV_OS61_H002A.ndi,    PCI\VEN_168C&DEV_002A&SUBSYS_1382103C
%ATHR.DeviceDesc.H3096%    = ATHR_DEV_OS61_H002A.ndi,    PCI\VEN_168C&DEV_002A&SUBSYS_3041103C
%ATHR.DeviceDesc.H3096%    = ATHR_DEV_OS61_H002A.ndi,    PCI\VEN_168C&DEV_002A&SUBSYS_3042103C
%ATHR.DeviceDesc.H30A1%    = ATHR_DEV_OS61_H30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_303F103C
%ATHR.DeviceDesc.H30A1%    = ATHR_DEV_OS61_H30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_3040103C
%ATHR.DeviceDesc.H30AB%    = ATHR_DEV_OS61_H30AB.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_1461103C
%ATHR.DeviceDesc.H30A4%    = ATHR_DEV_OS61_H30A4.ndi,    PCI\VEN_168C&DEV_002E&SUBSYS_1462103C
%ATHR.DeviceDesc.H3197%    = ATHR_DEV_OS61_H3197.ndi,    PCI\VEN_168C&DEV_002E&SUBSYS_1626103C
%ATHR.DeviceDesc.H3116%    = ATHR_DEV_OS61_H3116.ndi,    PCI\VEN_168C&DEV_0030&SUBSYS_1628103C
%ATHR.DeviceDesc.H3112%    = ATHR_DEV_OS61_H3112.ndi,    PCI\VEN_168C&DEV_0030&SUBSYS_1627103C
%ATHR.DeviceDesc.H3119%    = ATHR_DEV_OS61_H3119.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_1785103C
%ATHR.DeviceDesc.H3119%    = ATHR_DEV_OS61_H3119.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_179F103C
%ATHR.DeviceDesc.H3118%    = ATHR_DEV_OS61_H3118.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_1838103C
%ATHR.DeviceDesc.H3118%    = ATHR_DEV_OS61_H3118.ndi,    PCI\VEN_168C&DEV_0032&SUBSYS_191A103C
%ATHR.DeviceDesc.H3335%    = ATHR_DEV_OS61_H3335.ndi,    PCI\VEN_168C&DEV_0034&SUBSYS_1864103C
%ATHR.DeviceDesc.H9565%    = ATHR_DEV_OS61_H9565.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_18E3103C
%ATHR.DeviceDesc.H9565%    = ATHR_DEV_OS61_H9565.ndi,    PCI\VEN_168C&DEV_0036&SUBSYS_217F103C
%ATHR.DeviceDesc.H9565%    = ATHR_DEV_OS61_HNFA335.ndi,  PCI\VEN_168C&DEV_0036&SUBSYS_2005103C
; Asus
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_2062.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_7112144f
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7137144F
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_3072.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_7122144F
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_1071.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_7132144F
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_1071.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_2072144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_7182144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_7183144F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A0111113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_1A891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A8311113
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB2C37.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A8421113
%ATHR.DeviceDesc.2A371A3B% = ATHR_DEV_OS61_2A371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_A8411113
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E049105B
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB2C37.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E048105B
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_666111AD
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB2C37.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_662311AD
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_E03E105B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_11861A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E04E105B
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_850D1043.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_850D1043
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_2C971A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E04F105B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_2C971A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_7197144F
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_850E1043.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_850E1043
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_21161A3B.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_21161A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_CUS198_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_E075105B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_CUS198_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_21521A3B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_21301A3B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_21301A3B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_066211AD.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_066211AD
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_21761A3B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_21761A3B
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_213A1A3B.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_213A1A3B
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_CUS198_2.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_126A1A3B

; Sharp(Mitac)
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7138144F 
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7139144F
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_7140144F 
; Fujitsu
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_13C010CF.ndi, PCI\VEN_168C&DEV_0024&SUBSYS_13C010CF
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_147C10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_147C10CF
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_147D10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_147D10CF
%ATHR.DeviceDesc.1071%     = ATHR_DEV_OS61_13C010CF.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_147E10CF
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123410CF
%ATHR.DeviceDesc.0013%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123510CF
%ATHR.DeviceDesc.10CF%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_123610CF
%ATHR.DeviceDesc.001B%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_132910CF
%ATHR.DeviceDesc.10CF%     = ATHR_DEV_OS61_F013.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_134F10CF
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_F013C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_139C10CF
%ATHR.DeviceDesc.3067%     = ATHR_DEV_OS61_F01C.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_142E10CF
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_153710CF.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_153710CF
%ATHR.DeviceDesc.7163144F% = ATHR_DEV_OS61_147D10CF.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_153610CF
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_158F10CF.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_158F10CF
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_161910CF.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_161910CF
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_16A810CF.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_16A810CF
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_178310CF.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_178310CF
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_180E10CF.ndi, PCI\VEN_168C&DEV_0034&SUBSYS_180E10CF
; WNC
%ATHR.DeviceDesc.CM9%      = ATHR_DEV_OS61_2042.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_1012185F
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_03051A32w.ndi,PCI\VEN_168C&DEV_002B&SUBSYS_30AE185F
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_E016105B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_30A1185F
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_03091A32.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_30B3185F
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_3119185F.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_3119185F
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_3027185F.ndi, PCI\VEN_168C&DEV_0036&SUBSYS_3027185F
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_956x.ndi,     PCI\VEN_168C&DEV_0036&SUBSYS_3028185F
; TPLINK
%ATHR.DeviceDesc.1ACE%     = ATHR_DEV_OS61_T3091.ndi,    PCI\VEN_168C&DEV_0029&SUBSYS_92231ACE
%ATHR.DeviceDesc.0300T%    = ATHR_DEV_OS61_30A4TP.ndi,   PCI\VEN_168C&DEV_002D&SUBSYS_0300168C
%ATHR.DeviceDesc.0301T%    = ATHR_DEV_OS61_30A4TP.ndi,   PCI\VEN_168C&DEV_002D&SUBSYS_0301168C
; Pegatron
%ATHR.DeviceDesc.00341B0A% = ATHR_DEV_OS61_3091.ndi,     PCI\VEN_168C&DEV_002A&SUBSYS_00341B0A
; Belkin
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_701D1799
%ATHR.DeviceDesc.001A%     = ATHR_DEV_OS61_001A.ndi,     PCI\VEN_168C&DEV_001A&SUBSYS_700D1799
%ATHR.DeviceDesc.F6D3000%  = ATHR_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_30001799
%ATHR.DeviceDesc.F6D3000%  = ATHR_DEV_OS61_001B.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_30001799
%ATHR.DeviceDesc.80111799% = ATHR_DEV_OS61_80111799.ndi, PCI\VEN_168C&DEV_0023&SUBSYS_80111799
; NEC 
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102010E9
%ATHR.DeviceDesc.3062%     = ATHR_DEV_OS61_N2062.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_102510E9
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_N3072.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102210E9
%ATHR.DeviceDesc.3072%     = ATHR_DEV_OS61_N3073.ndi,    PCI\VEN_168C&DEV_0024&SUBSYS_102610E9
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_03051A32
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_03051A32.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_83051A32
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_651311AD.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_05081A32
; IO Data
%ATHR.DeviceDesc.D05B10FC% = ATHR_DEV_OS61_D05B10FC.ndi, PCI\VEN_168C&DEV_0029&SUBSYS_D05B10FC
; SEMCO
%ATHR.DeviceDesc.30AB%     = ATHR_DEV_OS61_BA91167D.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_BA91167D
; Dell LT
%ATHR.DeviceDesc.D3067%    = ATHR_DEV_OS61_02B0.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_02B01028
%ATHR.DeviceDesc.D3067%    = ATHR_DEV_OS61_02B0.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_02B11028
%ATHR.DeviceDesc.D3067%    = ATHR_DEV_OS61_02B0.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_02D61028
%ATHR.DeviceDesc.D3067%    = ATHR_DEV_OS61_D001C.ndi,    PCI\VEN_168C&DEV_001C&SUBSYS_0202168C
%ATHR.DeviceDesc.D30A1%    = ATHR_DEV_OS61_D30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_0204168C
%ATHR.DeviceDesc.D30AB%    = ATHR_DEV_OS61_D30AB.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_0205168C
%ATHR.DeviceDesc.D30AB%    = ATHR_DEV_OS61_D30ABHZ.ndi,  PCI\VEN_168C&DEV_002B&SUBSYS_04641028
%ATHR.DeviceDesc.D30AB%    = ATHR_DEV_OS61_D30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_30AF185F
%ATHR.DeviceDesc.D30AB%    = ATHR_DEV_OS61_D30A1.ndi,    PCI\VEN_168C&DEV_002B&SUBSYS_A3051A32
; Xavi 
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_04001B9A 
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_03091A32.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_08001B9A 
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0C001B9A 
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_04011B9A 
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_04021B9A 
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_04031B9A.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_04031B9A 
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_04101B9A 
%ATHR.DeviceDesc.30A1%     = ATHR_DEV_OS61_10891A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_04111B9A  
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_03091A32.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_08011B9A 
%ATHR.DeviceDesc.30A4%     = ATHR_DEV_OS61_03091A32.ndi, PCI\VEN_168C&DEV_002E&SUBSYS_08021B9A 
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0C011B9A 
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0C021B9A 
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0C031B9A
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0C041B9A
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_0C051B9A
%ATHR.DeviceDesc.30ABLT%   = ATHR_DEV_OS61_30AB2C37.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_0C101B9A
%ATHR.DeviceDesc.2A371A3B% = ATHR_DEV_OS61_2A371A3B.ndi, PCI\VEN_168C&DEV_002B&SUBSYS_0C111B9A
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_651311AD.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_18001B9A
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_651311AD.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_18011B9A
%ATHR.DeviceDesc.938x%     = ATHR_DEV_OS61_651311AD.ndi, PCI\VEN_168C&DEV_0030&SUBSYS_18021B9A
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_11861A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_1C001B9A
%ATHR.DeviceDesc.9485%     = ATHR_DEV_OS61_11861A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_1C011B9A
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_2C971A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_20001B9A
%ATHR.DeviceDesc.3119%     = ATHR_DEV_OS61_2C971A3B_1.ndi, PCI\VEN_168C&DEV_0032&SUBSYS_20011B9A
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_01186931.ndi,   PCI\VEN_168C&DEV_0036&SUBSYS_28111B9A
%ATHR.DeviceDesc.956x%     = ATHR_DEV_OS61_01186931.ndi,   PCI\VEN_168C&DEV_0036&SUBSYS_28121B9A
; Via
%ATHR.DeviceDesc.3B001106% = ATHR_DEV_OS61_30A1.ndi,     PCI\VEN_168C&DEV_002B&SUBSYS_3B001106
; USI
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946x.ndi,     PCI\VEN_168C&DEV_0034&SUBSYS_006314CD
%ATHR.DeviceDesc.946x%     = ATHR_DEV_OS61_946x.ndi,     PCI\VEN_168C&DEV_0034&SUBSYS_006414CD
; Compex
%ATHR.DeviceDesc.3091%     = ATHR_DEV_OS61_20001071.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_20001071

[Gigabyte.NTX86.6.2]
%GIGA.DeviceDesc.E801%     = GIGA_DEV_OS61_E801.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E8011458
%GIGA.DeviceDesc.E811%     = GIGA_DEV_OS61_E811.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E8111458
%GIGA.DeviceDesc.E814%     = GIGA_DEV_OS61_E814.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E8141458
%GIGA.DeviceDesc.0013%     = GIGA_DEV_OS61_0013.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E9011458
%GIGA.DeviceDesc.E901%     = GIGA_DEV_OS61_E901.ndi,     PCI\VEN_168C&DEV_001B&SUBSYS_E9011458
%GIGA.DeviceDesc.E911%     = GIGA_DEV_OS61_E911.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E9111458
%GIGA.DeviceDesc.E912%     = GIGA_DEV_OS61_E912.ndi,     PCI\VEN_168C&DEV_0013&SUBSYS_E9121458
%GIGA.DeviceDesc.E913%     = GIGA_DEV_OS61_E913.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_E9131458
%GIGA.DeviceDesc.E917%     = GIGA_DEV_OS61_E917.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_E9171458
%GIGA.DeviceDesc.E815%     = GIGA_DEV_OS61_E914.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_E8151458
%GIGA.DeviceDesc.E914%     = GIGA_DEV_OS61_E914.ndi,     PCI\VEN_168C&DEV_0023&SUBSYS_E9141458
%GIGA.DeviceDesc.E915%     = GIGA_DEV_OS61_E914.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_E9151458
%GIGA.DeviceDesc.E916%     = GIGA_DEV_OS61_E916.ndi,     PCI\VEN_168C&DEV_0024&SUBSYS_E9161458
%GIGA.DeviceDesc.E918%     = GIGA_DEV_OS61_E918.ndi,     PCI\VEN_168C&DEV_001C&SUBSYS_E9181458
%GIGA.DeviceDesc.E9191458% = ATHR_DEV_OS61_03011A32.ndi, PCI\VEN_168C&DEV_002A&SUBSYS_E9191458 

;
; OS 6.1 Manufacturer section
;
[GIGA_DEV_OS61_E801.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E801.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E801.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E811.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E811.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E811.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E814.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E814.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E814.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_0013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_0013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_0013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E901.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E901.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E901.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E911.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E911.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E911.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E912.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed0.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E912.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E912.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E913.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E913.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E913.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E917.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E917.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E917.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E918.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_GigaByteLed2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E918.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E918.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E914.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer_GigaByte.reg, customer_GigaByteLed0.reg, 5416.antennacontrols.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E914.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E914.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[GIGA_DEV_OS61_E916.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer_GigaByte.reg, customer_GigaByteLed1.reg, 5416.antennacontrols.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[GIGA_DEV_OS61_E916.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[GIGA_DEV_OS61_E916.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_OSPEMU.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_OSPEMU.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_OSPEMU.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_9485.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, paprdenable.reg, customer2GreenTx.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_9485.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_9485.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_9485s.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, paprdenable.reg, customer2GreenTx.reg, cmdRegister.reg, ignore11denable.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_9485s.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_9485s.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1111.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, paprdenable.reg, customer2GreenTx.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1111.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1111.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3119.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, 9485LnaDivUseBtAntEnable.reg, cemspecled_func0_6.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3119.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3119.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3119185F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, 9485LnaDivUseBtAntEnable.reg, cemspecled_func1_6.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3119185F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3119185F.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3119s.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cmdRegister.reg, 9485BTcoex.reg, c3war.reg, rxLatencyWar.reg, customer2GreenTx.reg, paprdenable.reg, 9485LnaDivUseBtAntEnable.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3119s.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3119s.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_4107144D.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cmdRegister.reg, c3war.reg, rxLatencyWar.reg, customer_Samsung.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_4107144D.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_4107144D.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T3119.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTCoexAgent0.reg, customer2GreenTx.reg, paprdenable.reg, ampGUID.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T3119.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T3119.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_OSPREY.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_OSPREY.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_OSPREY.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_K110x.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, led_func0_10.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_K110x.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_K110x.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_938x.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_938x.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_938x.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_946x.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_946x.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_946x.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_K1202.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, led_func0_4.reg, htAdhoc.reg, jupiter2ant.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_K1202.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_K1202.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration


[ATHR_DEV_OS61_21101A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, wowenable.reg, cemspecled_func0_4.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_21101A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_21101A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_664111AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_664111AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_664111AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_946xs.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, cmdRegister.reg, ignore11denable.reg, halShortRetry.reg, ConnectionFailure.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_946xs.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_946xs.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T946x.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, ampGUID.reg, ampTFilter.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T946x.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T946x.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_CUS217.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_CUS217.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_CUS217.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_21161A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant2.reg, cemspecled_func0_4.reg, RestoreSettingCount.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_21161A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_21161A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_850E1043.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, customer3h.reg, S5wow.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_850E1043.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_850E1043.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_311711AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant2.reg, customer3h.reg, roamPolicy2.reg, AdjustRSSI.reg, halShortRetry.reg, SleepTimePwrSaveMax1000.reg, FilterOutCCK.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_311711AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_311711AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1186788.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant2.reg, customer3h.reg, roamPolicy2.reg, AdjustRSSI.reg, halShortRetry.reg, SleepTimePwrSaveMax1000.reg, FilterOutCCK.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1186788.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1186788.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration


[ATHR_DEV_OS61_956x.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_956x.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_956x.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_956xs.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, ledcontrol8.reg, ConnectionFailure.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_956xs.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_956xs.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_ACER956x.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeantTS.reg, ledcontrol8.reg, delayNWSleep.reg, FilterOutCCK.reg, miracast_off.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_ACER956x.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_ACER956x.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_ACER_956x_CH2.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, ledcontrol8.reg, delayNWSleep.reg, aphroditeantdiv2.reg, AphroditeMitiShift.reg, customer_power.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_ACER_956x_CH2.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_ACER_956x_CH2.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_A120185F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, ledcontrol8.reg, delayNWSleep.reg, aphroditeantdiv2.reg, AphroditeMitiShift.reg, customer_power.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_A120185F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_A120185F.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_01186931.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, ledcontrol8.reg, ConnectionFailure.reg, FilterOutCCK.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_01186931.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_01186931.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_21301A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_21301A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_21301A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

; Levi add for liteon pcie 1.1
[ATHR_DEV_OS61_067211AD_PCIE_1_1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, customer3gpcie11.reg, ConnectionFailure.reg, aphroditeantdiv.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_067211AD_PCIE_1_1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_067211AD_PCIE_1_1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_081211AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, wowenable.reg, customer3gpcie11.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_081211AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_081211AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_066211AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_066211AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_066211AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_21761A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_21761A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_21761A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_213A1A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_213A1A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_213A1A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T956x.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg, AphroditeMitiShift.reg, customer_power.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T956x.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T956x.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

; 061211ad
[ATHR_DEV_OS61_061211AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg, AphroditeMitiShift.reg, customer_power_Toshiba.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_061211AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_061211AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

; 7202144f
[ATHR_DEV_OS61_7202144F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg, AphroditeMitiShift.reg, customer_power_Toshiba.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_7202144F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_7202144F.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

; 28101B9A
[ATHR_DEV_OS61_28101B9A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg, AphroditeMitiShift.reg, customer_power_Toshiba.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_28101B9A.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_28101B9A.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration


[ATHR_DEV_OS61_3027168C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3027168C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3027168C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3028.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3028.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3028.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_302617AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, ledcontrol8.reg, ConnectionFailure.reg, wowenable.reg, aphroditeantdiv2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_302617AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_302617AA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_9580.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_9580.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_9580.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_651311AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cemspecled_func2_10.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_651311AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_651311AD.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_652311AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cemspecled_func1_10.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_652311AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_652311AD.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_001A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_001A.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_001A.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_001B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_001B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_001B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_001C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_001C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_001C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_6313.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func1_3.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_6313.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_6313.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3064.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3064.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3064.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1055.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, gpioled.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1055.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1055.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2055.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2055.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2055.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1030.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1030.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1030.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2030.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2030.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2030.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1031.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1031.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1031.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2031.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2031.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2031.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1041.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1041.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1041.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2041.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2041.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2041.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1042.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1042.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1042.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2042.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2042.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2042.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1051.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1051.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1051.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2051.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2051.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2051.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_7111144F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, expresscardaspmoff.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_7111144F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_7111144F.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1052.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1052.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1052.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2052.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2052.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2052.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_01001A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer9Led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_01001A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_01001A32.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1053.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1053.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1053.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2053.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2053.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2053.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1054.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1054.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1054.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2054.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2054.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2054.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1062.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1062.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1062.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2062.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2062.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2062.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1063.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1063.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1063.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2063.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2063.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2063.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1071.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1071.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1071.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_90001385.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, expresscardaspmoff.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_90001385.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_90001385.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2A5F103C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer2.11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2A5F103C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2A5F103C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_11AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_11AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_11AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3072.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3072.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3072.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10671A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htWepTkipOpt.reg, htAdhoc.reg, indicaterxlinkspeed.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10671A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10671A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1A671A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1A671A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1A671A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10711A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htEnableWepTkip.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10711A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10711A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1C711A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, 5416.bandselect.reg, htEnableWepTkip.reg, htAdhoc.reg, d3forcel1disable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1C711A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1C711A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_03011A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_03011A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_03011A32.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3091.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3091.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3091.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_20001071.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, roamPolicy2.reg, wirelessmodeselectCompex.reg, TxPowerSelect.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_20001071.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_20001071.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_309D168C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, customer1roamPolicy.reg, wirelessmodeselectkite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_309D168C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_309D168C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3091amd.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cemspecled_func1_1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3091amd.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3091amd.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_008F106B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, wowenable.reg, merlinshiftdelay.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_008F106B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_008F106B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_309D17AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, Customer15a.led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_309D17AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_309D17AA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A117AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, Customer15a.led.reg, triggerlevelkiteonly.reg, c3war.reg, sharegpio.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A117AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A117AA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A117AAw.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, Customer15a.led.reg, triggerlevelkiteonly.reg, c3war.reg, sharegpio.reg, janusda.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A117AAw.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A117AAw.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_311817AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, paprdenable.reg, customer2GreenTx.reg, cemspecled_func2_6.reg, wowenable.reg, power_management.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_311817AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_311817AA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_321817AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, 9485LnaDivUseBtAntEnable.reg, cemspecled_func2_6.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_321817AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_321817AA.ndi.NTX86.HW]
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_321917AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, 9485LnaDivUseBtAntEnable.reg, cemspecled_func2_6.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_321917AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_321917AA.ndi.NTX86.HW]
AddReg  = MSI.reg
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_311417AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, customer2GreenTx.reg, customer3h.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_311417AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_311417AA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_321417AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, customer2GreenTx.reg, customer3h.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_321417AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_321417AA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_00911969.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, customer2GreenTx.reg, customer3h.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_00911969.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_00911969.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

;Liteon, Alan Liu
[ATHR_DEV_OS61_321417AAA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, jupiter2ant.reg, customer2GreenTx.reg, customer3h.reg, wowenable.reg, bandselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_321417AAA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_321417AAA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A417AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cemspecled_func2_8.reg, c3war.reg, sharegpio.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A417AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A417AA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A417AAw.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cemspecled_func2_8.reg, c3war.reg, sharegpio.reg, WB197da.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A417AAw.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A417AAw.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_316417AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, Customer15b.led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_316417AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_316417AA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_7136144F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, merlinshiftdelay.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_7136144F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_7136144F.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_7163144F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, merlinshiftdelay.reg, fullhwresethb93.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_7163144F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_7163144F.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_D05B10FC.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, customer_IODATA.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_D05B10FC.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_D05B10FC.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T3091.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, pcibusconfig.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T3091.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T3091.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_309917AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_309917AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_309917AA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg 
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A1op.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg, customerop.reg, regdmn.reg, cmdRegister.reg, rxLatencyWar.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A1op.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A1op.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A4.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A4.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A4.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A4TP.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, tpshiftdelay.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A4TP.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A4TP.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T30A1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T30A1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T30A1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_T30A4.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_T30A4.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_T30A4.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_660311AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer3f.reg, amp.reg, ampFilter.reg, c3war.reg, roamPolicy2.reg, smpsDynamic.reg, maxpowersave.reg, customer1GreenTx.reg, wowenable.reg, hb97ChainMask.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_660311AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_660311AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_03091A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cemspecled_func1_8.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_03091A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_03091A32.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30AA.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg, Customer15a.led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30AA.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30AA.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30AB.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg, Customer15a.led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30AB.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30AB.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30AB2C37.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg, Customer15a.led.reg, amp.reg, ampFilter.reg, htWepTkipOpt.reg, wirelessmodeselectkite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30AB2C37.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30AB2C37.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30B0.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, heliusda.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30B0.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30B0.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30B07189.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, heliusda.reg, btcoexa2dp99.reg, cmdRegister.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30B07189.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30B07189.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30ABLT.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, janusda.reg, cemspecled_func0_1.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30ABLT.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30ABLT.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A1LT.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cemspecled_func0_1.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A1LT.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A1LT.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_BA91167D.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, janusda.reg, cemspecled_func1_1.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_BA91167D.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_BA91167D.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_7173144Fw.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, janusda_CoexAgent0.reg, triggerlevelkiteonly.reg, c3war.reg, roamPolicy.reg, ampGuid.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_7173144Fw.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_7173144Fw.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A1a.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cmdRegister.reg, triggerlevelkiteonly.reg, c3war.reg, rxLatencyWar.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A1a.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A1a.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_30A1w.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cmdRegister.reg, janusda_coexPTA_40_21.reg, triggerlevelkiteonly.reg, c3war.reg, rxLatencyWar.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_30A1w.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_30A1w.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E023105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cemspecled_func1_1.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E023105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E023105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E036105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cemspecled_func2_1.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E036105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E036105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E033105Bw.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, cemspecled_func1_1.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E033105Bw.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E033105Bw.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E029105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func1_1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E029105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E029105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_11121A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func1_1.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_11121A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_11121A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_662111AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_662111AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_662111AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_662211AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_662211AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_662211AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3091PB.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, pushbutton.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3091PB.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3091PB.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1000168C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer2merlin.reg, smpsDynamic.reg, htAdhoc.reg, fastclockdisable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1000168C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1000168C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1001168C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer2.11n.reg, smpsDynamic.reg, htAdhoc.reg, fastclockdisable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1001168C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1001168C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3091SF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer_Samsung.reg, smpsDynamic.reg, htAdhoc.reg, ignore11denable.reg, cmdRegister.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3091SF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3091SF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_03051A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_03051A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_03051A32.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_03051A32w.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_03051A32w.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_03051A32w.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_D8111113.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_D8111113.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_D8111113.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10891A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10891A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10891A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1D891A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg, triggerlevelkiteonly.reg, c3war.reg, amp.reg, ampFilter.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1D891A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1D891A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_11211A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func2_8.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_11211A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_11211A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1A211A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func2_8.reg, htWepTkipOpt.reg, htAdhoc.reg, wirelessmodeselectkite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1A211A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1A211A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_20371A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htEnableWepTkip.reg, htAdhoc.reg, wirelessmodeselectkite.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_20371A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_20371A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1A891A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1A891A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1A891A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2A371A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, Customer15a.led.reg, triggerlevelkiteonly.reg, c3war.reg, janusda.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2A371A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2A371A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2C971A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2C971A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2C971A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2C971A3B_1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2C971A3B_1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2C971A3B_1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2C971A3B_2.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoexPTA.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg,
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2C971A3B_2.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2C971A3B_2.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_20971A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg, S5wow.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_20971A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_20971A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_209C1A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_209C1A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_209C1A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_CUS198.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoexDivEn.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg, 9485LnaDivUseBtAntEnable.reg, CUS198_xLnaGpioCfg.reg, antCtrlComm2gSwitchEnable.reg, rateCtrlTxFastDrop.reg, IdleConfiguration.reg, amp.reg,ampFilter.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_CUS198.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_CUS198.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_CUS198_1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoexDivEn_1.reg, customer2GreenTx.reg, paprdenable.reg, customer3h.reg, 9485LnaDivUseBtAntEnable.reg, CUS198_xLnaGpioCfg.reg, antCtrlComm2gSwitchEnable.reg, rateCtrlTxFastDrop.reg, IdleConfiguration.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_CUS198_1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_CUS198_1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_CUS198_2.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoexDivEn_1.reg, customer2GreenTx.reg, paprdenable.reg, customer3h.reg, 9485LnaDivUseBtAntEnable.reg, CUS198_xLnaGpioCfg.reg, antCtrlComm2gSwitchEnable.reg, rateCtrlTxFastDrop.reg, IdleConfiguration.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_CUS198_2.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_CUS198_2.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_11861A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_11861A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_11861A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_11861A3B_1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_11861A3B_1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_11861A3B_1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_118C1A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_118C1A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_118C1A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_118C1A3B1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg, wowenable.reg, customer1roamPolicy.reg, wirelessmodeselectkite.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_118C1A3B1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_118C1A3B1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_850D1043.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer2GreenTx.reg, paprdenable.reg, cemspecled_func2_6.reg, S5wow.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_850D1043.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_850D1043.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E006105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, htAdhoc.reg, roamPolicy2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E006105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E006105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_655211AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, htAdhoc.reg, 5416.bandselect.reg, roamPolicy2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_655211AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_655211AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_661711AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, paprdenable.reg, customer3g.reg, maxpowersave.reg, serializing.reg, roamPolicy2.reg, customer1GreenTx.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_661711AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_661711AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

;add by alan liu for liteon pcie 1.1
[ATHR_DEV_OS61_661711ADPCIE_1_1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, paprdenable.reg, customer3gpcie11.reg, maxpowersave.reg, serializing.reg, roamPolicy2.reg, customer1GreenTx.reg, wowenable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_661711ADPCIE_1_1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_661711ADPCIE_1_1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration
;----------------------------------------------------------------------

[ATHR_DEV_OS61_E04A105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, htAdhoc.reg, cemspecled_func2_10.reg, serializing.reg, maxpowersave.reg, roamPolicy2.reg, customer1GreenTx.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E04A105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E04A105B.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E01F105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5 
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, htAdhoc.reg, maxpowersave.reg, serializing.reg, d3forcel1disable1.reg, cmdRegister.reg, amp.reg, ampFilter.reg, c3war.reg, roamPolicy2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E01F105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E01F105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_664211AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, maxpowersave.reg, serializing.reg, d3forcel1disable1.reg, cmdRegister.reg, amp.reg, ampFilter.reg, roamPolicy2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_664211AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_664211AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_663111AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, smpsDynamic.reg, htAdhoc.reg, maxpowersave.reg, serializing.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_663111AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_663111AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E016105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, htAdhoc.reg, maxpowersave.reg, serializing.reg, triggerlevelkiteonly.reg, c3war.reg, cmdRegister.reg, amp.reg, ampFilter.reg, roamPolicy2.reg, customer1GreenTx.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E016105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E016105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E035105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5 
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, maxpowersave.reg, serializing.reg, cmdRegister.reg, amp.reg, ampFilter.reg, triggerlevelkiteonly.reg, c3war.reg, roamPolicy2.reg, customer1GreenTx.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E035105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E035105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E031105Bw.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer3c.reg, htAdhoc.reg, maxpowersave.reg, serializing.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg, amp.reg, ampFilter.reg, roamPolicy2.reg, customer1GreenTx.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E031105Bw.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E031105Bw.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_2013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED.reg, customer0.reg, roamthreshA.reg, ignore11d.reg, bandselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_2013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_2013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED1.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_4013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED1.reg, customer0.reg, roamthreshA.reg, ignore11d.reg, bandselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_4013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_4013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_5013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED2.reg, customer0.reg, roamthreshA.reg, ignore11d.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_5013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_5013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_6013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer0LED2.reg, customer0.reg, roamthreshA.reg, ignore11d.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_6013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_6013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0036.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer0LED1.reg, customer0_HB93.reg, roamthreshA.reg, ignore11d.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0036.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0036.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0037.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer0LED1.reg, customer0_HB95.reg, roamthreshA.reg, ignore11d.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0037.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0037.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_F013.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer1ani.reg, bandselect.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_F013.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_F013.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_F013C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer1ani.reg, bandselect.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg, minpower.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_F013C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_F013C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_F01C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_F01C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_F01C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_04221468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer3.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_04221468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_04221468.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E000105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer4b.reg, customer4a_ASPM.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = PciASPMOptIn, VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E000105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E000105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E002105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer4b.reg, customer4a_ASPM.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = PciASPMOptIn, VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E002105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E002105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_04281468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer3e.reg, interruptpolling.reg, customer3_legacybgwmode.reg, adhocchannelselect.reg, d3hot.reg, roamPolicy2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_04281468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_04281468.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_01051A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer3a.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_01051A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_01051A32.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_01121A32.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer3d.reg, d3hot.reg, adhocchannelselect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_01121A32.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_01121A32.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_04061468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer4.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_04061468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_04061468.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_04231468.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer4a.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = PciASPMOptIn, VWiFiBus.CopyFiles

[ATHR_DEV_OS61_04231468.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_04231468.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_E007105B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer4a.reg, customer4adhoc.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = PciASPMOptIn, VWiFiBus.CopyFiles

[ATHR_DEV_OS61_E007105B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_E007105B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S30A1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer4adhoc.reg, customer4a.reg, ratecap.reg, triggerlevelkiteonly.reg, c3war.reg, cmdRegister.reg, ocsEnable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = PciASPMOptIn, VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S30A1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S30A1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S30A1w.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer4adhoc.reg, customer4a.reg, ratecap.reg, triggerlevelkiteonly.reg, c3war.reg, cmdRegister.reg, janusda.reg, amp.reg, ampFilter.reg, cemspecled_func0_6.reg, customer2GreenTx.reg, ocsEnable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = PciASPMOptIn, VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S30A1w.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S30A1w.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S3119.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, cemspecled_func0_6.reg, customer2GreenTx.reg, customer4c.reg, customer4adhoc.reg, paprdenable.reg, amp.reg, ampFilter.reg, ocsEnable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S3119.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S3119.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_661811AD.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, 9485BTcoex.reg, paprdenable.reg, customer3g.reg, roamPolicy2.reg, maxpowersave2.reg, AdjustRSSI.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_661811AD.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_661811AD.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_SS30A1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, customer4adhoc.reg, customer4as.reg, ratecap.reg, c3war.reg, amp.reg, ampBFilter.reg, ocsEnable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = PciASPMOptIn, VWiFiBus.CopyFiles

[ATHR_DEV_OS61_SS30A1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_SS30A1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0032168c.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer0_11n.reg, 5416.antennacontrols.reg, 5416.bgnxb.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0032168c.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0032168c.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_0033168c.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer0_11n.reg, 5416.antennacontrols.reg, 5416.bandselect.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_0033168c.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_0033168c.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_13C010CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.bandselect.reg, 5416.antennacontrols.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, customer1roamPolicy.reg, htAdhocdisable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_13C010CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_13C010CF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_147C10CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.bandselect.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, smpsDynamic.reg, htAdhocdisable.reg, merlinshiftdelay.reg, d3forcel1disable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_147C10CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_147C10CF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_147D10CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, htAdhocdisable.reg, merlinshiftdelay.reg, d3forcel1disable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_147D10CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_147D10CF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_153710CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, htAdhocdisable.reg, triggerlevelkiteonly.reg, c3war.reg, customer1GreenTx.reg, SleepTimePwrSaveMax2000.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_153710CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_153710CF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_158F10CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, htAdhocdisable.reg, customer1GreenTx.reg, SleepTimePwrSaveMax2000.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_158F10CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_158F10CF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_161910CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, htAdhocdisable.reg, janusda.reg, triggerlevelkiteonly.reg, c3war.reg, customer1GreenTx.reg, SleepTimePwrSaveMax2000.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_161910CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_161910CF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_16A810CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.bandselect.reg, customer1ani.reg, adhocchannelselect.reg, enableswretry, overridetxok.reg, customer1roamPolicy.reg, smpsDynamic.reg, htAdhocdisable.reg, customer1GreenTx.reg, SleepTimePwrSaveMax2000.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_16A810CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_16A810CF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_7125144F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.antennacontrols.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_7125144F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_7125144F.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_03841014.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.antennacontrols.reg, xb72.via.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_03841014.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_03841014.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A171186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer5Led.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A171186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A171186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10261A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func1_3.reg, d3hot.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10261A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10261A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_80111799.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer7Led.reg, ratecap.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_80111799.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_80111799.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer5.11nLED.reg, ratecap.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_1186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A691186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, pcibusconfig.reg, customer5.11nLED.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A691186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A691186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A6D1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, pcibusconfig.reg, customer5.3x3.reg, customer5.11nLED.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A6D1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A6D1186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A6F1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer5.PCIe11nLed.reg, expresscardaspmoff.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A6F1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A6F1186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A701186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer5.3x3.reg, customer5.PCIe11nLed.reg, expresscardaspmoff.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A701186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A701186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A7A1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, pcibusconfig.reg, customer5.11nLED.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A7A1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A7A1186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3A7B1186.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer5.11nLED.reg, ratecap.reg, smpsDynamic.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3A7B1186.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3A7B1186.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_N2062.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, customer11.reg, customer11custom.reg, customer11_legacywmode.reg, cemspecled_func1_1.reg, customer11Ant.reg, rfKillDelayDetect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_N2062.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_N2062.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_N3072.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, customer11n.reg, customer11custom.reg, customer11_11nwmode.reg, cemspecled_func1_1.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_N3072.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_N3072.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_N3073.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, customer11n.reg, customer11custom.reg, customer11_11n40wmode.reg, cemspecled_func1_1.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_N3073.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_N3073.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S001A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_Samsung.reg, cmdRegister.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S001A.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S001A.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S001B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_Samsung.reg, cmdRegister.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S001B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S001B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S3067.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_Samsung.reg, rssiAdjust.reg, cmdRegister.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S3067.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S3067.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_S3067b.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, customer_Samsung.reg, rssiAdjust.reg, cmdRegister.reg, ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_S3067b.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_S3067b.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_10241A3B.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func1_1.reg, htEnableWepTkip.reg, htAdhoc.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_10241A3B.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_10241A3B.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_02B0.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, ledcontrol.reg, power.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_02B0.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_02B0.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_D001C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, ledcontrol.reg, power.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_D001C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_D001C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_D30ABHZ.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, ledcontrol3.reg, kitec3.reg, djanusda.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_D30ABHZ.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_D30ABHZ.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_D30A1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, ledcontrol2.reg, kitec3.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_D30A1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_D30A1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_D30AB.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, ledcontrol2.reg, kitec3.reg, djanusda2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_D30AB.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_D30AB.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H001C.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, ledcontrol.reg, AdhocModeSelect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H001C.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H001C.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H2063.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros.reg, cemspecled_func0_1.reg, AdhocModeSelect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H2063.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H2063.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H002A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func0_1.reg, AdhocModeSelect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H002A.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H002A.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H30A1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func0_1.reg, AdhocModeSelect.reg, amp_default.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H30A1.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H30A1.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H30AB.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func0_1.reg, janusda.reg, throughput.reg, AdhocModeSelect.reg, amp_default.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H30AB.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H30AB.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H30A4.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, ledcontrol4.reg, AdhocModeSelect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H30A4.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H30A4.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H3197.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, cemspecled_func0_1.reg, HPheliusda.reg, AdhocModeSelect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H3197.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H3197.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H3116.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, ledcontrol6.reg, AdhocModeSelect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H3116.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H3116.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H3112.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, ledcontrol6.reg, AdhocModeSelect.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H3112.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H3112.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H3119.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 9485BTcoex.reg, customer2GreenTx.reg, paprdenable.reg, AdhocModeSelect.reg, edmaStopRecvDelay.reg, cemspecled_func0_6.reg, sharegpio.reg, amp_default.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H3119.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H3119.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H3118.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, customer2GreenTx.reg, paprdenable.reg, AdhocModeSelect.reg, edmaStopRecvDelay.reg, cemspecled_func0_6.reg, sharegpio.reg, amp_default.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H3118.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H3118.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H3335.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, smpsDynamic.reg, ledcontrol7.reg, customer2GreenTx.reg, paprdenable.reg, jupiter2ant.reg, AdhocModeSelect.reg, wowenable.reg, roamPolicy.reg, amp_default.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H3335.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H3335.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_H9565.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv.reg, amp_default.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_H9565.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_H9565.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_HNFA335.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant.reg, ledcontrol8acthi.reg, ConnectionFailure.reg, aphroditeantdiv.reg, amp_default.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_HNFA335.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_HNFA335.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_178310CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.bandselect.reg, customer1ani.reg, adhocchannelselect.reg, customer1roamPolicy.reg, smpsDynamic.reg, jupiter2ant.reg, htAdhocdisable.reg, customer1GreenTx.reg, SleepTimePwrSaveMax2000.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_178310CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_178310CF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_180E10CF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.bandselect.reg, customer1ani.reg, adhocchannelselect.reg, customer1roamPolicy.reg, smpsDynamic.reg, jupiter2ant.reg, htAdhocdisable.reg, customer1GreenTx.reg, j21swwow.reg, SleepTimePwrSaveMax2000.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_180E10CF.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_180E10CF.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_3117104D.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, 5416.bandselect.reg, customer1ani.reg, adhocchannelselect.reg, customer1roamPolicy.reg, smpsDynamic.reg, jupiter2ant.reg, htAdhocdisable.reg, customer1GreenTx.reg, j21swwow.reg, SleepTimePwrSaveMax2000.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3117104D.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3117104D.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration
AddReg  = MSI.reg

[ATHR_DEV_OS61_3027185F.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, aphroditeant2.reg, ledcontrol8.reg, ConnectionFailure.reg, aphroditeantdiv2.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_3027185F.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_3027185F.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS61_04031B9A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os61.reg, atheros11n.reg, htAdhoc.reg, triggerlevelkiteonly.reg, c3war.reg, ledcontrol9.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71            ; IF_TYPE_IEEE80211
*MediaType      = 16            ; NdisMediumNative802_11
*PhysicalMediaType = 9          ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS61_04031B9A.ndi.NTX86.Services]
AddService = athr, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS61_04031B9A.ndi.NTX86.HW]
Include = netvwifibus.inf
Needs   = VWiFiBus.PnPFilterRegistration

;;End of Others Section

[atheros_os61.reg]
HKR, Ndi,                           Service,    0, "athr"
HKR, Ndi\Interfaces,                UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,                LowerRange, 0, "wlan,ethernet,vwifi"

[atheros11n.reg]
HKR, Ndi\params\*ReceiveBuffers,    ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,    default,    0, "256"
HKR, Ndi\params\*ReceiveBuffers,    min,        0, "1"
HKR, Ndi\params\*ReceiveBuffers,    max,        0, "00000512"
HKR, Ndi\params\*ReceiveBuffers,    step,       0, "1"
HKR, Ndi\params\*ReceiveBuffers,    Base,       0, "10"
HKR, Ndi\params\*ReceiveBuffers,    type,       0, "int"
HKR, Ndi\params\*TransmitBuffers,   ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,   default,    0, "512"
HKR, Ndi\params\*TransmitBuffers,   min,        0, "1"
HKR, Ndi\params\*TransmitBuffers,   max,        0, "00000512"
HKR, Ndi\params\*TransmitBuffers,   step,       0, "1"
HKR, Ndi\params\*TransmitBuffers,   Base,       0, "10"
HKR, Ndi\params\*TransmitBuffers,   type,       0, "int"
HKR, Ndi\params\NetworkAddress,     ParamDesc,  0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,     default,    0,  ""
HKR, Ndi\params\NetworkAddress,     LimitText,  0,  "12"
HKR, Ndi\params\NetworkAddress,     UpperCase,  0,  "1"
HKR, Ndi\params\NetworkAddress,     optional,   0,  "1"
HKR, Ndi\params\NetworkAddress,     type,       0,  "edit"
HKR, Ndi\params\shortPreamble,      ParamDesc,  0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,      Base,       0,  "10"
HKR, Ndi\params\shortPreamble,      default,    0,  "1"
HKR, Ndi\params\shortPreamble,      type,       0,  "enum"
HKR, Ndi\params\shortPreamble\enum, "1",        0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0",        0,  %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,      ParamDesc,  0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,      default,    0,  "60"
HKR, Ndi\params\scanTimeValid,      min,        0,  "20"
HKR, Ndi\params\scanTimeValid,      max,        0,  "120"
HKR, Ndi\params\scanTimeValid,      step,       0,  "5"
HKR, Ndi\params\scanTimeValid,      base,       0,  "10"
HKR, Ndi\params\scanTimeValid,      type,       0,  "int"

;/* Enable these if VLAN or 802.1p is to be enabled */
;HKR, Ndi\Params\*PriorityVLANTag,  ParamDesc,  , %PriorityVLAN%
;HKR, Ndi\Params\*PriorityVLANTag,  default,    , "3"
;HKR, Ndi\Params\*PriorityVLANTag,  type,       , "enum"
;HKR, Ndi\Params\*PriorityVLANTag\enum, 0,      , %PriorityVLANDisabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 1,      , %PriorityEnabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 2,      , %VLANEnabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 3,      , %PriorityVLANEnabled%

[atheros.reg]
HKR, Ndi\params\*ReceiveBuffers,    ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,    default,    0, "256"
HKR, Ndi\params\*ReceiveBuffers,    min,        0, "1"
HKR, Ndi\params\*ReceiveBuffers,    max,        0, "00000512"
HKR, Ndi\params\*ReceiveBuffers,    step,       0, "1"
HKR, Ndi\params\*ReceiveBuffers,    Base,       0, "10"
HKR, Ndi\params\*ReceiveBuffers,    type,       0, "int"
HKR, Ndi\params\*TransmitBuffers,   ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,   default,    0, "256"
HKR, Ndi\params\*TransmitBuffers,   min,        0, "1"
HKR, Ndi\params\*TransmitBuffers,   max,        0, "00000512"
HKR, Ndi\params\*TransmitBuffers,   step,       0, "1"
HKR, Ndi\params\*TransmitBuffers,   Base,       0, "10"
HKR, Ndi\params\*TransmitBuffers,   type,       0, "int"
HKR, Ndi\params\NetworkAddress,     ParamDesc,  0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,     default,    0,  ""
HKR, Ndi\params\NetworkAddress,     LimitText,  0,  "12"
HKR, Ndi\params\NetworkAddress,     UpperCase,  0,  "1"
HKR, Ndi\params\NetworkAddress,     optional,   0,  "1"
HKR, Ndi\params\NetworkAddress,     type,       0,  "edit"
HKR, Ndi\params\shortPreamble,      ParamDesc,  0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,      Base,       0,  "10"
HKR, Ndi\params\shortPreamble,      default,    0,  "1"
HKR, Ndi\params\shortPreamble,      type,       0,  "enum"
HKR, Ndi\params\shortPreamble\enum, "1",        0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0",        0,  %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,      ParamDesc,  0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,      default,    0,  "60"
HKR, Ndi\params\scanTimeValid,      min,        0,  "20"
HKR, Ndi\params\scanTimeValid,      max,        0,  "120"
HKR, Ndi\params\scanTimeValid,      step,       0,  "5"
HKR, Ndi\params\scanTimeValid,      base,       0,  "10"
HKR, Ndi\params\scanTimeValid,      type,       0,  "int"

[atheros.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,ccode
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin
HKR,,halPcieClockReq
HKR,Ndi\params,MapRegisters,0x2000
HKR,,MapRegisters
HKR,Ndi\params,radioEnable,0x2000
HKR,Ndi\params,sleepMode,0x2000
HKR,,sleepMode
HKR,,gpioFunc0ActHi
HKR,,gpioFunc1ActHi
HKR,,gpioLedCustom
HKR,,gpioPinFunc0
HKR,,gpioPinFunc1
HKR,,transmitRateMax
HKR, Ndi\params\*TransmitBuffers
HKR,,*TransmitBuffers
HKR,,rxChainMask
HKR,,txChainMaskLegacy
HKR,,rxChainMaskLegacy
HKR,,rxChainDetect
HKR,,rxChainDetectRef
HKR,,rxChainDetectThreshA
HKR,,rxChainDetectThreshG
HKR,,rxChainDetectDeltaA
HKR,,rxChainDetectDeltaG
HKR, Ndi\params\smpsDynamic
HKR,,d3forcel1disable.reg
HKR,,d3forcel1disablekite.reg
HKR,,d3forcel1disablekite1.reg
HKR,,wmeEnabled
HKR,,halPcieWaen
HKR,,halPcieDetach
HKR,,ampEnable
HKR,Ndi\IHVExtensions
HKR,,roamPolicy
HKR,,btCoexAntDivEnable
HKR,,wowEnable
HKR,,GreenTx
HKR,,translateNullSsid
HKR,,defaultIbssChannel
HKR,,paprdEnable
HKR,,lnaDivUseBtAntEnable
HKR,,antCtrlComm2gSwitchEnable
HKR,,extLnaCtlGpio
HKR,,rateCtrlTxFastDrop
HKR,,antDivLowRssiCfg
HKR,,btCoexDivDefVal
HKR,,antDivFastDivBias
HKR,,halWakeUpCfg
HKR,,extAttenMarginCfg
HKR, Interrupt Management
HKR, Ndi\params\ignore11dBeacon
HKR,,ignore11dBeacon
HKR,,halShortRetry
HKR,,ampFilterName
HKR,,ampEnable
HKR,Ndi\params\ampEnable
HKR,,halWowNFRTC
HKR,,CMQ
HKR,,halWowOffload
HKR,,halWowOffloadBtTimeout
HKR,,halWakeupDelay
HKR,,halNlo
HKR,,enableReportNdisHWWowCap
HKR,,wowEnable
HKR,,WowEnablePME
HKR,,SleepTimePwrSaveMax
HKR,,SleepTimePwrSave
HKR,,SleepTimePerf
HKR,,AwakeTimePwrSaveMax
HKR,,AwakeTimePwrSave
HKR,,periodicScanEnable
HKR,,swBeaconProcess

[expresscardaspmoff.reg]
HKR, ,                                  pciDetectEnable,                0x00002,  "2"
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1"
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[rfKillDelayDetect.reg]
HKR, ,                                  rfKillDelayDetect,              0x00002,  "1"

[d3hot.reg] 
HKR, ,                                  halPciePowerReset,              0x00002,  "0"
HKR, ,                                  halPcieRestore,                 0x00002,  "1"

[enableswretry] 
HKR, ,                                  numSwRetries,                   0x00002,  "4"

[interruptpolling.reg]
HKR, ,                                  isrPollInterval,                0x00002,  "100"

[pcibusconfig.reg]
HKR, ,                                  BusConfig,                      0x00002,  "0"
HKR, ,                                  serializeRegMode,               0x00002,  "2"

[serializing.reg]
HKR, ,                                  serializeRegMode,               0x00002,  "1"

[bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,        %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,        "10"
HKR, Ndi\params\NetBand,                default,                        0,        "1647"
HKR, Ndi\params\NetBand,                type,                           0,        "enum"
HKR, Ndi\params\NetBand\enum,           "1647",                         0,        %Auto%
HKR, Ndi\params\NetBand\enum,           "1603",                         0,        %5GOnly%
HKR, Ndi\params\NetBand\enum,           "44",                           0,        %2GOnly%

[roamthreshA.reg]
HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,        %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,        "15"
HKR, Ndi\params\roamRssiA,              min,                            0,        "1"
HKR, Ndi\params\roamRssiA,              max,                            0,        "95"
HKR, Ndi\params\roamRssiA,              step,                           0,        "1"
HKR, Ndi\params\roamRssiA,              base,                           0,        "10"
HKR, Ndi\params\roamRssiA,              type,                           0,        "int"

[ignore11d.reg]
HKR,NDI\params\ignore11dBeacon,         ParamDesc,,                               %11DModeSwitch%
HKR,NDI\params\ignore11dBeacon,         type,,                                    "enum"
HKR,NDI\params\ignore11dBeacon,         Default,,                                 "1"
HKR,NDI\params\ignore11dBeacon\enum,    0,,                                       %Enable%
HKR,NDI\params\ignore11dBeacon\enum,    1,,                                       %Disable%

;[radioswitch.reg]
;HKR, Ndi\params\radioEnable,            ParamDesc,                      0,        %radioEnable%
;HKR, Ndi\params\radioEnable,            Base,                           0,        "10"
;HKR, Ndi\params\radioEnable,            default,                        0,        "1"
;HKR, Ndi\params\radioEnable,            type,                           0,        "enum"
;HKR, Ndi\params\radioEnable\enum,       "1",                            0,        %radioEnableOn%
;HKR, Ndi\params\radioEnable\enum,       "0",                            0,        %radioEnableOff%

[overridetxok.reg]
HKR, ,                                  OverrideTxOk,                   0x00002,  "1"

[adhocchannelselect.reg]
HKR, Ndi\params\defaultIbssChannel,     ParamDesc,                      0,        %adhocchannel%
HKR, Ndi\params\defaultIbssChannel,     default,                        0,        "10"
HKR, Ndi\params\defaultIbssChannel,     min,                            0,        "1"
HKR, Ndi\params\defaultIbssChannel,     max,                            0,        "11"
HKR, Ndi\params\defaultIbssChannel,     step,                           0,        "1"
HKR, Ndi\params\defaultIbssChannel,     base,                           0,        "10"
HKR, Ndi\params\defaultIbssChannel,     type,                           0,        "int"

[5416.bgnxb.reg]
HKR, ,                                  NetBand,                        0x00002,  "26636"
HKR, ,                                  wmodeselect,                    0x00002,  "26636"

[5416.bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "130671"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "130671",                       0,  %Auto%
HKR, Ndi\params\NetBand\enum,           "104003",                       0,  %5GOnly%
HKR, Ndi\params\NetBand\enum,           "26668",                        0,  %2GOnly%

[wirelessmodeselectCompex.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "130671"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "1",                            0,  %11AOnly%
HKR, Ndi\params\NetBand\enum,           "104003",                       0,  %11ANOnly%
HKR, Ndi\params\NetBand\enum,           "12",                           0,  %11BGOnly%
HKR, Ndi\params\NetBand\enum,           "26668",                        0,  %11BGNOnly%
HKR, Ndi\params\NetBand\enum,           "130671",                       0,  %11ABGN%

[wirelessmodeselectkite.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "26636"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "26636",                        0,  %WirelessModeAuto%
HKR, Ndi\params\NetBand\enum,           "12",                           0,  %WirelessMode11bgOnly%

[5416.antennacontrols.reg] 
HKR, ,                                  rxChainMask,                    0x00002,  "7"
;HKR, ,                                  txChainMaskLegacy,              0x00002,  "5"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "7"
HKR, ,                                  rxChainDetect,                  0x00002,  "1"
HKR, ,                                  rxChainDetectRef,               0x00002,  "0"
HKR, ,                                  rxChainDetectThreshA,           0x00002,  "0"
HKR, ,                                  rxChainDetectThreshG,           0x00002,  "0"
HKR, ,                                  rxChainDetectDeltaA,            0x00002,  "20"
HKR, ,                                  rxChainDetectDeltaG,            0x00002,  "20"

[9485BTcoex.reg]
HKR, ,                                  wlanActiveGpioSelect,           0x00002,  "5"
HKR, ,                                  btActiveGpioSelect,             0x00002,  "4"
HKR, ,                                  btPriorityGpioSelect,           0x00002,  "8"
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "0"

[9485BTcoexPTA.reg]
HKR, ,                                  wlanActiveGpioSelect,           0x00002,  "5"
HKR, ,                                  btActiveGpioSelect,             0x00002,  "4"
HKR, ,                                  btPriorityGpioSelect,           0x00002,  "8"
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "3932161"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "0"

[9485BTCoexAgent0.reg]
HKR, ,                                  wlanActiveGpioSelect,           0x00002,  "5"
HKR, ,                                  btActiveGpioSelect,             0x00002,  "4"
HKR, ,                                  btPriorityGpioSelect,           0x00002,  "8"
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "0"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "0"

[9485BTcoexDivEn.reg]
HKR, ,                                  wlanActiveGpioSelect,           0x00002,  "5"
HKR, ,                                  btActiveGpioSelect,             0x00002,  "4"
HKR, ,                                  btPriorityGpioSelect,           0x00002,  "8"
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "3932161"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "3"
HKR, ,                                  antDivLowRssiCfg,               0x00002,  "20"
HKR, ,                                  antDivFastDivBias,              0x00002,  "3"
HKR, ,                                  btCoexDivDefVal,                0x00002,  "1"

[9485BTcoexDivEn_1.reg]
HKR, ,                                  wlanActiveGpioSelect,           0x00002,  "5"
HKR, ,                                  btActiveGpioSelect,             0x00002,  "4"
HKR, ,                                  btPriorityGpioSelect,           0x00002,  "8"
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "3"
HKR, ,                                  antDivLowRssiCfg,               0x00002,  "20"
HKR, ,                                  antDivFastDivBias,              0x00002,  "3"
HKR, ,                                  btCoexDivDefVal,                0x00002,  "1"

[pushbutton.reg]
HKR, ,                                  wpsButtonGpio,                  0x00002,  "9"

[smpsDynamic.reg]
HKR, Ndi\params\smpsDynamic,            ParamDesc,  0,  %smpsDynamic%
HKR, Ndi\params\smpsDynamic,            Base,       0,  "10"
HKR, Ndi\params\smpsDynamic,            default,    0,  "0"
HKR, Ndi\params\smpsDynamic,            type,       0,  "enum"
HKR, Ndi\params\smpsDynamic\enum,       "1",        0,  %Enable%
HKR, Ndi\params\smpsDynamic\enum,       "0",        0,  %Disable%

[amp.reg]
HKR, ,                                  ampEnable,                      0x00002,  "1"
HKR, Ndi\params\ampEnable,              ParamDesc,                      0,        %bt30%
HKR, Ndi\params\ampEnable,              default,                        0,        "1"
HKR, Ndi\params\ampEnable,              type,                           0,        "enum"
HKR, Ndi\params\ampEnable\enum,         "1",                            0,        %bt30enable%
HKR, Ndi\params\ampEnable\enum,         "0",                            0,        %bt30disable%

[ampTFilter.reg]
HKR, ,                                  ampFilterName,                  0x00002,  "ATHAMPFLx"

[ampBFilter.reg]
HKR, ,                                  ampFilterName,                  0x00002,  "BTWAMPFL"

[ampFilter.reg]
HKR, ,                                  ampFilterName,                  0x00002,  "ATHAMPFL"

[ampGUID.reg]
HKR, ,                                  ampGUID,                        0x00002,  "1"

[amp_default.reg]
HKR, ,                                  ampEnable,                      0x00002,  "0"
HKR, Ndi\params\ampEnable,              ParamDesc,                      0,        %bt30%
HKR, Ndi\params\ampEnable,              default,                        0,        "0"
HKR, Ndi\params\ampEnable,              type,                           0,        "enum"
HKR, Ndi\params\ampEnable\enum,         "1",                            0,        %bt30enable%
HKR, Ndi\params\ampEnable\enum,         "0",                            0,        %bt30disable%

[customer0.reg]
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,                                  scanTimePreSleep,               0x00002,  "60" 
HKR, ,                                  capLinkSp,                      0x00002,  "1" 
HKR, ,                                  pcieAspm,                       0x00002,  "2" 
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1" 
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer0_HB95.reg]
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,                                  scanTimePreSleep,               0x00002,  "60" 
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer0_HB93.reg]
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR, ,                                  scanTimePreSleep,               0x00002,  "60" 
HKR, ,                                  pcieAspm,                       0x00002,  "2" 
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1" 
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customerop.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[customer0LED.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "0"

[customer0LED1.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"

[customer0LED2.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"

[customer0_11n.reg]
;PCIe Related
HKR, ,                                  radioEnableInterval,            0x00002,  "5"
HKR, ,                                  pcieAspm,                       0x00002,  "2"
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  forceWake,                      0x00002,  "0"
HKR, ,                                  antennaSwitchSwap,              0x00002,  "1"
;LED Related
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
;General Customer0
HKR, ,                                  ssid,                           0x00002,  "randomssidtoshutoffautoconnectib"
HKR,NDI\params\ignore11dBeacon,ParamDesc,,      %11DModeSwitch%
HKR,NDI\params\ignore11dBeacon,type,,           "enum"
HKR,NDI\params\ignore11dBeacon,Default,,        "1"
HKR,NDI\params\ignore11dBeacon\enum,0,,         %Enable%
HKR,NDI\params\ignore11dBeacon\enum,1,,         %Disable%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,  %roamRssiA%
HKR, Ndi\params\roamRssiA,              default,                        0,  "15"
HKR, Ndi\params\roamRssiA,              min,                            0,  "1"
HKR, Ndi\params\roamRssiA,              max,                            0,  "95"
HKR, Ndi\params\roamRssiA,              step,                           0,  "1"
HKR, Ndi\params\roamRssiA,              base,                           0,  "10"
HKR, Ndi\params\roamRssiA,              type,                           0,  "int"

HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,  %scanTime%
HKR, Ndi\params\scanTimeValid,          default,                        0,  "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,  "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,  "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,  "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,  "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,  "int"

[customer1ani.reg]
HKR, Ndi\params\rssiThrHigh,            ParamDesc,                      0,        %rssiThrHigh%
HKR, Ndi\params\rssiThrHigh,            Base,                           0,        "10"
HKR, Ndi\params\rssiThrHigh,            default,                        0,        "40"
HKR, Ndi\params\rssiThrHigh,            type,                           0,        "enum"
HKR, Ndi\params\rssiThrHigh\enum,       "40",                           0,        %rssiThrHighNormal%
HKR, Ndi\params\rssiThrHigh\enum,       "32",                           0,        %rssiThrHighMin%

[customer1roamPolicy.reg]
HKR, Ndi\params\roamPolicy,             ParamDesc,                      0,        %roamPolicy%
HKR, Ndi\params\roamPolicy,             Base,                           0,        "10"
HKR, Ndi\params\roamPolicy,             default,                        0,        "3"
HKR, Ndi\params\roamPolicy,             type,                           0,        "enum"
HKR, Ndi\params\roamPolicy\enum,        "1",                            0,        %roamPolicyVeryLow%
HKR, Ndi\params\roamPolicy\enum,        "2",                            0,        %roamPolicyLow%
HKR, Ndi\params\roamPolicy\enum,        "3",                            0,        %roamPolicyNormal%
HKR, Ndi\params\roamPolicy\enum,        "4",                            0,        %roamPolicyHigh%
HKR, Ndi\params\roamPolicy\enum,        "5",                            0,        %roamPolicyVeryHigh%

[customer1GreenTx.reg]
HKR, Ndi\params\GreenTx,                ParamDesc,                      0,        %GreenTx%
HKR, Ndi\params\GreenTx,                Base,                           0,        "10"
HKR, Ndi\params\GreenTx,                default,                        0,        "0"
HKR, Ndi\params\GreenTx,                type,                           0,        "enum"
HKR, Ndi\params\GreenTx\enum,           "0",                            0,        %GreenTxEnableOff%
HKR, Ndi\params\GreenTx\enum,           "1",                            0,        %GreenTxEnableOn%

[customer2GreenTx.reg]
HKR, ,                                  GreenTx,                            0x00002,  "15"

[customer_power_Toshiba.reg]
HKR, ,                                  SleepTimePwrSave,               0x00002,  "1000"
HKR, ,                                  SleepTimePerf,                  0x00002,  "1000"
HKR, ,                                  PsActivityCheckInterval,		0x00002,  "4"
HKR, ,                                  AwakeTimePwrSaveMax,            0x00002,  "35"
HKR, ,                                  AwakeTimePwrSave,               0x00002,  "35"
HKR, ,                                  periodicScanEnable,             0x00002,  "0"
HKR, ,                                  swBeaconProcess,                0x00002,  "0"

[power_management.reg]
HKR, ,                                  PsActivityCheckInterval,		0x00002,  "4"
HKR, ,                                  AwakeTimePwrSaveMax,            0x00002,  "35"
HKR, ,                                  AwakeTimePwrSave,               0x00002,  "35"
HKR, ,                                  bkScanEnable,               	0x00002,  "0"
HKR, ,                                  swBeaconProcess,				0x00002,  "0"

[customer2.reg]
HKR,,                                   linkLEDFunc,                    0,        "53"
HKR,,                                   activityLEDFunc,                0,        "51"
HKR,,                                   connectionLEDFunc,              0,        "55"

[customer2.11n.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"

[customer2merlin.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"

[customer3.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  LinkLEDFunc,                    0x00002,  "19"
HKR, ,                                  ActivityLEDFunc,                0x00002,  "21"

;add by alan liu for liteon PCIE 1.1
[customer3gpcie11.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "6"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "6"
HKR, ,                                  gpioPinFunc2,                   0x00002,  "6"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"
;-----------------------------------------------------------------------------------------------------

[customer3a.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

;[customer3b.reg]
;HKR, ,                                  gpioPinFunc1,                  0x00002,  "3"
;HKR, ,                                  overrideACstatus,              0x00002,  "1"
;HKR, ,                                  halPcieClockReq,               0x00002,  "0"
;HKR, ,                                  gpioLedCustom,                 0x00002,  "4"
;HKR, ,                                  gpioFunc1ActHi,                0x00002,  "0"

[customer3c.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer3d.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "0"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer3e.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer3f.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "8"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer3g.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "6"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer3h.reg]
HKR, ,                                  scanTimePreSleep,               0x00002,  "60"
HKR, ,                                  SleepTimePerf,                  0x00002,  "500"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "4"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[customer3_legacybgwmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "12"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "4",                            0,        %wModeLegacy11bonly%
HKR, Ndi\params\wModeSelect\enum,       "12",                           0,        %wModeLegacy11bg%

[customer4.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4a.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4as.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "8"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4adhoc.reg]
HKR, ,                                  defaultIbssChannel,             0x00002,  "11"

[customer4b.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "3"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  halPcieClockReq,                0x00002,  "0"
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4c.reg]
HKR, ,                                  translateNullSsid,              0x00002,  "1"
HKR, ,                                  AwakeTimePerf,                  0x00002,  "200"

[customer4a_ASPM.reg]
HKR, ,                                  pcieAspm,                       0x00002,  "0"

[customer5Led.reg]
HKR, ,                                  softLEDEnable,                  0x00002,  "1"
HKR, ,                                  swapDefaultLED,                 0x00002,  "1"

[customer5.11nLED.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "1"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "2"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "0"

[customer5.PCIe11nLed.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[customer5.3x3.reg]
HKR, ,                                  txChainMask,                    0x00002,  "7"
HKR, ,                                  rxChainMask,                    0x00002,  "7"

[customer7Led.reg]
HKR, ,                                  gpioLedCustom,                  0x00002,  "2"
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "2"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"
HKR, ,                                  gpioFunc1ActHi,                 0x00002,  "1"

[customer9Led.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"

[Customer15a.led.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[Customer15b.led.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[gpioled.reg]
HKR,,                                   linkLEDFunc,                    0,        "49"
HKR,,                                   activityLEDFunc,                0,        "51"
HKR,,                                   connectionLEDFunc,              0,        "55"

[ratecap.reg]
HKR, ,                                  txCoalescingEnable,             0x00002,  "1"

[customer11n.reg]
HKR, Ndi\params\*ReceiveBuffers,        ParamDesc,                      0,        "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,        default,                        0,        "256"
HKR, Ndi\params\*ReceiveBuffers,        min,                            0,        "1"
HKR, Ndi\params\*ReceiveBuffers,        max,                            0,        "00000512"
HKR, Ndi\params\*ReceiveBuffers,        step,                           0,        "1"
HKR, Ndi\params\*ReceiveBuffers,        Base,                           0,        "10"
HKR, Ndi\params\*ReceiveBuffers,        type,                           0,        "int"
HKR, Ndi\params\*TransmitBuffers,       ParamDesc,                      0,        "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,       default,                        0,        "512"
HKR, Ndi\params\*TransmitBuffers,       min,                            0,        "1"
HKR, Ndi\params\*TransmitBuffers,       max,                            0,        "00000512"
HKR, Ndi\params\*TransmitBuffers,       step,                           0,        "1"
HKR, Ndi\params\*TransmitBuffers,       Base,                           0,        "10"
HKR, Ndi\params\*TransmitBuffers,       type,                           0,        "int"
HKR, Ndi\params\shortPreamble,          ParamDesc,                      0,        %shortPreamble%
HKR, Ndi\params\shortPreamble,          Base,                           0,        "10"
HKR, Ndi\params\shortPreamble,          default,                        0,        "1"
HKR, Ndi\params\shortPreamble,          type,                           0,        "enum"
HKR, Ndi\params\shortPreamble\enum,     "1",                            0,        %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum,     "0",                            0,        %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,          ParamDesc,                      0,        %scanTimeValid%
HKR, Ndi\params\scanTimeValid,          default,                        0,        "60"
HKR, Ndi\params\scanTimeValid,          min,                            0,        "20"
HKR, Ndi\params\scanTimeValid,          max,                            0,        "120"
HKR, Ndi\params\scanTimeValid,          step,                           0,        "5"
HKR, Ndi\params\scanTimeValid,          base,                           0,        "10"
HKR, Ndi\params\scanTimeValid,          type,                           0,        "int"

[customer11.reg]
HKR, Ndi\params\*ReceiveBuffers,    ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,    default,    0, "256"
HKR, Ndi\params\*ReceiveBuffers,    min,        0, "1"
HKR, Ndi\params\*ReceiveBuffers,    max,        0, "00000512"
HKR, Ndi\params\*ReceiveBuffers,    step,       0, "1"
HKR, Ndi\params\*ReceiveBuffers,    Base,       0, "10"
HKR, Ndi\params\*ReceiveBuffers,    type,       0, "int"
HKR, Ndi\params\*TransmitBuffers,   ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,   default,    0, "256"
HKR, Ndi\params\*TransmitBuffers,   min,        0, "1"
HKR, Ndi\params\*TransmitBuffers,   max,        0, "00000512"
HKR, Ndi\params\*TransmitBuffers,   step,       0, "1"
HKR, Ndi\params\*TransmitBuffers,   Base,       0, "10"
HKR, Ndi\params\*TransmitBuffers,   type,       0, "int"
HKR, Ndi\params\shortPreamble,      ParamDesc,  0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,      Base,       0,  "10"
HKR, Ndi\params\shortPreamble,      default,    0,  "1"
HKR, Ndi\params\shortPreamble,      type,       0,  "enum"
HKR, Ndi\params\shortPreamble\enum, "1",        0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0",        0,  %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,      ParamDesc,  0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,      default,    0,  "60"
HKR, Ndi\params\scanTimeValid,      min,        0,  "20"
HKR, Ndi\params\scanTimeValid,      max,        0,  "120"
HKR, Ndi\params\scanTimeValid,      step,       0,  "5"
HKR, Ndi\params\scanTimeValid,      base,       0,  "10"
HKR, Ndi\params\scanTimeValid,      type,       0,  "int"

[customer11custom.reg]
HKR, Ndi\params\bkScanEnable,           ParamDesc,                      0,        %bkScanEnable%
HKR, Ndi\params\bkScanEnable,           Base,                           0,        "10"
HKR, Ndi\params\bkScanEnable,           default,                        0,        "1"
HKR, Ndi\params\bkScanEnable,           type,                           0,        "enum"
HKR, Ndi\params\bkScanEnable\enum,      "1",                            0,        %bkScanEnableOn%
HKR, Ndi\params\bkScanEnable\enum,      "0",                            0,        %bkScanEnableOff%

HKR, Ndi\params\radioEnable,            ParamDesc,                      0,        %radioEnable%
HKR, Ndi\params\radioEnable,            Base,                           0,        "10"
HKR, Ndi\params\radioEnable,            default,                        0,        "1"
HKR, Ndi\params\radioEnable,            type,                           0,        "enum"
HKR, Ndi\params\radioEnable\enum,       "1",                            0,        %radioEnableOn%
HKR, Ndi\params\radioEnable\enum,       "0",                            0,        %radioEnableOff%

HKR, Ndi\params\roamRssiA,              ParamDesc,                      0,        %roamRssi11A%
HKR, Ndi\params\roamRssiA,              default,                        0,        "15"
HKR, Ndi\params\roamRssiA,              min,                            0,        "1"
HKR, Ndi\params\roamRssiA,              max,                            0,        "95"
HKR, Ndi\params\roamRssiA,              step,                           0,        "1"
HKR, Ndi\params\roamRssiA,              base,                           0,        "10"
HKR, Ndi\params\roamRssiA,              type,                           0,        "int"

HKR, Ndi\params\roamRssiBOnly,          ParamDesc,                      0,        %roamRssi11BOnly%
HKR, Ndi\params\roamRssiBOnly,          default,                        0,        "8"
HKR, Ndi\params\roamRssiBOnly,          min,                            0,        "0"
HKR, Ndi\params\roamRssiBOnly,          max,                            0,        "95"
HKR, Ndi\params\roamRssiBOnly,          step,                           0,        "1"
HKR, Ndi\params\roamRssiBOnly,          base,                           0,        "10"
HKR, Ndi\params\roamRssiBOnly,          type,                           0,        "int"

HKR, Ndi\params\roamRssiB,              ParamDesc,                      0,        %roamRssi11B%
HKR, Ndi\params\roamRssiB,              default,                        0,        "24"
HKR, Ndi\params\roamRssiB,              min,                            0,        "0"
HKR, Ndi\params\roamRssiB,              max,                            0,        "95"
HKR, Ndi\params\roamRssiB,              step,                           0,        "1"
HKR, Ndi\params\roamRssiB,              base,                           0,        "10"
HKR, Ndi\params\roamRssiB,              type,                           0,        "int"

HKR, Ndi\params\roamRateA,              ParamDesc,                      0,        %roamRateA%
HKR, Ndi\params\roamRateA,              Base,                           0,        "10"
HKR, Ndi\params\roamRateA,              default,                        0,        "24000"
HKR, Ndi\params\roamRateA,              type,                           0,        "enum"
HKR, Ndi\params\roamRateA\enum,         "6000",                         0,        %roamRateA6M%
HKR, Ndi\params\roamRateA\enum,         "9000",                         0,        %roamRateA9M%
HKR, Ndi\params\roamRateA\enum,         "12000",                        0,        %roamRateA12M%
HKR, Ndi\params\roamRateA\enum,         "18000",                        0,        %roamRateA18M%
HKR, Ndi\params\roamRateA\enum,         "24000",                        0,        %roamRateA24M%
HKR, Ndi\params\roamRateA\enum,         "36000",                        0,        %roamRateA36M%
HKR, Ndi\params\roamRateA\enum,         "48000",                        0,        %roamRateA48M%
HKR, Ndi\params\roamRateA\enum,         "54000",                        0,        %roamRateA54M%

HKR, Ndi\params\roamRateBOnly,          ParamDesc,                      0,        %roamRateBOnly%
HKR, Ndi\params\roamRateBOnly,          Base,                           0,        "10"
HKR, Ndi\params\roamRateBOnly,          default,                        0,        "5000"
HKR, Ndi\params\roamRateBOnly,          type,                           0,        "enum"
HKR, Ndi\params\roamRateBOnly\enum,     "1000",                         0,        %roamRateBOnly1M%
HKR, Ndi\params\roamRateBOnly\enum,     "2000",                         0,        %roamRateBOnly2M%
HKR, Ndi\params\roamRateBOnly\enum,     "5000",                         0,        %roamRateBOnly5M%
HKR, Ndi\params\roamRateBOnly\enum,     "11000",                        0,        %roamRateBOnly11M%

HKR, Ndi\params\roamRateB,              ParamDesc,                      0,        %roamRateB%
HKR, Ndi\params\roamRateB,              Base,                           0,        "10"
HKR, Ndi\params\roamRateB,              default,                        0,        "9000"
HKR, Ndi\params\roamRateB,              type,                           0,        "enum"
HKR, Ndi\params\roamRateB\enum,         "1000",                         0,        %roamRateB1M%
HKR, Ndi\params\roamRateB\enum,         "2000",                         0,        %roamRateB2M%
HKR, Ndi\params\roamRateB\enum,         "5000",                         0,        %roamRateB5M%
HKR, Ndi\params\roamRateB\enum,         "6000",                         0,        %roamRateB6M%
HKR, Ndi\params\roamRateB\enum,         "9000",                         0,        %roamRateB9M%
HKR, Ndi\params\roamRateB\enum,         "11000",                        0,        %roamRateB11M%

HKR, Ndi\params\pcieAspm,               ParamDesc,                      0,        %pcieAspm%
HKR, Ndi\params\pcieAspm,               Base,                           0,        "10"
HKR, Ndi\params\pcieAspm,               default,                        0,        "0"
HKR, Ndi\params\pcieAspm,               type,                           0,        "enum"
HKR, Ndi\params\pcieAspm\enum,          "0",                            0,        %pcieAspmOff%
HKR, Ndi\params\pcieAspm\enum,          "1",                            0,        %pcieAspmL0sOn%
HKR, Ndi\params\pcieAspm\enum,          "2",                            0,        %pcieAspmL1On%
HKR, Ndi\params\pcieAspm\enum,          "3",                            0,        %pcieAspmL0sandL1On%

[customer11_11n40wmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "129055"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "26628",                        0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "102403",                       0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "26652",                        0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "129055",                       0,        %wModeSelect11abgn%

[customer11_11nwmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "6175"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "2052",                         0,        %wModeSelect11bonly%
HKR, Ndi\params\wModeSelect\enum,       "4099",                         0,        %wModeSelect11na%
HKR, Ndi\params\wModeSelect\enum,       "2076",                         0,        %wModeSelect11nbg%
HKR, Ndi\params\wModeSelect\enum,       "6175",                         0,        %wModeSelect11abgn%

[customer11_legacywmode.reg]
HKR, Ndi\params\wModeSelect,            ParamDesc,                      0,        %wModeSelect%
HKR, Ndi\params\wModeSelect,            Base,                           0,        "10"
HKR, Ndi\params\wModeSelect,            default,                        0,        "31"
HKR, Ndi\params\wModeSelect,            type,                           0,        "enum"
HKR, Ndi\params\wModeSelect\enum,       "4",                            0,        %wModeLegacy11bonly%
HKR, Ndi\params\wModeSelect\enum,       "3",                            0,        %wModeLegacy11a%
HKR, Ndi\params\wModeSelect\enum,       "28",                           0,        %wModeLegacy11bg%
HKR, Ndi\params\wModeSelect\enum,       "31",                           0,        %wModeLegacy11abg%

[customer11Ant.reg]
HKR, Ndi\params\antennaSwitch,          ParamDesc,                      0,        %antennaSwitch%
HKR, Ndi\params\antennaSwitch,          Base,                           0,        "10"
HKR, Ndi\params\antennaSwitch,          default,                        0,        "2"
HKR, Ndi\params\antennaSwitch,          type,                           0,        "enum"
HKR, Ndi\params\antennaSwitch\enum,     "0",                            0,        %antennaSwitchA%
HKR, Ndi\params\antennaSwitch\enum,     "1",                            0,        %antennaSwitchB%
HKR, Ndi\params\antennaSwitch\enum,     "2",                            0,        %antennaSwitchAuto%

[customer_GigaByte.reg]
HKR, ,                          txChainMask,          0x00002,  "5"

[customer_GigaByteLed0.reg]
HKR, ,                                  LinkLedFunc,                    0, "19"
HKR, ,                                  ActivityLedFunc,        0, "21" 

[customer_GigaByteLed1.reg]
HKR, ,                                  LinkLedFunc,                    0, "03"
HKR, ,                                  ActivityLedFunc,                0, "05"

[customer_GigaByteLed2.reg]
HKR, ,                                  LinkLedFunc,                    0, "07"
HKR, ,                                  ActivityLedFunc,                0, "05"

[customer_Samsung.reg]
HKR, Ndi\params\sleepMode,                ParamDesc,                      0,  %PowerSaveMode%
HKR, Ndi\params\sleepMode,                Base,                           0,  "10"
HKR, Ndi\params\sleepMode,                default,                        0,  "2"
HKR, Ndi\params\sleepMode,                type,                           0,  "enum"
HKR, Ndi\params\sleepMode\enum,           "0",                            0,  %Off%
HKR, Ndi\params\sleepMode\enum,           "1",                            0,  %Maximum%
HKR, Ndi\params\sleepMode\enum,           "2",                            0,  %Normal%
HKR, ,                                  pcieAspm,                       0x00002,  "2" 
HKR, ,                                  halPciePowerSaveEnable,         0x00002,  "1" 

[ignore11denable.reg]
HKR, ,                                  ignore11dBeacon,                0x00002,  "1" 

[xb72.via.reg]
HKLM, SYSTEM\CurrentControlSet\Services\pci\Parameters,168c0024,0x00000001, 00,00,00,20,00,00,00,00

[rssiAdjust.reg]
HKR, ,                                  rssiAdjust,                     0x00002,  "7"

[cmdRegister.reg]
HKR, ,                                  cmdRegister,                    0x00002,  "838"

[htAdhocdisable.reg]
HKR, ,                                  htAdhocEnable,                  0x00002,  "0"

[htAdhoc.reg]
HKR, NDI\params\htAdhocEnable,ParamDesc,,       %AdHoc11n%
HKR, NDI\params\htAdhocEnable,type,,            "enum"
HKR, NDI\params\htAdhocEnable,Default,,         "0"
HKR, NDI\params\htAdhocEnable\enum,0,,          %Disable%
HKR, NDI\params\htAdhocEnable\enum,1,,          %Enable%

[AdhocModeSelect.reg]
HKR, NDI\params\AdhocModeSelect,ParamDesc,,             %AdhocMode%
HKR, NDI\params\AdhocModeSelect,type,,                  "enum"
HKR, NDI\params\AdhocModeSelect,Default,,               "2"
HKR, NDI\params\AdhocModeSelect\enum,0,,                %wModeSelect11g%
HKR, NDI\params\AdhocModeSelect\enum,1,,                %wModeSelect11n%
HKR, NDI\params\AdhocModeSelect\enum,2,,                %wModeSelect11b%

[edmaStopRecvDelay.reg]
HKR, ,                                  edmaStopRecvDelay,              0x10001,  3

[htWepTkipOpt.reg]
HKR, Ndi\params\htEnableWepTkip,ParamDesc,  0,  %WepTkip11n%
HKR, NDI\params\htEnableWepTkip,type,,          "enum"
HKR, NDI\params\htEnableWepTkip,Default,,       "1"
HKR, NDI\params\htEnableWepTkip\enum,0,,        %Disable%
HKR, NDI\params\htEnableWepTkip\enum,1,,        %Enable%

[htEnableWepTkip.reg]
HKR, ,                                  htEnableWepTkip,                  0x00002,  "1"

[cemspecled_func1_1.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func1_3.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "3"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func1_6.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "6"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func1_8.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "8"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[cemspecled_func2_1.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[cemspecled_func2_8.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "8"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[cemspecled_func2_6.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "6"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[cemspecled_func0_1.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"

[cemspecled_func0_6.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "6"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"

[cemspecled_func2_10.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "10"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[cemspecled_func1_10.reg]
HKR, ,                                  gpioPinFunc1,                   0x00002,  "10"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[d3forcel1disable.reg]
HKR, ,                                  halPcieWaen,                    0x00002,  "4212539"

[d3forcel1disable1.reg]
HKR, ,                                  halPcieWaen,                         0x00002,  "4212539"
HKR, ,                                  halPcieDetach,                    0x00002,  "1"

[maxpowersave.reg]
HKR, ,                                  sleepTimePwrSave,               0x00002,  "1000"
HKR, ,                                  SleepTimePerf,                  0x00002,  "1000"

[maxpowersave2.reg]
HKR, ,                                  sleepTimePwrSave,               0x00002,  "1000"
HKR, ,                                  SleepTimePerf,                  0x00002,  "1000"
HKR, ,                                  AwakeTimePwrSaveMax,            0x00002,  "150"

[customer_IODATA.reg]
HKR, ,                                  LinkLedFunc,                    0, "49"
HKR, ,                                  ActivityLedFunc,                0, "51"

[janusda.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "0"

[janusda_coexPTA_40_21.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "21"

[janusda_CoexAgent0.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "0"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "0"

[roamPolicy.reg]
HKR, Ndi\params\roamPolicy,             ParamDesc,                      0,        %roamPolicy%
HKR, Ndi\params\roamPolicy,             Base,                           0,        "10"
HKR, Ndi\params\roamPolicy,             default,                        0,        "3"
HKR, Ndi\params\roamPolicy,             type,                           0,        "enum"
HKR, Ndi\params\roamPolicy\enum,        "1",                            0,        %roamPolicyVeryLow%
HKR, Ndi\params\roamPolicy\enum,        "2",                            0,        %roamPolicyLow%
HKR, Ndi\params\roamPolicy\enum,        "3",                            0,        %roamPolicyNormal%
HKR, Ndi\params\roamPolicy\enum,        "4",                            0,        %roamPolicyHigh%
HKR, Ndi\params\roamPolicy\enum,        "5",                            0,        %roamPolicyVeryHigh%

[roamPolicy2.reg]
HKR, Ndi\params\roamPolicy,             ParamDesc,                      0,        %roamPolicy%
HKR, Ndi\params\roamPolicy,             Base,                           0,        "10"
HKR, Ndi\params\roamPolicy,             default,                        0,        "3"
HKR, Ndi\params\roamPolicy,             type,                           0,        "enum"
HKR, Ndi\params\roamPolicy\enum,        "1",                            0,        %roamPolicyVeryLow2%
HKR, Ndi\params\roamPolicy\enum,        "2",                            0,        %roamPolicyLow2%
HKR, Ndi\params\roamPolicy\enum,        "3",                            0,        %roamPolicyNormal2%
HKR, Ndi\params\roamPolicy\enum,        "4",                            0,        %roamPolicyHigh2%
HKR, Ndi\params\roamPolicy\enum,        "5",                            0,        %roamPolicyVeryHigh2%

[hb97ChainMask.reg]
HKR, ,                                  txChainMaskLegacy,              0x00002,  "3"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "3"

[heliusda.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btModule,                       0x00002,  "2"
HKR, ,                                  txCoalescingEnable,             0x00002,  "1"
HKR, ,                                  txChainMaskLegacy,              0x00002,  "2"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "2"
HKR, ,                                  btCoexEnhanceA2DP,              0x00002,  "70"

[WB197da.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btModule,                       0x00002,  "2"
HKR, ,                                  txCoalescingEnable,             0x00002,  "1"
HKR, ,                                  txChainMaskLegacy,              0x00002,  "3"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "3"
HKR, ,                                  btCoexEnhanceA2DP,              0x00002,  "70"

[btcoexa2dp99.reg]
HKR, ,                                  btCoexEnhanceA2DP,              0x00002,  "99"

[jupiter2ant.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "5"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  halPllPwrSave,                  0x00002,  "7"
HKR, ,                                  txChainMaskLegacy,              0x00002,  "2"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "3"

[jupiter2ant2.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "5"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  halPllPwrSave,                  0x00002,  "7"
HKR, ,                                  txChainMaskLegacy,              0x00002,  "3"
HKR, ,                                  rxChainMaskLegacy,              0x00002,  "3"

[aphroditeant.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "5"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  halPllPwrSave,                  0x00002,  "7"
HKR, ,                                  mciConfig,                      0x00000,  "16819393"
HKR, ,                                  btCoexLowACKPwr,                0x00000,  "1835777"
HKR, ,                                  btCoexStompA2DPCfg,             0x00000,  "24323329"
HKR, ,                                  btCoexStompSCOCfg,              0x00000,  "25502465"
HKR, ,                                  btCoexMiscCfg,                  0x00000,  "5"
HKR, ,                                  btCoexdisablePKDET,             0x00000,  "949"

[aphroditeantTS.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "5"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  halPllPwrSave,                  0x00002,  "7"
HKR, ,                                  mciConfig,                      0x00000,  "16819393"
HKR, ,                                  btCoexLowACKPwr,                0x00000,  "1835777"
HKR, ,                                  btCoexStompA2DPCfg,             0x00000,  "24323329"
HKR, ,                                  btCoexStompSCOCfg,              0x00000,  "25502465"
HKR, ,                                  btCoexMiscCfg,                  0x00000,  "7"
HKR, ,                                  btCoexdisablePKDET,             0x00000,  "949"

[aphroditeant2.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "5"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  halPllPwrSave,                  0x00002,  "7"
HKR, ,                                  mciConfig,                      0x00000,  "33596642"
HKR, ,                                  btCoexLowACKPwr,                0x00000,  "2622209"
HKR, ,                                  btCoexStompA2DPCfg,             0x00000,  "24323329"
HKR, ,                                  btCoexStompSCOCfg,              0x00000,  "25502465"
HKR, ,                                  btCoexMiscCfg,                  0x00000,  "1"

[aphroditeantdiv.reg]
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "3"
HKR, ,                                  lnaDivUseBtAntEnable,           0x00002,  "1"

[aphroditeantdiv2.reg]
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "3"
HKR, ,                                  btCoexDivDefVal,                0x00002,  "1"
HKR, ,                                  lnaDivUseBtAntEnable,           0x00002,  "1"

[merlinshiftdelay.reg]
HKR, ,                                  analogShiftRegDelay,            0x00002,  "10"

[tpshiftdelay.reg]
HKR, ,                                  analogShiftRegDelay,            0x00002,  "30"

[minpower.reg]
HKR, ,                                  legacyMinTxPowerLimit,          0x00002,  "10"

[wowenable.reg]
HKR, ,                                  wowEnable,                      0x00002,  "1"
HKR, ,                                  CMQ,                            0x00002,  "0"

[j21swwow.reg]
HKR, ,                                  halWowOffload,                  0x00010001,  0x00e3ec01
HKR, ,                                  halWowOffloadBtTimeout,         0x00010001,  0x00000030
HKR, ,                                  halWakeupDelay,                 0x00010001,  0x0000003C
HKR, ,                                  halNlo,                         0x00010001,  0x00000001
HKR, ,                                  enableReportNdisHWWowCap,       0x00010001,  0x00000001
HKR, ,                                  WowEnablePME,                   0x00010001,  0x00000000
HKR, ,                                  wowEnable,                      0x00002,     "1"

[S5wow.reg]
HKR, ,                                  wsis5,                          0x00002,  "1"
HKR, ,                                  wowEnable,                      0x00002,  "1"

[RestoreSettingCount.reg]
HKR, ,                                  halRestoreSettingCount,         0x00002,  "150"

[triggerlevelkiteonly.reg]
HKR, ,                                  txTrigLevelMax ,                0x00002,  "32"
HKR, ,                                  fakeAIFSN4WFA ,                 0x00002,  "1"

[c3war.reg]
HKR, ,                                  c3WarTimerPeriod,               0x00002,  "130"

[indicaterxlinkspeed.reg]
HKR, ,                                  indicateRxLinkSpeed ,           0x00002,  "1"

[fullhwresethb93.reg]
HKR, ,                                  halFullResetWarEnable ,         0x00002,  "0"

[sharegpio.reg]
HKR, ,                                  sharedGpioFunc0 ,               0x00002,  "1"

[rxLatencyWar.reg]
HKR, ,                                  rxLatencyWar ,                  0x00002,  "1"

[power.reg]
HKR, ,                                  pcieAspm,                       0x00002,  "2"
HKR, ,                                  halpciePowerSaveEnable,         0x00002,  "1"
HKR, ,                                  overrideACstatus,               0x00002,  "1"
HKR, ,                                  scanTimePreSleep,               0x00002,  "5"

[ledcontrol.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "3"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"

[ledcontrol2.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"

[ledcontrol3.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[ledcontrol7.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "4"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"

[kitec3.reg]
HKR, ,                                  c3WarTimerPeriod,               0x00002,  "130"
HKR, ,                                  txTrigLevelMax ,                0x00002,  "32"

[regdmn.reg]
HKR, ,                                  regdmn,                         0x00010001,  0x65

[djanusda.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  netband,                        0x00002,  "2060"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "0"

[djanusda2.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  netband,                        0x00002,  "2060"
HKR, ,                                  btCoexRSSIModeProfile,          0x00002,  "17115137"
HKR, ,                                  btCoexDisablePTA,               0x00002,  "2621441"
HKR, ,                                  btWlanIsolation,                0x00002,  "25"
HKR, ,                                  btCoexAntDivEnable,             0x00002,  "0"

[fastclockdisable.reg]
HKR, ,                                  fastClockEnable,                0x00002,  "0"

[paprdenable.reg]
HKR, ,                                  paprdEnable,                    0x00002,  "1"

[MSI.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 4

[9485LnaDivUseBtAntEnable.reg]
HKR, ,                                  lnaDivUseBtAntEnable,           0x00002,  "1"

[antCtrlComm2gSwitchEnable.reg]
HKR, ,                                  antCtrlComm2gSwitchEnable,      0x00010001,  0x000BBB88

[CUS198_xLnaGpioCfg.reg]
HKR, ,                                  extLnaCtlGpio,                  0x00010001,  0x00000200
HKR, ,                                  extAttenMarginCfg,              0x00002,  "1"

[rateCtrlTxFastDrop.reg]
HKR, ,                                  rateCtrlTxFastDrop,             0x00002,  "1"

[led_func0_4.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "4"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"

[led_func0_10.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "10"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  gpioLedCustom,                  0x00002,  "10"
HKR, ,                                  sharedGpioFunc0 ,               0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "10"
HKR, ,                                  gpioPinFunc2,                   0x00002,  "10"

[ledcontrol4.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "8"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"

[ledcontrol6.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "10"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"

[ledcontrol7.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "6"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"

[ledcontrol8.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "4"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "0"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"

[ledcontrol8acthi.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "4"
HKR, ,                                  gpioFunc0ActHi,                 0x00002,  "1"
HKR, ,                                  sharedGpioFunc0,                0x00002,  "1"

[throughput.reg]
HKR, ,                                  ampTxopLimit,                   0x00002,  "16"
HKR, ,                                  ampIgnoreNonERP,                0x00002,  "1"

[HPheliusda.reg]
HKR, ,                                  btCoexEnable,                   0x00002,  "4"
HKR, ,                                  btCoexAgent,                    0x00002,  "1"
HKR, ,                                  btModule,                       0x00002,  "2"
HKR, ,                                  txCoalescingEnable,             0x00002,  "1"

[AdjustRSSI.reg]
HKR, ,                                  AdjustRSSI,                     0x00002,  "1"

[halShortRetry.reg]
HKR, ,                                  halShortRetry,                  0x00002,  "11"

[IdleConfiguration.reg]
HKR, ,                                  IdleConfiguration,              0x00002,  "0"

[delayNWSleep.reg]
HKR, ,                                  delayNWSleep,                   0x00002,  "1"

[ConnectionFailure.reg]
HKR, ,                                  delayNWSleep,                   0x00002,  "1"
HKR, ,                                  swBeaconProcess,                0x00002,  "1"

[ocsEnable.reg]
HKR, ,                                  ocsEnable,                      0x00002,  "1"

[cemspecled_func0_4.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "4"
HKR, ,                                  gpioLedCustom,                  0x00002,  "3"

[TxPowerSelect.reg]
HKR, Ndi\params\overRideTxPower,        ParamDesc,                      0,  %TxPower%
HKR, Ndi\params\overRideTxPower,        Base,                           0,  "10"
HKR, Ndi\params\overRideTxPower,        default,                        0,  "0"
HKR, Ndi\params\overRideTxPower,        type,                           0,  "enum"
HKR, Ndi\params\overRideTxPower\enum,   "10",                           0,  %TxPowerLowest%
HKR, Ndi\params\overRideTxPower\enum,   "15",                           0,  %TxPowerMediumLow%
HKR, Ndi\params\overRideTxPower\enum,   "20",                           0,  %TxPowerMedium%
HKR, Ndi\params\overRideTxPower\enum,   "25",                           0,  %TxPowerMediumHigh%
HKR, Ndi\params\overRideTxPower\enum,   "0",                            0,  %TxPowerHighest%

[SleepTimePwrSaveMax1000.reg]
HKR, ,                                  SleepTimePwrSaveMax,            0x00002,  "1000"

[SleepTimePwrSaveMax2000.reg]
HKR, ,                                  SleepTimePwrSaveMax,            0x00002,  "2000"

[FilterOutCCK.reg]
HKR, ,                                  FilterOutCCKRateEnable,         0x00002,  "1"

[AphroditeMitiShift.reg]
HKR, ,                                  halMitiShiftValue,             0x10001, 0x00050003

[ledcontrol9.reg]
HKR, ,                                  gpioPinFunc0,                   0x00002,  "1"
HKR, ,                                  gpioPinFunc1,                   0x00002,  "1"
HKR, ,                                  gpioLedCustom,                  0x00002,  "4"

[customer_power.reg]
HKR, ,                                  SleepTimePwrSave,               0x00002,  "1000"
HKR, ,                                  SleepTimePerf,                  0x00002,  "1000"
HKR, ,                                  AwakeTimePwrSaveMax,            0x00002,  "150"
HKR, ,                                  AwakeTimePwrSave,               0x00002,  "150"
HKR, ,                                  periodicScanEnable,             0x00002,  "0"
HKR, ,                                  swBeaconProcess,                0x00002,  "0"


;;End of Customized Section
[miracast_off.reg]
HKR, ,                                                                  *MiracastSupported,                             0x10001,        0x0

[atheros.Service]
DisplayName     = %ATHR.Service.DispName%
ServiceType     = 1         ;SERVICE_KERNEL_DRIVER
StartType       = 3         ;SERVICE_DEMAND_START
ErrorControl    = 1         ;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\athwb.sys
LoadOrderGroup  = NDIS

[atheros.EventLog]
AddReg = atheros.AddEventLog.reg

[atheros.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


[atheros.CopyFiles]
athwb.sys,,,2

[SourceDisksNames]
1 = %DiskDescription%,athwb.sys,,

[SourceDisksFiles]
athwb.sys = 1,,

[DestinationDirs]
atheros.CopyFiles            = 12
DefaultDestDir               = 11

[Strings]
Msft                         = "Microsoft"
Atheros                      = "Qualcomm Atheros Communications Inc."
Gigabyte                     = "Gigabyte Technology Corp."
ATHR.Service.DispName        = "Qualcomm Atheros Extensible Wireless LAN device driver"
DiskDescription              = "Qualcomm Atheros Sample Driver Disk 1"
TransmitBuffers              = "Transmit Buffers"
ReceiveBuffers               = "Receive Buffers"
NetworkAddress               = "Network Address"
scanTimeValid                = "Scan Valid Interval"
shortPreamble                = "802.11b Preamble"
shortPreambleEnable          = "Long and Short"
shortPreambleDisable         = "Long only"
rssiThrHigh                  = "RSSI Threshold"
rssiThrHighNormal            = "Normal"
rssiThrHighMin               = "Min"
;radioEnable                 = "Radio On/Off"
;radioEnableOn               = "On"
;radioEnableOff              = "Off"
scanTime                     = "Roam Time (sec)"
roamRssiA                    = "Roam Time Threshold (db)"
WirelessMode                 = "Wireless Mode Selection"
WirelessMode11bgOnly         = "802.11b/g"
WirelessModeAuto             = "Auto"
adhocchannel                 = "Adhoc channel Selection"
bkScanEnable                 = "BackgroundScan On/Off"
bkScanEnableOn               = "On"
bkScanEnableOff              = "Off"
radioEnable                  = "Radio On/Off"
radioEnableOn                = "On"
radioEnableOff               = "Off"
bt30                         = "802.11 Bluetooth High Speed"
bt30enable                   = "Enable"
bt30disable                  = "Disable"
roamRssi11A                  = "roamRssiA"
roamRssi11B                  = "roamRssiB"
roamRssi11BOnly              = "roamRssiBOnly"
roamRateA                    = "roamRateA"
roamRateA6M                  = " 6Mbps"
roamRateA9M                  = " 9Mbps"
roamRateA12M                 = "12Mbps"
roamRateA18M                 = "18Mbps"
roamRateA24M                 = "24Mbps"
roamRateA36M                 = "36Mbps"
roamRateA48M                 = "48Mbps"
roamRateA54M                 = "54Mbps"
roamRateBOnly                = "roamRateBOnly"
roamRateBOnly1M              = " 1Mbps"
roamRateBOnly2M              = " 2Mbps"
roamRateBOnly5M              = " 5Mbps"
roamRateBOnly11M             = "11Mbps"
roamRateB                    = "roamRateB"
roamRateB1M                  = " 1Mbps"
roamRateB2M                  = " 2Mbps"
roamRateB5M                  = " 5Mbps"
roamRateB6M                  = " 6Mbps"
roamRateB9M                  = " 9Mbps"
roamRateB11M                 = "11Mbps"
pcieAspm                     = "pcieAspm"
pcieAspmOff                  = "L0s Off, L1 Off"
pcieAspmL0sOn                = "L0s On,  L1 Off"
pcieAspmL1On                 = "L0s Off, L1 On"
pcieAspmL0sandL1On           = "L0s On,  L1 On"
wModeSelect                  = "Wireless Mode"
wModeSelect11bonly           = "11b only"
wModeSelect11b               = "11b"
wModeSelect11g               = "11g"
wModeSelect11n               = "11n"
wModeSelect11nbg             = "11n(2.4GHz) and g and b"
wModeSelect11na              = "11n(5GHz) and a"
wModeSelect11abgn            = "11abgn"
wModeLegacy11a               = "11a only"
wModeLegacy11bonly           = "11b only"
wModeLegacy11bg              = "11g and 11b"
wModeLegacy11abg             = "11abg"
antennaSwitch                = "AntennaSwitch"
antennaSwitchAuto            = "Auto"
antennaSwitchA               = "Antenna A"
antennaSwitchB               = "Antenna B"
Auto                         = "Auto"
5GOnly                       = "5Ghz Only"
2GOnly                       = "2Ghz Only"
11AOnly                      = "802.11a (5GHz)"
11ANOnly                     = "802.11a/n (5GHz)"
11BGOnly                         = "802.11b/g (2.4GHz)"
11BGNOnly                        = "802.11b/g/n (2.4GHz)"
11ABGN                       = "802.11a/b/g/n (2.4GHz/5GHz)"
11DModeSwitch                = "11d Mode Switch"
Enable                       = "Enable"
Disable                      = "Disable"
WepTkip11n                   = "WepTKIP 11n"
PowerSaveMode                = "Power Save Mode"
Off                          = "Off"
Maximum                      = "Maximum"
Normal                       = "Normal"
802_11d                      = "802.11d"
smpsDynamic                  = "Dynamic MIMO Power Save"
AdHoc11n                     = "AdHoc 11n"
AdhocMode                    = "AdHoc Mode"
roamPolicy                   = "Roaming Policy"
roamPolicyVeryHigh           = "Very High"
roamPolicyHigh               = "High"
roamPolicyNormal             = "Normal"
roamPolicyLow                = "Low"
roamPolicyVeryLow            = "Very Low"
roamPolicyVeryHigh2          = "5.Very High"
roamPolicyHigh2              = "4.High"
roamPolicyNormal2            = "3.Normal"
roamPolicyLow2               = "2.Low"
roamPolicyVeryLow2           = "1.Very Low"
GreenTx                      = "Green Tx"
GreenTxEnableOn              = "On"
GreenTxEnableOff             = "Off"
TxPower                      = "Transmit Power"
TxPowerLowest                = "1.Lowest"
TxPowerMediumLow             = "2.Medium-Low"
TxPowerMedium                = "3.Medium"
TxPowerMediumHigh            = "4.Medium-High"
TxPowerHighest               = "5.Highest"
ATHR.DeviceDesc.0013         = "Qualcomm Atheros Wireless Network Adapter"
ATHR.DeviceDesc.001A         = "Qualcomm Atheros AR5005G Wireless Network Adapter"
ATHR.DeviceDesc.001B         = "Qualcomm Atheros AR5006X Wireless Network Adapter"
ATHR.DeviceDesc.1030         = "Qualcomm Atheros AR5002G Wireless Network Adapter"
ATHR.DeviceDesc.2030         = "Qualcomm Atheros AR5002G Wireless Network Adapter"
ATHR.DeviceDesc.1031         = "Qualcomm Atheros AR5002X Wireless Network Adapter"
ATHR.DeviceDesc.2031         = "Qualcomm Atheros AR5002X Wireless Network Adapter"
ATHR.DeviceDesc.1041         = "Qualcomm Atheros AR5004G Wireless Network Adapter"
ATHR.DeviceDesc.2041         = "Qualcomm Atheros AR5004G Wireless Network Adapter"
ATHR.DeviceDesc.1042         = "Qualcomm Atheros AR5004X Wireless Network Adapter"
ATHR.DeviceDesc.2042         = "Qualcomm Atheros AR5004X Wireless Network Adapter"
ATHR.DeviceDesc.1051         = "Qualcomm Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.2051         = "Qualcomm Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.1053         = "Qualcomm Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.2053         = "Qualcomm Atheros AR5005GS Wireless Network Adapter"
ATHR.DeviceDesc.1061         = "Qualcomm Atheros AR5006GS Wireless Network Adapter"
ATHR.DeviceDesc.2061         = "Qualcomm Atheros AR5006GS Wireless Network Adapter"
ATHR.DeviceDesc.1062         = "Qualcomm Atheros AR5006XS Wireless Network Adapter"
ATHR.DeviceDesc.2062         = "Qualcomm Atheros AR5006XS Wireless Network Adapter"
ATHR.DeviceDesc.1065         = "Qualcomm Atheros AR5006G Wireless Network Adapter"
ATHR.DeviceDesc.2065         = "Qualcomm Atheros AR5006G Wireless Network Adapter"
ATHR.DeviceDesc.3061         = "Qualcomm Atheros AR5006EGS Wireless Network Adapter"
ATHR.DeviceDesc.3062         = "Qualcomm Atheros AR5006EXS Wireless Network Adapter"
ATHR.DeviceDesc.3063         = "Qualcomm Atheros AR5006EX Wireless Network Adapter"
ATHR.DeviceDesc.3065         = "Qualcomm Atheros AR5006EG Wireless Network Adapter"
ATHR.DeviceDesc.2055         = "Qualcomm Atheros AR5007G Wireless Network Adapter"
ATHR.DeviceDesc.3067         = "Qualcomm Atheros AR5007EG Wireless Network Adapter"
ATHR.DeviceDesc.1071         = "Qualcomm Atheros AR5008 Wireless Network Adapter"
ATHR.DeviceDesc.3072         = "Qualcomm Atheros AR5008X Wireless Network Adapter"
ATHR.DeviceDesc.3091         = "Qualcomm Atheros AR928X Wireless Network Adapter"
ATHR.DeviceDesc.2091         = "Qualcomm Atheros AR922X Wireless Network Adapter"
ATHR.DeviceDesc.30A1         = "Qualcomm Atheros AR9285 Wireless Network Adapter"
ATHR.DeviceDesc.30ABLT       = "Qualcomm Atheros AR9002WB-1NG Wireless Network Adapter"
ATHR.DeviceDesc.30AB         = "Qualcomm Atheros AR9002WB-1NG Wireless Network Adapter #1"
ATHR.DeviceDesc.30AD         = "Qualcomm Atheros AR9002WB-1NG Wireless Network Adapter #2"
ATHR.DeviceDesc.2A371A3B     = "Qualcomm Atheros AR9002WB Wireless Network Adapter"
ATHR.DeviceDesc.30AE         = "Qualcomm Atheros AR5008WB-EG Wireless Network Adapter #1"
ATHR.DeviceDesc.30AF         = "Qualcomm Atheros AR5008WB-EG Wireless Network Adapter #2"
ATHR.DeviceDesc.30A7         = "Qualcomm Atheros AR2427 Wireless Network Adapter"
ATHR.DeviceDesc.10CF         = "IEEE 802.11a/g Wireless LAN Adapter (A)"
ATHR.DeviceDesc.1737_g       = "Linksys Wireless-G Notebook Adapter"
ATHR.DeviceDesc.1737_bg      = "Linksys Wireless A+G Notebook Adapter"
ATHR.DeviceDesc.1737_abg     = "Linksys Wireless A+G PCI Adapter"
ATHR.DeviceDesc.0044         = "Linksys Dual-Band Wireless A+G PCI Adapter"
ATHR.DeviceDesc.1013         = "11b/g Wireless LAN Mini PCI Adapter"
ATHR.DeviceDesc.2013         = "11a/b/g Wireless LAN Mini PCI Adapter II" 
ATHR.DeviceDesc.3013         = "11b/g Wireless LAN Mini PCI Express Adapter"
ATHR.DeviceDesc.4013         = "11a/b/g Wireless LAN Mini PCI Express Adapter"
ATHR.DeviceDesc.5013         = "11b/g Wireless LAN Mini PCI Express Adapter II"
ATHR.DeviceDesc.6013         = "11b/g Wireless LAN Mini PCI Express Adapter III"
ATHR.DeviceDesc.0032168c     = "11b/g/n Wireless LAN Mini-PCI Express Adapter"
ATHR.DeviceDesc.0033168c     = "11a/b/g/n Wireless LAN Mini-PCI Express Adapter"
ATHR.DeviceDesc.90001385     = "NETGEAR WN711 RangeMax Wireless-N Expresscard Adapter"
ATHR.DeviceDesc.4B001385     = "NETGEAR 108 Mbps Wireless PC Card WG511T"
ATHR.DeviceDesc.5D001385     = "NETGEAR RangeMax(TM) Wireless PC Card WPN511"
ATHR.DeviceDesc.4D001385     = "NETGEAR 108 Mbps Wireless PCI Adapter WG311T"
ATHR.DeviceDesc.4F001385     = "NETGEAR Double 108 Mbps Wireless PC Card WG511U"
ATHR.DeviceDesc.04061468     = "LAN-Express AS IEEE 802.11g miniPCI Adapter"
ATHR.DeviceDesc.04071468     = "LAN-Express AS IEEE 802.11a/g miniPCI Adapter"
ATHR.DeviceDesc.04231468     = "LAN-Express AS IEEE 802.11g PCI-E Adapter"
ATHR.DeviceDesc.F6D3000      = "Belkin Wireless A/G Desktop Network Card"
ATHR.DeviceDesc.80111799     = "Belkin N1 Wireless Notebook Card"
ATHR.DeviceDesc.G650         = "D-Link AirPlus DWL-G650 Wireless Cardbus Adapter(rev.C)"
ATHR.DeviceDesc.G520X        = "D-Link AirPlus Xtreme G DWL-G520 Adapter"
ATHR.DeviceDesc.G520         = "D-Link AirPlus DWL-G520 Wireless PCI Adapter(rev.B)"
ATHR.DeviceDesc.AG520        = "D-Link AirXpert DWL-AG520 Wireless PCI Adapter"
ATHR.DeviceDesc.AG530        = "D-Link AirPremier DWL-AG530 Wireless PCI Adapter"
ATHR.DeviceDesc.G630         = "D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter(rev.D)"
ATHR.DeviceDesc.G510         = "D-Link AirPlus G DWL-G510 Wireless PCI Adapter(rev.B)"
ATHR.DeviceDesc.AG650        = "D-Link AirXpert DWL-AG650 Wireless Cardbus Adapter"
ATHR.DeviceDesc.AG660        = "D-Link AirPremier DWL-AG660 Wireless Cardbus Adapter"
ATHR.DeviceDesc.G680         = "D-Link AirPremier DWL-G680 Wireless Cardbus Adapter"
ATHR.DeviceDesc.G550         = "D-Link AirPremier DWL-G550 Wireless PCI Adapter"
ATHR.DeviceDesc.AG660B       = "D-Link AirPremier AG DWL-AG660 Wireless Cardbus Adapter"
ATHR.DeviceDesc.AG530B       = "D-Link AirPremier AG DWL-AG530 Wireless PCI Adapter"
ATHR.DeviceDesc.G650P        = "D-Link AirPlus G DWL-G650+A Wireless Cardbus Adapter"
ATHR.DeviceDesc.G520P        = "D-Link AirPlus G DWL-G520+A Wireless PCI Adapter"
ATHR.DeviceDesc.WDA1320      = "D-Link WDA-1320 Desktop Adapter"
ATHR.DeviceDesc.WDA2320      = "D-Link WDA-2320 Desktop Adapter"
ATHR.DeviceDesc.DWA520       = "D-Link Wireless 108G DWA-520 Desktop Adapter"
ATHR.DeviceDesc.DWA620       = "D-Link Wireless 108G DWA-620 Notebook Adapter"
ATHR.DeviceDesc.CWNA2330     = "D-Link WNA-2330 Notebook Adapter"
ATHR.DeviceDesc.CWNA1330     = "D-Link WNA-1330 Notebook Adapter"
ATHR.DeviceDesc.CG650        = "D-Link AirPlus Xtreme G DWL-G650 Adapter"
ATHR.DeviceDesc.CG630        = "D-Link AirPlus G DWL-G630 Wireless Cardbus Adapter"
ATHR.DeviceDesc.DWA642       = "D-Link DWA-642 RangeBooster N Notebook Adapter"
ATHR.DeviceDesc.DWA645       = "D-Link DWA-645 RangeBooster N650 Notebook Adapter"
ATHR.DeviceDesc.DWA542       = "D-Link DWA-542 RangeBooster N Desktop Adapter"
ATHR.DeviceDesc.DWA547       = "D-Link DWA-547 RangeBooster N650 Desktop Adapter"
ATHR.DeviceDesc.DWA652       = "D-Link DWA-652 XtremeN Notebook Adapter"
ATHR.DeviceDesc.DWA552       = "D-Link DWA-552 XtremeN Desktop Adapter"
ATHR.DeviceDesc.DWA643       = "D-Link DWA-643 Xtreme N ExpressCard Notebook Adapter"
ATHR.DeviceDesc.DWA556       = "D-Link DWA-556 Xtreme N PCIe Desktop Adapter"
ATHR.DeviceDesc.3070         = "Gigaset PC Card 108"
ATHR.DeviceDesc.3071         = "Speedport Gigaset 54 Mbit"
ATHR.DeviceDesc.800118CB     = "Gigaset PC Card 300"
ATIWC.DeviceDesc.ATICB       = "Allied Telesyn AT-WCC201g Wireless Card Bus Adapter"
ATIWC.DeviceDesc.ATIPC       = "Allied Telesyn AT-WCP201g Wireless PCI Adapter"
ATHR.DeviceDesc.2A5F103C     = "Foxconn 802.11 a/b/g/n Wireless System Adaptor"
ATHR.DeviceDesc.500011AD     = "HP 802.11a/b/g Wireless Network Adapter"
ATHR.DeviceDesc.500111AD     = "HP 802.11b/g Wireless Network Adapter"
ATHR.DeviceDesc.1000168c     = "Qualcomm Atheros 802.11 a/b/g/n Dualband Wireless Network Module"
GIGA.DeviceDesc.E914         = "Gigabyte GN-WI03N (mini) PCI WLAN Card"
GIGA.DeviceDesc.E915         = "Gigabyte GN-WP02N PCI Express WLAN Card"
GIGA.DeviceDesc.E916         = "Gigabyte GN-WI06N (mini) PCI Express WLAN Card"
GIGA.DeviceDesc.E815         = "Gigabyte GN-WM02N Express WLAN Card"
GIGA.DeviceDesc.E801         = "Gigabyte GN-WLMA102 Cardbus WLAN Card"
GIGA.DeviceDesc.E811         = "Gigabyte GN-WMAG Cardbus WLAN Card"
GIGA.DeviceDesc.E814         = "Gigabyte GN-WM01GT Cardbus WLAN Card"
GIGA.DeviceDesc.0013         = "Gigabyte GN-WIAH (mini) PCI WLAN Card"
GIGA.DeviceDesc.E901         = "Gigabyte GN-WI01HT (mini) PCI WLAN Card"
GIGA.DeviceDesc.E911         = "Gigabyte GN-WIAG/GN-WPEAG (mini) PCI WLAN Card"
GIGA.DeviceDesc.E912         = "Gigabyte GN-WP01GT (mini) PCI WLAN Card"
GIGA.DeviceDesc.E913         = "Gigabyte GN-WI01GT (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E917         = "Gigabyte GN-WI07HT (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E918         = "Gigabyte GN-WS50G (mini) PCI-E WLAN Card"
GIGA.DeviceDesc.E9191458     = "Gigabyte GN-WS53HN Wireless LAN Mini PCI Express Adapter"
ATHR.DeviceDesc.7141144F     = "Qualcomm Atheros AR9281 Wireless Network Adapter"
ATHR.DeviceDesc.7136144F     = "Qualcomm Atheros AR9280 Wireless Network Adapter"
ATHR.DeviceDesc.E006105B     = "Qualcomm Atheros AR5B91 Wireless Network Adapter"
ATHR.DeviceDesc.655211AD     = "Qualcomm Atheros AR5B92 Wireless Network Adapter"
ATHR.DeviceDesc.CM9          = "WNC CM9 Wireless LAN mini-PCI Network Adapter"
ATHR.DeviceDesc.1ACE         = "TP-LINK Wireless N Adapter"
ATHR.DeviceDesc.00341B0A     = "Qualcomm Atheros AR9281 802.11b/g/n WLAN HMC Network"
ATHR.DeviceDesc.2063         = "Qualcomm Atheros AR5006 802.11a/b/g WiFi Adapter"
ATHR.DeviceDesc.3096         = "Qualcomm Atheros AR5009 802.11a/g/n WiFi Adapter"
ATHR.DeviceDesc.5E001385     = "NETGEAR WPN311 RangeMax(TM) Wireless PCI Adapter"
ATHR.DeviceDesc.0036         = "11b/g/n Wireless LAN Mini-PCI Express Adapter II"
ATHR.DeviceDesc.0037         = "11b/g/n Wireless LAN Mini-PCI Express Adapter III"
ATHR.DeviceDesc.309917AA     = "11a/b/g/n Wireless LAN Adapter"
ATHR.DeviceDesc.7163144F     = "Qualcomm Atheros AR9283 Wireless Network Adapter"
ATHR.DeviceDesc.E01F105B     = "Qualcomm Atheros AR5B93 Wireless Network Adapter"
ATHR.DeviceDesc.663111AD     = "Qualcomm Atheros AR5B95 Wireless Network Adapter"
ATHR.DeviceDesc.660311AD     = "Qualcomm Atheros AR5B97 Wireless Network Adapter"
ATHR.DeviceDesc.661711AD     = "Qualcomm Atheros AR5B125 Wireless Network Adapter"
ATHR.DeviceDesc.E04A105B     = "Qualcomm Atheros AR5B116 Wireless Network Adapter"
ATHR.DeviceDesc.661811AD     = "Qualcomm Atheros AR5BWB225 Wireless Network Adapter"
ATHR.DeviceDesc.E051105B     = "Qualcomm Atheros AR5BMD225 Wireless Network Adapter"
ATHR.DeviceDesc.311711AD     = "Qualcomm Atheros AR5BWB222 Wireless Network Adapter"
ATHR.DeviceDesc.E059105B     = "Qualcomm Atheros AR5BMD222 Wireless Network Adapter"
ATHR.DeviceDesc.30A4         = "Qualcomm Atheros AR9287 Wireless Network Adapter"
ATHR.DeviceDesc.2099         = "Qualcomm Atheros AR9227 Wireless Network Adapter"
ATHR.DeviceDesc.D05B10FC     = "I-O DATA WHG-AGDN/CB Wireless LAN Adapter"
ATHR.DeviceDesc.30B0         = "Qualcomm Atheros AR9002WB-2NG Wireless Network Adapter"
ATHR.DeviceDesc.ospsim       = "Qualcomm Atheros Osprey Simulation Wireless Network Adapter"
ATHR.DeviceDesc.ospemu       = "Qualcomm Atheros Osprey Emulation Wireless Network Adapter"
ATHR.DeviceDesc.osprey       = "Qualcomm Atheros Osprey Wireless Network Adapter"
ATHR.DeviceDesc.938x         = "Qualcomm Atheros AR938x Wireless Network Adapter"
ATHR.DeviceDesc.9485         = "Qualcomm Atheros AR9485 Wireless Network Adapter"
ATHR.DeviceDesc.1111         = "Qualcomm Atheros AR1111 Wireless Network Adapter"
ATHR.DeviceDesc.9580         = "Qualcomm Atheros AR9580 Wireless Network Adapter"
ATHR.DeviceDesc.3119         = "Qualcomm Atheros AR9485WB-EG Wireless Network Adapter"
ATHR.DeviceDesc.D3067        = "Qualcomm Atheros AR5007 802.11b/g WiFi Adapter"
ATHR.DeviceDesc.D30A1        = "Qualcomm Atheros AR9285 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.D30AB        = "Qualcomm Atheros AR9285 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.0300T        = "TP-LINK 300Mbps Wireless N Adapter"
ATHR.DeviceDesc.0301T        = "TP-LINK 150Mbps Wireless N Adapter"
ATHR.DeviceDesc.3B001106     = "VIA 802.11b/g/n PCIe Wireless Network Adapter"
ATHR.DeviceDesc.00231931     = "Option GTM67x PCIe WiFi Adapter"
ATHR.DeviceDesc.11951A3B     = "Qualcomm Atheros AR1111 Wireless Network Adapter"
ATHR.DeviceDesc.21001A3B     = "Qualcomm Atheros AR1111 WB-EG Wireless Network Adapter"
ATHR.DeviceDesc.H3067        = "Qualcomm Atheros AR5007 802.11b/g WiFi Adapter"
ATHR.DeviceDesc.H2063        = "Qualcomm Atheros AR5006 802.11a/b/g WiFi Adapter"
ATHR.DeviceDesc.H3096        = "Qualcomm Atheros AR5009 802.11a/g/n WiFi Adapter"
ATHR.DeviceDesc.H30A1        = "Qualcomm Atheros AR9285 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.H30AB        = "Qualcomm Atheros AR9285 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.H30A4        = "Qualcomm Atheros AR9287 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.H3197        = "Qualcomm Atheros AR9287 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.H3116        = "Qualcomm Atheros AR9382 802.11a/g/n WiFi Adapter"
ATHR.DeviceDesc.H3112        = "Qualcomm Atheros AR9380 802.11a/g/n WiFi Adapter"
ATHR.DeviceDesc.H3119        = "Qualcomm Atheros AR9485 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.H3118        = "Qualcomm Atheros AR9485 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.946x         = "Qualcomm Atheros AR946x Wireless Network Adapter"
ATHR.DeviceDesc.H3335        = "Qualcomm Atheros AR9462 802.11a/b/g/n WiFi Adapter"
ATHR.DeviceDesc.956x         = "Qualcomm Atheros AR956x Wireless Network Adapter"
ATHR.DeviceDesc.H9565        = "Qualcomm Atheros QCA9565 802.11b/g/n WiFi Adapter"
ATHR.DeviceDesc.E031105B     = "Qualcomm Atheros AR5B195 Wireless Network Adapter"
ATHR.DeviceDesc.E068105B     = "Qualcomm Atheros AR956x Wireless Network Adapter"
ATHR.DeviceDesc.302617AA     = "Qualcomm Atheros AR956x Wireless Network Adapter"
ATHR.DeviceDesc.DWA566       = "D-Link DWA-566 Wireless N 300 Dual Band PCIe Desktop Adapter"
ATHR.DeviceDesc.TEW726       = "TRENDnet N600 Wireless Dual Band PCIe Adapter"
ATHR.DeviceDesc.k1102        = "Killer Wireless-N 1102 Network Adapter"
ATHR.DeviceDesc.k1103        = "Killer Wireless-N 1103 Network Adapter"
ATHR.DeviceDesc.k1202        = "Killer Wireless-N 1202 Network Adapter"


;/* Enable these if VLAN or 802.1p is to be enabled */
;PriorityVLAN                = "Priority & VLAN"
;PriorityVLANDisabled        = "Priority & VLAN Disabled"
;PriorityEnabled             = "Priority Enabled"
;VLANEnabled                 = "VLAN Enabled"
;PriorityVLANEnabled         = "Priority & VLAN Enabled"
