;/****************************************************************************
; * Copyright 2011-2014 Qualcomm Atheros Inc., all rights reserved.          *
; *                                                                          *
; * Copyright (c) 2011-2014 Qualcomm Atheros, Inc.                           *
; * All Rights Reserved.                                                     *
; * Qualcomm Atheros Confidential and Proprietary.                           *
; *                                                                          *
; * INF file for Qualcomm Atheros reference designs                          *
; ****************************************************************************/

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHEROS%
CatalogFile = Qcamainext10.cat
DriverVer   = 06/21/2017,12.0.0.318

[Manufacturer]
%ATHEROS%     = Atheros, NTX86.10.0

[ControlFlags]
ExcludeFromSelect = *

;
; OS 6.3 Manufacturer section
;
[Atheros.NTX86.10.0]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
;;Rome 2.2
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_FTM.ndi,                PCI\VEN_168C&DEV_003E&SUBSYS_00000000
%ATHR.DeviceDesc.2582%     = ATHR_DEV_OS63_988x_Killer_NFA344.ndi,      PCI\VEN_168C&DEV_003E&SUBSYS_15251A56&REV_20 ;for Killer QCA2582
%ATHR.DeviceDesc.2582%     = ATHR_DEV_OS63_988x_LE_Killer_NFA344.ndi,   PCI\VEN_168C&DEV_003E&SUBSYS_152517AA&REV_20 ;for Lenovo Killer QCA2582
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_NFA344.ndi,             PCI\VEN_168C&DEV_003E&SUBSYS_3344168C&REV_20 ;for QCA NFA344i
%ATHR.DeviceDesc.6320_2%   = ATHR_DEV_OS63_988x_NFA345.ndi,             PCI\VEN_168C&DEV_0041&SUBSYS_3345168C&REV_20 ;for QCA NFA345i
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_NFA324.ndi,             PCI\VEN_168C&DEV_003E&SUBSYS_3346168C        ;for QCA NFA324
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_NFA354.ndi,             PCI\VEN_168C&DEV_003E&SUBSYS_3348168C&REV_20 ;for QCA NFA354 
%ATHR.DeviceDesc.6320_2%   = ATHR_DEV_OS63_988x_NFA355.ndi,             PCI\VEN_168C&DEV_0041&SUBSYS_3349168C&REV_20 ;for QCA NFA355i
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_FUJI_NFA344.ndi,        PCI\VEN_168C&DEV_003E&SUBSYS_190D10CF&REV_20 ;for Fujitsu NFA344
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_LE_NFA344.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_304417AA&REV_20 ;for Lenovo NFA344-WW 
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_LE_NFA344.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_314417AA&REV_20 ;for Lenovo NFA344-US 
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_LE_NFA344.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_324417AA&REV_20 ;for Lenovo NFA344-Indonesia 
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_LE_NFA344.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_334417AA&REV_20 ;for Lenovo NFA344-Russia/Ukraine/Egypt
%ATHR.DeviceDesc.6320_2%   = ATHR_DEV_OS63_988x_LE_NFA345.ndi,          PCI\VEN_168C&DEV_0041&SUBSYS_304517AA&REV_20 ;for Lenovo NFA345-WW 
%ATHR.DeviceDesc.6320_2%   = ATHR_DEV_OS63_988x_LE_NFA345.ndi,          PCI\VEN_168C&DEV_0041&SUBSYS_314517AA&REV_20 ;for Lenovo NFA345-US 
%ATHR.DeviceDesc.6320_2%   = ATHR_DEV_OS63_988x_LE_NFA345.ndi,          PCI\VEN_168C&DEV_0041&SUBSYS_324517AA&REV_20 ;for Lenovo NFA345-Indonesia
%ATHR.DeviceDesc.6320_2%   = ATHR_DEV_OS63_988x_LE_NFA345_IPG.ndi,      PCI\VEN_168C&DEV_0041&SUBSYS_354517AA&REV_20 ;for Lenovo NFA345-WW 
%ATHR.DeviceDesc.6320_2%   = ATHR_DEV_OS63_988x_LE_NFA345_IPG.ndi,      PCI\VEN_168C&DEV_0041&SUBSYS_364517AA&REV_20 ;for Lenovo NFA345-US 
%ATHR.DeviceDesc.6320_2%   = ATHR_DEV_OS63_988x_LE_NFA345_IPG.ndi,      PCI\VEN_168C&DEV_0041&SUBSYS_374517AA&REV_20 ;for Lenovo NFA345-Indonesia
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_AC_NFA344.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_080411AD&REV_20 ;for Acer NFA344
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_AC_NFA344.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_E08E105B&REV_20 ;for Acer NFA344
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_AC_NFA344.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_180411AD&REV_20 ;for Acer NFA344 US
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_NFA344.ndi,             PCI\VEN_168C&DEV_003E&SUBSYS_082411AD&REV_20 ;for generic NFA344
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_AS_NFA344.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_081411AD&REV_20 ;for Asus NFA344
%ATHR.DeviceDesc.6320_2%   = ATHR_DEV_OS63_988x_AS_NFA345.ndi,          PCI\VEN_168C&DEV_0041&SUBSYS_080511AD&REV_20 ;for Asus NFA345 
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_ss_NFA354.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_4125144D&REV_20 ;for Samsung NFA354
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_ss_NFA354.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_4126144D&REV_20 ;for Samsung NFA354
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_ss_NFA354.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_4127144D&REV_20 ;for Samsung NFA354
%ATHR.DeviceDesc.6320%     = ATHR_DEV_OS63_988x_ss_NFA354.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_4128144D&REV_20 ;for Samsung NFA354
%ATHR.DeviceDesc.6320_2%   = ATHR_DEV_OS63_988x_ss_NFA355.ndi,          PCI\VEN_168C&DEV_0041&SUBSYS_4121144D&REV_20 ;for Samsung NFA355
%ATHR.DeviceDesc.6320_2%   = ATHR_DEV_OS63_988x_ss_NFA355.ndi,          PCI\VEN_168C&DEV_0041&SUBSYS_4122144D&REV_20 ;for Samsung NFA355
%ATHR.DeviceDesc.6320_2%   = ATHR_DEV_OS63_988x_ss_NFA355.ndi,          PCI\VEN_168C&DEV_0041&SUBSYS_4123144D&REV_20 ;for Samsung NFA355
%ATHR.DeviceDesc.6320_2%   = ATHR_DEV_OS63_988x_ss_NFA355.ndi,          PCI\VEN_168C&DEV_0041&SUBSYS_4124144D&REV_20 ;for Samsung NFA355

;;Tufello 1.0
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_FTM.ndi,                PCI\VEN_168C&DEV_0042&SUBSYS_00000000
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_NFA425_TF.ndi,          PCI\VEN_168C&DEV_0042&SUBSYS_3365168C&REV_30 ;for QCA NFA425
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_NFA435_TF.ndi,          PCI\VEN_168C&DEV_0042&SUBSYS_334F168C&REV_30 ;for QCA NFA435
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_SS_NFA455_TF.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_412B144D&REV_30 ;for Samsung
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_SS_NFA435_TF.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_412C144D&REV_30 ;for Samsung
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_SS_NFA435_TF.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_412D144D&REV_30 ;for Samsung
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_SS_NFA435_TF.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_412E144D&REV_30 ;for Samsung
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_SS_NFA425_TF.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_4133144D&REV_30 ;for Samsung
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_2_TF.ndi,     PCI\VEN_168C&DEV_0042&SUBSYS_22311A3B&REV_30 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_SGL_CS_TF.ndi,PCI\VEN_168C&DEV_0042&SUBSYS_2B311A3B&REV_30 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_2_TF.ndi,     PCI\VEN_168C&DEV_0042&SUBSYS_2C311A3B&REV_30 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_2_TF.ndi,     PCI\VEN_168C&DEV_0042&SUBSYS_2D311A3B&REV_30 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_2_TF.ndi,     PCI\VEN_168C&DEV_0042&SUBSYS_081611AD&REV_30 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_SGL_TF.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_2F311A3B&REV_30 ;for Asus Indonesia
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_TF.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_7145144F&REV_30 ;for Asus Askey
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AC_NFA435_TF.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_E09A105B&REV_30 ;for Acer
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AC_NFA435_TF.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_080611AD&REV_30 ;for Acer
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AC_NFA435_TF.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_180611AD&REV_30 ;for Acer
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_LE_NFA435_TF.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_403517AA&REV_30 ;for Lenovo
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_LE_NFA435_TF.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_413517AA&REV_30 ;for Lenovo
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_LE_NFA435_TF.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_423517AA&REV_30 ;for Lenovo
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_LE_NFA435_TF.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_433517AA&REV_30 ;for Lenovo
;;Tufello 1.1
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_NFA425_TF11.ndi,      PCI\VEN_168C&DEV_0042&SUBSYS_3365168C&REV_31 ;for QCA NFA425
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_NFA425_SGL_TF11.ndi,  PCI\VEN_168C&DEV_0042&SUBSYS_3369168C&REV_31 ;for QCA NFA425-5s
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_NFA435_TF11.ndi,      PCI\VEN_168C&DEV_0042&SUBSYS_334F168C&REV_31 ;for QCA NFA435
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_NFA435_SGL_TF11.ndi,  PCI\VEN_168C&DEV_0042&SUBSYS_3368168C&REV_31 ;for QCA NFA435as
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_NFA435_TF11.ndi,      PCI\VEN_168C&DEV_0042&SUBSYS_09011235&REV_31 ;for Smart
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_SS_NFA455_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_412B144D&REV_31 ;for Samsung
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_SS_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_412C144D&REV_31 ;for Samsung
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_SS_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_412D144D&REV_31 ;for Samsung
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_SS_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_412E144D&REV_31 ;for Samsung
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_SS_NFA425_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_4133144D&REV_31 ;for Samsung
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_TF11.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_223A1A3B&REV_31 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_SGL_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_223B1A3B&REV_31 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_TF11.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_223C1A3B&REV_31 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_TF11.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_22311A3B&REV_31 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_SGL_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_2B311A3B&REV_31 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_TF11.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_7145144F&REV_31 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_TF11.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_2C311A3B&REV_31 ;for Asus Indonesia
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_SGL_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_2F311A3B&REV_31 ;for Asus Indonesia
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_SGL_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_7148144F&REV_31 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA425_2_TF11.ndi,     PCI\VEN_168C&DEV_0042&SUBSYS_22511A3B&REV_31 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA425_2_TF11.ndi,     PCI\VEN_168C&DEV_0042&SUBSYS_25131A3B&REV_31 ;for Asus Indonesia
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA425_TF11.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_2B511A3B&REV_31 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA425_TF11.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_2C511A3B&REV_31 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA425_TF11.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_7142144F&REV_31 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA425_TF11.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_25111A3B&REV_31 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA425_3_SGL_TF11.ndi, PCI\VEN_168C&DEV_0042&SUBSYS_2A511A3B&REV_31 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA425_2_SGL_TF11.ndi, PCI\VEN_168C&DEV_0042&SUBSYS_25141A3B&REV_31 ;for Asus Indonesia
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA425_SGL_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_25121A3B&REV_31 ;for Asus
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_ECS_NFA425_TF11.ndi,  PCI\VEN_168C&DEV_0042&SUBSYS_25151A3B&REV_31 ;for ECS
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AC_NFA425_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_050711AD&REV_31 ;for Acer
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AC_NFA425_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_25101A3B&REV_31 ;for Acer
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AC_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_E09A105B&REV_31 ;for Acer
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AC_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_080611AD&REV_31 ;for Acer
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AC_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_180611AD&REV_31 ;for Acer
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AC_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_08A611AD&REV_31 ;for Acer
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AC_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_E0A1105B&REV_31 ;for Acer
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_LE_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_403517AA&REV_31 ;for Lenovo
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_LE_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_413517AA&REV_31 ;for Lenovo
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_LE_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_423517AA&REV_31 ;for Lenovo
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_LE_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_433517AA&REV_31 ;for Lenovo
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_LE_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_090117AA&REV_31 ;for Lenovo
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_LE_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_091117AA&REV_31 ;for Lenovo Indonesia SKU
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_LE_NFA435_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_092117AA&REV_31 ;for Lenovo AGN SKU
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_LE_NFA425_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_093117AA&REV_31 ;for Lenovo
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_LE_NFA425_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_402517AA&REV_31 ;for Lenovo
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_NFA425_TF11.ndi,      PCI\VEN_168C&DEV_0042&SUBSYS_050811AD&REV_31 ;for LiteOn
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_NFA435A_TF11.ndi,     PCI\VEN_168C&DEV_0042&SUBSYS_082611AD&REV_31 ;for LiteOn
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA425_2_TF11.ndi,     PCI\VEN_168C&DEV_0042&SUBSYS_051811AD&REV_31 ;for LiteOn
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA425_3_SGL_TF11.ndi, PCI\VEN_168C&DEV_0042&SUBSYS_151811AD&REV_31 ;for LiteOn
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_TF11.ndi,       PCI\VEN_168C&DEV_0042&SUBSYS_083611AD&REV_31 ;for LiteOn
%ATHR.DeviceDesc.9377%     = ATHR_DEV_OS63_988x_AS_NFA435_SGL_TF11.ndi,   PCI\VEN_168C&DEV_0042&SUBSYS_183611AD&REV_31 ;for LiteOn

;;Rome 3.x
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA324A_1.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_334E168C&REV_30 ;for QCA NFA324A-1
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA324A_5.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_3360168C&REV_30 ;for QCA NFA324A-5
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA344A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_3361168C&REV_30 ;for QCA NFA344A
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA354A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_3362168C&REV_30 ;for QCA NFA354A
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA364A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_3363168C&REV_30 ;for QCA NFA364A
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA324A_1.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_334E168C&REV_32 ;for QCA NFA324A-1
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA324A_5.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_3360168C&REV_32 ;for QCA NFA324A-5
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA344A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_3361168C&REV_32 ;for QCA NFA344A
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA344A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_525A1A56&REV_32 ;for Killer1525A
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA354A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_3362168C&REV_32 ;for QCA NFA354A
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA364A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_3363168C&REV_32 ;for QCA NFA364A
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_QCA9008.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_3366168C&REV_32 ;for QCA QCA9008
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_USI_9008.ndi,           PCI\VEN_168C&DEV_003E&SUBSYS_900814CD&REV_32 ;for USI 9008
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_AS_9008.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_980114CD&REV_32 ;for Asus 9008
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_QCA9008.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_87511043&REV_32 ;for Asus WW SKU
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_QCA9008.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_87521043&REV_32 ;for Asus US SKU
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_AC_9008.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_980214CD&REV_32 ;for Acer 9008
%ATHR.DeviceDesc.2582_2%   = ATHR_DEV_OS63_988x_Killer_NFA344A.ndi,     PCI\VEN_168C&DEV_003E&SUBSYS_14351A56&REV_32 ;for Killer 1435
%ATHR.DeviceDesc.2582_3%   = ATHR_DEV_OS63_988x_Killer_NFA364A.ndi,     PCI\VEN_168C&DEV_003E&SUBSYS_535A1A56&REV_32 ;for Killer
%ATHR.DeviceDesc.2582_3%   = ATHR_DEV_OS63_988x_RV_Killer_NFA364A_2.ndi,PCI\VEN_168C&DEV_003E&SUBSYS_15351A56&REV_32 ;for Rivet Killer
%ATHR.DeviceDesc.2582_3%   = ATHR_DEV_OS63_988x_RV_Killer_NFA364A.ndi,  PCI\VEN_168C&DEV_003E&SUBSYS_15361A56&REV_32 ;for Rivet Killer
%ATHR.DeviceDesc.2582_3%   = ATHR_DEV_OS63_988x_LE_Killer_NFA364A.ndi,  PCI\VEN_168C&DEV_003E&SUBSYS_153517AA&REV_32 ;for Lenovo Killer
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_FJ_1_NFA344A.ndi,       PCI\VEN_168C&DEV_003E&SUBSYS_192A10CF&REV_32 ;for Fujitsu
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_FJ_NFA344A.ndi,         PCI\VEN_168C&DEV_003E&SUBSYS_192B10CF&REV_32 ;for Fujitsu
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_SS_NFA324A_5.ndi,       PCI\VEN_168C&DEV_003E&SUBSYS_412F144D&REV_32 ;for Samsung
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_SS_NFA324A_5.ndi,       PCI\VEN_168C&DEV_003E&SUBSYS_4130144D&REV_32 ;for Samsung
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_SS_NFA324A_5.ndi,       PCI\VEN_168C&DEV_003E&SUBSYS_4131144D&REV_32 ;for Samsung
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_SS_NFA324A_5.ndi,       PCI\VEN_168C&DEV_003E&SUBSYS_4132144D&REV_32 ;for Samsung
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_AC_NFA324A_5.ndi,       PCI\VEN_168C&DEV_003E&SUBSYS_E0A0105B&REV_32 ;for Acer
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_AC_NFA324A_5.ndi,       PCI\VEN_168C&DEV_003E&SUBSYS_050311AD&REV_32 ;for Acer
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_SS_COB.ndi,             PCI\VEN_168C&DEV_003E&SUBSYS_C135144D&REV_32 ;for Samsung ; Win10 only
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_SS_COB_1.ndi,           PCI\VEN_168C&DEV_003E&SUBSYS_C14F144D&REV_32 ;for Samsung ; Win10 only
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_SS_COB_2.ndi,           PCI\VEN_168C&DEV_003E&SUBSYS_C150144D&REV_32 ;for Samsung ; Win10 only
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_AC_NFA344A.ndi,         PCI\VEN_168C&DEV_003E&SUBSYS_080711AD&REV_32 ;for Acer WW SKU
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_AC_NFA344A.ndi,         PCI\VEN_168C&DEV_003E&SUBSYS_180711AD&REV_32 ;for Acer US SKU
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_AC_NFA344A.ndi,         PCI\VEN_168C&DEV_003E&SUBSYS_E09D105B&REV_32 ;for Acer WW,US,Indonesia
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_VA_NFA344A.ndi,         PCI\VEN_168C&DEV_003E&SUBSYS_E0A2105B&REV_32 ;for VAIO
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_AS_NFA364A_3.ndi,       PCI\VEN_168C&DEV_003E&SUBSYS_86CD1043&REV_32 ;for Asus
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_AS_NFA364A_3.ndi,       PCI\VEN_168C&DEV_003E&SUBSYS_86E01043&REV_32 ;for Asus
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_AS_NFA364A.ndi,         PCI\VEN_168C&DEV_003E&SUBSYS_22601A3B&REV_32 ;for Asus
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_AS_NFA364A_2.ndi,       PCI\VEN_168C&DEV_003E&SUBSYS_080811AD&REV_32 ;for Asus
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA364A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_7144144F&REV_32 ;for Asus
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA344A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_7143144F&REV_32 ;for Asus
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_AS_NFA344A.ndi,         PCI\VEN_168C&DEV_003E&SUBSYS_86F81043&REV_32 ;for Asus WW SKU
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_AS_NFA344A.ndi,         PCI\VEN_168C&DEV_003E&SUBSYS_86F91043&REV_32 ;for Asus US SKU
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_LE_NFA344A.ndi,         PCI\VEN_168C&DEV_003E&SUBSYS_082717AA&REV_32 ;for Lenovo
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_LE_NFA344A.ndi,         PCI\VEN_168C&DEV_003E&SUBSYS_083717AA&REV_32 ;for Lenovo FCC SKU
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_LE_NFA344A.ndi,         PCI\VEN_168C&DEV_003E&SUBSYS_084717AA&REV_32 ;for Lenovo Indonesia SKU
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_LE_NFA344A.ndi,         PCI\VEN_168C&DEV_003E&SUBSYS_085717AA&REV_32 ;for Lenovo AGN SKU
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_LE_Killer_NFA344A.ndi,  PCI\VEN_168C&DEV_003E&SUBSYS_143517AA&REV_32 ;for Lenovo
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA344A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_083711AD&REV_32 ;for LiteOn
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA364A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_081811AD&REV_32 ;for LiteOn
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA324A_5.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_052311AD&REV_32 ;for LiteOn
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_LE_NFA324A_5.ndi,       PCI\VEN_168C&DEV_003E&SUBSYS_302417AA&REV_32 ;for LiteOn
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_LG_NFA324A_5.ndi,       PCI\VEN_168C&DEV_003E&SUBSYS_051311AD&REV_32 ;for LG
%ATHR.DeviceDesc.2582_2%   = ATHR_DEV_OS63_988x_Killer_NFA324A_5.ndi,   PCI\VEN_168C&DEV_003E&SUBSYS_143A1A56&REV_32 ;for Killer1435-S
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA344A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_02581DAC ;for Sparklan (white brand)
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA364A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_02591DAC ;for Sparklan
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA324A_5.ndi,          PCI\VEN_168C&DEV_003E&SUBSYS_02611DAC&REV_32 ;for Sparklan
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA344A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_E0A6105B&REV_32 ;for Foxconn
%ATHR.DeviceDesc.6320_3%   = ATHR_DEV_OS63_988x_NFA344A.ndi,            PCI\VEN_168C&DEV_003E&SUBSYS_E0A5105B&REV_32 ;for Foxconn
;;Start of FTM section

[ATHR_DEV_OS63_988x_FTM.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, UtfMode.reg, D0PC.reg, roam.reg, wmmac.reg, FW_FTM.reg, BD_FTM.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_FTM.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_FTM.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

;;End of FTM section

;;Start of Rome 2.x section
[ATHR_DEV_OS63_988x_NFA324.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_20.reg, BD_NFA324.reg, enableLegacyBurst.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA324.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA324.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA324.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_Killer_NFA344.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_20.reg, BD_NFA344_le.reg, CoexConfig_dell.reg, wowEnable.reg, enableSmbios.reg, enableLegacyBurst.reg, BandPrefer_WirelessMode.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA344_le.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_Killer_NFA344.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_Killer_NFA344.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_LE_Killer_NFA344.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_20.reg, BD_NFA344_le.reg, 11acUefi.reg, CoexConfig_le.reg, enableLegacyBurst.reg, enableSmbios.reg, BandPrefer_WirelessMode.reg, NotifyChannelChangeEnable.reg ; Win10 only 1
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA344_le.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_LE_Killer_NFA344.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_LE_Killer_NFA344.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_NFA344.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_20.reg, BD_NFA344.reg, enableLegacyBurst.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA344.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA344.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA344.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_NFA345.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_20.reg, BD_NFA345.reg, enableLegacyBurst.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA345.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA345.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA345.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_NFA354.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_20.reg, BD_NFA354.reg, enableLegacyBurst.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA354.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA354.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA354.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_NFA355.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_20.reg, BD_NFA355.reg, enableLegacyBurst.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA355.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA355.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA355.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_FUJI_NFA344.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_20.reg, BD_NFA344.reg, wowEnable.reg, enableLegacyBurst.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA344.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_FUJI_NFA344.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_FUJI_NFA344.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_LE_NFA344.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_20.reg, BD_NFA344_le.reg, TPCOffset_le_344.reg, TPC_Profile_LE_344.reg, resumeAsyncDlFw.reg, 11acUefi.reg, CoexConfig_le.reg, enableLegacyBurst.reg, NotifyChannelChangeEnable.reg ; Win10 only 1
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA344_le.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_LE_NFA344.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_LE_NFA344.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_LE_NFA345.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_20.reg, BD_NFA345.reg, resumeAsyncDlFw.reg, 11acUefi.reg, CoexConfig_le.reg, enableLegacyBurst.reg, NotifyChannelChangeEnable.reg ; Win10 only 1
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA345.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_LE_NFA345.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_LE_NFA345.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_LE_NFA345_IPG.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_20.reg, BD_NFA345_le.reg, TPCOffset_le_345.reg, TPC_Profile_LE_345.reg, resumeAsyncDlFw.reg, 11acUefi.reg, CoexConfig_le.reg, enableLegacyBurst.reg, MAX_MSDU.reg, NotifyChannelChangeEnable.reg ; Win10 only 2
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA345_le.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_LE_NFA345_IPG.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_LE_NFA345_IPG.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AC_NFA344.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_20.reg, BD_NFA344.reg, enableIOACv20.reg, BandPrefer_WirelessMode.reg, GOTimeQuota.reg, enableLegacyBurst.reg, AdjustRSSI2.reg ; Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA344.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AC_NFA344.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AC_NFA344.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AS_NFA344.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_20.reg, BD_NFA344.reg, enableLegacyBurst.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA344.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA344.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA344.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AS_NFA345.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_20.reg, BD_NFA345.reg, enableLegacyBurst.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA345.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA345.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA345.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_ss_NFA354.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, ignore11denable.reg, FW_20.reg, BD_NFA354.reg, CoexConfig_ss.reg, TPC_Profile_SS.reg, D3TimingOpEnable_ss.reg, BandPrefer_WirelessMode.reg, ANI_Disable.reg, DYN_ANI_On_RTS.reg, BeLatency.reg, enableLegacyBurst.reg, enableSmbios.reg, DisableAmsdu.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA354.CopyFiles, atheros_BD_NFA354_SS.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_ss_NFA354.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_ss_NFA354.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_ss_NFA355.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, ignore11denable.reg, FW_20.reg, BD_NFA355.reg, CoexConfig_ss.reg, D3TimingOpEnable_ss.reg, BandPrefer_WirelessMode.reg, BeLatency.reg, enableLegacyBurst.reg, DisableAmsdu.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW.CopyFiles, atheros_BD_NFA355.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_ss_NFA355.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_ss_NFA355.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

;;End of Rome 2.x Section

;;Start of Tufello 1.0 Sections

[ATHR_DEV_OS63_988x_NFA425_TF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA425_TF.reg, enableTxbfee.reg, enableDVS.reg, enableVht2G.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA425_TF.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA425_TF.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA425_TF.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_SS_NFA425_TF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA425_TF.reg, enableTxbfee.reg, enableDVS.reg, enableSmbios.reg, enableVht2G.reg, DisableAmsdu.reg , ignore11denable.reg, CoexConfig_ss.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA425_TF.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_SS_NFA425_TF.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_SS_NFA425_TF.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_NFA435_TF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF.reg, enableTxbfee.reg, enableDVS.reg, enableVht2G.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA435_TF.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA435_TF.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_SS_NFA435_TF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF.reg, enableTxbfee.reg, enableDVS.reg, BandPrefer_WirelessMode.reg, enableVht2G.reg, DisableAmsdu.reg , ignore11denable.reg, CoexConfig_ss.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_SS_NFA435_TF.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_SS_NFA435_TF.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_SS_NFA455_TF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA455_TF.reg, enableTxbfee.reg, enableDVS.reg, CoexConfig_ss.reg, BandPrefer_WirelessMode.reg, enableVht2G.reg, DisableAmsdu.reg , ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA455_TF.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_SS_NFA455_TF.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_SS_NFA455_TF.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AC_NFA435_TF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF.reg, enableTxbfee.reg, enableDVS.reg, enableVht2G.reg, BandPrefer_WirelessMode.reg, enableSmbios.reg, AdjustRSSI2.reg ; Win10 only 1
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AC_NFA435_TF.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AC_NFA435_TF.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_LE_NFA435_TF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF.reg, enableTxbfee.reg, wowEnable.reg, enableDVS.reg, enableTTA.reg, 11acUefi.reg, TPC_Profile_NFA435_LE.reg, enableVht2G.reg, stbcTxbfWar.reg, BdfExtPerUEFI.reg, WarScanAfterRadioOn.reg, enableLegacyBurst.reg, DPC_Core_2.reg, NotifyChannelChangeEnable.reg ; Win10 only 5
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF.CopyFiles, atheros_BD_NFA435_TF_LE.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_LE_NFA435_TF.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_LE_NFA435_TF.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AS_NFA435_TF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF_A.reg, enableTxbfee.reg, enableDVS.reg, wowEnable.reg, TPC_Profile_NFA435_AS.reg, enableVht2G.reg, serviceMonWlan.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF_A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA435_TF.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA435_TF.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AS_NFA435_2_TF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF_A.reg, enableTxbfee.reg, enableDVS.reg, wowEnable.reg, TPC_Profile_NFA435_AS.reg, enableVht2G.reg, enableSMBIOS.reg, enableLegacyBurst.reg, serviceMonWlan.reg, enableHwRfKill.reg ; Win8 Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF_A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA435_2_TF.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA435_2_TF.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = machine.inf, netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration, PciD3ColdSupported

[ATHR_DEV_OS63_988x_AS_NFA435_SGL_TF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF_A.reg, enableTxbfee.reg, wowEnable.reg, TPC_Profile_NFA435_AS.reg, enableVht2G.reg, enableSMBIOS.reg, enableLegacyBurst.reg, serviceMonWlan.reg, enableHwRfKill.reg ; Win8 Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF_A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA435_SGL_TF.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA435_SGL_TF.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = machine.inf, netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration, PciD3ColdSupported

[ATHR_DEV_OS63_988x_AS_NFA435_SGL_CS_TF.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF_A.reg, enableTxbfee.reg, wowEnable.reg, TPC_Profile_NFA435_AS.reg, enableVht2G.reg, enableSMBIOS.reg, enableLegacyBurst.reg, serviceMonWlan.reg, EnableModulatedDTIM3.reg, enableHwRfKill.reg ; Win8 Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF_A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA435_SGL_CS_TF.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA435_SGL_CS_TF.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = machine.inf, netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration, PciD3ColdSupported

;;End of Tufello 1.0 Sections

;;Start of Tufello 1.1 Sections

[ATHR_DEV_OS63_988x_NFA425_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA425_TF11.reg, enableTxbfee.reg, enableDVS.reg, enableVht2G.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA425_TF11.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA425_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA425_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_NFA435A_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF11.reg, enableTxbfee.reg, enableDVS.reg, enableTTA.reg, wowEnable.reg, 11acUefi.reg, TPC_Profile_NFA435_LE.reg, enableVht2G.reg, stbcTxbfWar.reg, enableLegacyBurst.reg, BdfExtPerUEFI.reg, DPC_Core_2.reg ; Win8 Win10 only, Win10 only 1
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF11.CopyFiles, atheros_BD_NFA435_TF11_LE.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA435A_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA435A_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_LE_NFA425_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA425_TF11.reg, enableTxbfee.reg, wowEnable.reg, enableDVS.reg, enableTTA.reg, enableVht2G.reg, stbcTxbfWar.reg, enableLegacyBurst.reg, TPC_Profile_NFA435_LE.reg, BdfExtPerUEFI.reg, 11acUefi.reg, DPC_Core_2.reg, NotifyChannelChangeEnable.reg ; Win10 only 2
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA425_TF11_L.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_LE_NFA425_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_LE_NFA425_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AC_NFA425_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA425_TF11.reg, enableTxbfee.reg, enableDVS.reg, enableVht2G.reg, BandPrefer_WirelessMode.reg, CtlPerUEFI.reg, AdjustRSSI2.reg ; Win10 only 2 reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA425_TF11.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AC_NFA425_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AC_NFA425_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_NFA425_SGL_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA425_TF11.reg, enableTxbfee.reg, enableVht2G.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA425_TF11.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA425_SGL_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA425_SGL_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_SS_NFA425_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA425_TF11.reg, enableTxbfee.reg, enableDVS.reg, enableSmbios.reg, enableVht2G.reg, DisableAmsdu.reg, BandPrefer_WirelessMode.reg , ignore11denable.reg, CoexConfig_ss.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA425_TF11.CopyFiles, atheros_BD_NFA425_TF11_SS.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_SS_NFA425_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_SS_NFA425_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AS_NFA425_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA425_TF11_A.reg, enableTxbfee.reg, enableDVS.reg, wowEnable.reg, enableVht2G.reg, serviceMonWlan.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA425_TF11_A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA425_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA425_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AS_NFA425_2_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA425_TF11_A.reg, enableTxbfee.reg, enableDVS.reg, wowEnable.reg, enableVht2G.reg, serviceMonWlan.reg, enableSmbios.reg, Ch1213Option.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA425_TF11_A.CopyFiles, atheros_BD_NFA425_TF11_A_low.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA425_2_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA425_2_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = machine.inf, netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration, PciD3ColdSupported

[ATHR_DEV_OS63_988x_AS_NFA425_SGL_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA425_TF11_A.reg, enableTxbfee.reg, wowEnable.reg, enableVht2G.reg, serviceMonWlan.reg, enableHwRfKill.reg ; Win8 Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA425_TF11_A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA425_SGL_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA425_SGL_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AS_NFA425_2_SGL_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA425_TF11_A.reg, enableTxbfee.reg, wowEnable.reg, enableVht2G.reg, serviceMonWlan.reg, enableSmbios.reg, enableHwRfKill.reg ; Win8 Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA425_TF11_A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA425_2_SGL_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA425_2_SGL_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AS_NFA425_3_SGL_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA425_TF11_A.reg, enableTxbfee.reg, wowEnable.reg, enableVht2G.reg, serviceMonWlan.reg, enableSmbios.reg, Ch1213Option.reg, enableHwRfKill.reg ; Win8 Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA425_TF11_A.CopyFiles, atheros_BD_NFA425_TF11_A_low.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA425_3_SGL_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA425_3_SGL_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = machine.inf, netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration, PciD3ColdSupported

[ATHR_DEV_OS63_988x_ECS_NFA425_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA425_TF11_A.reg, enableTxbfee.reg, wowEnable.reg, enableVht2G.reg, serviceMonWlan.reg, enableSmbios.reg, enableHwRfKill.reg ; Win8 Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA425_TF11_A.CopyFiles, atheros_BD_NFA425_TF11_A_low.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_ECS_NFA425_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_ECS_NFA425_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_NFA435_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF11.reg, enableTxbfee.reg, enableDVS.reg, enableVht2G.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF11.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA435_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA435_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_NFA435_SGL_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF11.reg, enableTxbfee.reg, enableVht2G.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF11.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA435_SGL_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA435_SGL_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_SS_NFA435_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF11.reg, enableTxbfee.reg, enableDVS.reg, BandPrefer_WirelessMode.reg, enableVht2G.reg, DisableAmsdu.reg , ignore11denable.reg, CoexConfig_ss.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF11.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_SS_NFA435_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_SS_NFA435_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_SS_NFA455_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF11.reg, enableTxbfee.reg, enableDVS.reg, CoexConfig_ss.reg, BandPrefer_WirelessMode.reg, enableVht2G.reg, DisableAmsdu.reg , ignore11denable.reg, CoexConfig_ss.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF11.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_SS_NFA455_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_SS_NFA455_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AC_NFA435_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF11.reg, enableTxbfee.reg, enableDVS.reg, enableVht2G.reg, BandPrefer_WirelessMode.reg, enableSmbios.reg, enableLegacyBurst.reg, CtlPerUEFI.reg, AdjustRSSI2.reg ; Win10 only 2
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF11.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AC_NFA435_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AC_NFA435_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_LE_NFA435_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF11.reg, enableTxbfee.reg, wowEnable.reg, enableDVS.reg, enableTTA.reg, 11acUefi.reg, TPC_Profile_NFA435_LE.reg, enableVht2G.reg, stbcTxbfWar.reg, enableLegacyBurst.reg, BdfExtPerUEFI.reg, BdfExtPerACPI.reg, DPC_Core_2.reg, NotifyChannelChangeEnable.reg ; Win8 Win10 only, Win10 only 2
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF11.CopyFiles, atheros_BD_NFA435_TF11_LE.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_LE_NFA435_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_LE_NFA435_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AS_NFA435_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF11_A.reg, enableTxbfee.reg, enableDVS.reg, wowEnable.reg, enableVht2G.reg, enableSMBIOS.reg, enableLegacyBurst.reg, serviceMonWlan.reg, enableHwRfKill.reg ; Win8 Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF11_A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA435_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA435_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = machine.inf, netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration, PciD3ColdSupported

[ATHR_DEV_OS63_988x_AS_NFA435_SGL_TF11.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_TF.reg, BD_NFA435_TF11_A.reg, enableTxbfee.reg, wowEnable.reg, enableVht2G.reg, enableSMBIOS.reg, enableLegacyBurst.reg, serviceMonWlan.reg, enableHwRfKill.reg ; Win8 Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_TF.CopyFiles, atheros_BD_NFA435_TF11_A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA435_SGL_TF11.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA435_SGL_TF11.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = machine.inf, netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration, PciD3ColdSupported

;;End of Tufello 1.1 Sections

;;Start of Rome 3.x section

[ATHR_DEV_OS63_988x_NFA324A_1.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA324A_1.reg, enableTxbfee.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA324A_1.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA324A_1.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA324A_1.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_SS_COB.ndi.NTX86] ; Win10 only
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_SS_COB.reg, enableTxbfee.reg, wowEnable.reg, enableSmbios.reg, MacAddressPerUEFI.reg, enableLegacyBurst.reg, ch128Disable.reg, disable2gHt40.reg, CoexConfig_ss.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_SS_COB.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_SS_COB.ndi.NTX86.Services] ; Win10 only
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_SS_COB.ndi.NTX86.HW] ; Win10 only
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_SS_COB_1.ndi.NTX86] ; Win10 only
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_SS_COB_1.reg, enableTxbfee.reg, wowEnable.reg, enableSmbios.reg, MacAddressPerUEFI.reg, enableLegacyBurst.reg, ch128Disable.reg, disable2gHt40.reg, CoexConfig_ss.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_SS_COB_1.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_SS_COB_1.ndi.NTX86.Services] ; Win10 only
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_SS_COB_1.ndi.NTX86.HW] ; Win10 only
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_SS_COB_2.ndi.NTX86] ; Win10 only
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_SS_COB_2.reg, enableTxbfee.reg, wowEnable.reg, enableSmbios.reg, MacAddressPerUEFI.reg, enableLegacyBurst.reg, ch128Disable.reg, disable2gHt40.reg, CoexConfig_ss.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_SS_COB_2.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_SS_COB_2.ndi.NTX86.Services] ; Win10 only
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_SS_COB_2.ndi.NTX86.HW] ; Win10 only
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_NFA324A_5.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA324A_5.reg, enableTxbfee.reg, enableSmbiosLe.reg, ANI_Disable.reg, DYN_ANI_On_RTS.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA324A_5.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA324A_5.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA324A_5.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_LE_NFA324A_5.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA324A_5.reg, enableTxbfee.reg, ANI_Disable.reg, DYN_ANI_On_RTS.reg,enableTTA.reg, enableVht2G.reg, stbcTxbfWar.reg, disableTXBFforBadPerfAPs.reg, enableLegacyBurst.reg, BdfExtPerUEFI.reg, 11acUefi.reg, DPC_Core_2.reg ; Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA324A_5.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_LE_NFA324A_5.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_LE_NFA324A_5.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_LG_NFA324A_5.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA324A_5.reg, enableTxbfee.reg, ANI_Enable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA324A_5.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_LG_NFA324A_5.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_LG_NFA324A_5.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_Killer_NFA324A_5.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA324A_5.reg, enableTxbfee.reg, enableSmbios.reg, BandPrefer_WirelessMode.reg, DPC_Core_2.reg ; Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA324A_5.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_Killer_NFA324A_5.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_Killer_NFA324A_5.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AC_NFA324A_5.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA324A_5.reg, enableTxbfee.reg, BandPrefer_WirelessMode.reg, enableSmbios.reg, wowEnable.reg, serviceMonWlan.reg, CtlPerUEFI.reg, AdjustRSSI2.reg ; Win10 only 2 reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA324A_5.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AC_NFA324A_5.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AC_NFA324A_5.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_SS_NFA324A_5.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA324A_5.reg, enableTxbfee.reg, BandPrefer_WirelessMode.reg, enableSmbios.reg, CoexConfig_ss.reg, DisableAmsdu.reg , ignore11denable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA324A_5.CopyFiles, atheros_BD_NFA324A_SS.CopyFiles, atheros_BD_NFA324A_5_B.CopyFiles ; Win10 only
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_SS_NFA324A_5.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_SS_NFA324A_5.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_NFA344A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA344A.reg, enableTxbfee.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA344A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA344A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA344A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_LE_NFA344A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = TPC_Profile_LE_000.reg, atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA344A_H.reg, enableTxbfee.reg, wowEnable.reg, enableTTA.reg, enableVht2G.reg, stbcTxbfWar.reg, disableTXBFforBadPerfAPs.reg, enableLegacyBurst.reg, BdfExtPerUEFI.reg, 11acUefi.reg, DPC_Core_2.reg, NotifyChannelChangeEnable.reg ; Win10 only 3
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA344A_H.CopyFiles, atheros_BD_NFA344A_LE.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_LE_NFA344A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_LE_NFA344A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_Killer_NFA344A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA344A.reg, enableTxbfee.reg, enableSmbios.reg, BandPrefer_WirelessMode.reg, DPC_Core_2.reg ; Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA344A.CopyFiles, atheros_BD_NFA344A_RV.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_Killer_NFA344A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_Killer_NFA344A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AS_NFA344A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA344A.reg, enableTxbfee.reg, WowEventIgnore.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA344A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA344A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA344A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AC_NFA344A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA344A.reg, enableTxbfee.reg, enableSmbios.reg, BandPrefer_WirelessMode.reg, CtlPerUEFI.reg, AdjustRSSI2.reg ; Win10 only 2 reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA344A.CopyFiles, atheros_BD_NFA344A_AC.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AC_NFA344A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AC_NFA344A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_VA_NFA344A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, enableSmbios.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA344A.reg, enableTxbfee.reg, BandPrefer_WirelessMode.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA344A.CopyFiles, atheros_BD_NFA344A_AC.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_VA_NFA344A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_VA_NFA344A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_FJ_NFA344A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA344A.reg, enableTxbfee.reg, WirelessMode_simple.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA344A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_FJ_NFA344A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_FJ_NFA344A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_FJ_1_NFA344A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA344A.reg, enableTxbfee.reg, WirelessMode_simple.reg, wowEnable.reg, PCIEWarmReset.reg ; Win10 only 1
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA344A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_FJ_1_NFA344A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_FJ_1_NFA344A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_NFA354A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA354A.reg, enableTxbfee.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA354A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA354A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA354A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_NFA364A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA364A.reg, enableTxbfee.reg, wowEnable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA364A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_NFA364A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_NFA364A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AS_NFA364A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA364A.reg, enableTxbfee.reg, wowEnable.reg, enableSmbios.reg, serviceMonWlan.reg, enableHwRfKill.reg ; Win8 Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA364A.CopyFiles, atheros_BD_NFA364A_1213.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA364A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA364A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AS_NFA364A_2.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA364A_A.reg, enableTxbfee.reg, wowEnable.reg, enableSmbios.reg, serviceMonWlan.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA364A_A.CopyFiles, atheros_BD_NFA364A_1213.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA364A_2.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA364A_2.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AS_NFA364A_3.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA364A.reg, enableTxbfee.reg, wowEnable.reg, enableSmbios.reg, serviceMonWlan.reg, WowEventIgnore.reg, disableTXBFforBadPerfAPs.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA364A.CopyFiles, atheros_BD_NFA364A_1213.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_NFA364A_3.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_NFA364A_3.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_QCA9008.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_QCA9008.reg, enableTxbfee.reg, WowEventIgnore.reg, wowEnable.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_QCA9008.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_QCA9008.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_QCA9008.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_USI_9008.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_QCA9008.reg, enableTxbfee.reg, enableSmbios.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_QCA9008.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_USI_9008.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_USI_9008.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AC_9008.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_QCA9008.reg, enableTxbfee.reg, enableSmbios.reg, CtlPerUEFI.reg, AdjustRSSI2.reg ; Win10 only 2 reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_QCA9008.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AC_9008.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AC_9008.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_AS_9008.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_QCA9008.reg, enableTxbfee.reg, wowEnable.reg, serviceMonWlan.reg, Ch1213Option.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_QCA9008.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_AS_9008.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_AS_9008.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_Killer_NFA364A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA364A.reg, enableTxbfee.reg, enableSmbios.reg, BandPrefer_WirelessMode.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA364A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_Killer_NFA364A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_Killer_NFA364A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_RV_Killer_NFA364A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA364A.reg, enableTxbfee.reg, enableSmbios.reg, BandPrefer_WirelessMode.reg, wowEnable.reg, disableTXBFforBadPerfAPs.reg, stbcTxbfWar.reg, serviceMonWlan.reg, CtlPerUEFI.reg ; Win10 only
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA364A.CopyFiles, atheros_BD_NFA364A_RV.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_RV_Killer_NFA364A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_RV_Killer_NFA364A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_RV_Killer_NFA364A_2.ndi.NTX86] ; Win10 only
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA364A.reg, enableTxbfee.reg, enableSmbios.reg, BandPrefer_WirelessMode.reg, wowEnable.reg, disableTXBFforBadPerfAPs.reg, stbcTxbfWar.reg, serviceMonWlan.reg, CtlPerUEFI.reg, BdfExtPerUEFI.reg, DPC_Core_2.reg ; Win10 only 3
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA364A.CopyFiles, atheros_BD_NFA364A_RV.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_RV_Killer_NFA364A_2.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_RV_Killer_NFA364A_2.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_LE_Killer_NFA364A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA364A.reg, disableTxbfee.reg, DYN_ANI.reg, DYN_BURST.reg, 11acUefi.reg, DPC_Core_2.reg , NotifyChannelChangeEnable.reg, DPC_Core_2.reg ; Win10 only 3
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA364A.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_LE_Killer_NFA364A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_LE_Killer_NFA364A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

[ATHR_DEV_OS63_988x_LE_Killer_NFA344A.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = TPC_Profile_LE_000.reg, atheros_os63.reg, atheros11n.reg, smpsDynamic.reg, qca_utf.reg, D0PC.reg, roam.reg, wmmac.reg, FW_3X.reg, BD_NFA344A_H.reg, disableTXBFforBadPerfAPs.reg, enableLegacyBurst.reg, BdfExtPerUEFI.reg, disableTxbfee.reg, DYN_ANI.reg, DYN_BURST.reg, 11acUefi.reg, DPC_Core_2.reg , NotifyChannelChangeEnable.reg ; Win8 Win10 only 4, Win10 only 2
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles, atheros_FW_3X.CopyFiles, atheros_BD_NFA344A_H.CopyFiles, atheros_BD_NFA344A_LE.CopyFiles
*IfType         = 71        ; IF_TYPE_IEEE80211
*MediaType      = 16        ; NdisMediumNative802_11
*PhysicalMediaType = 9      ; NdisPhysicalMediumNative802_11
Include         = machine.inf, netvwifibus.inf
Needs           = VWiFiBus.CopyFiles

[ATHR_DEV_OS63_988x_LE_Killer_NFA344A.ndi.NTX86.Services]
AddService = Qcamain10x86, 2, atheros.Service, atheros.EventLog
Include    = netvwifibus.inf
Needs      = VWiFiBus.Services

[ATHR_DEV_OS63_988x_LE_Killer_NFA344A.ndi.NTX86.HW]
AddReg  = MSI.reg
Include = netvwifibus.inf
Needs   = PciASPMOptIn, VWiFiBus.PnPFilterRegistration

;;End of Rome 3.x section

[atheros_os63.reg]
HKR, Ndi,                           Service,    0, "Qcamain10x86"
HKR, Ndi\Interfaces,                UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,                LowerRange, 0, "wlan,ethernet,vwifi"
HKR, , AddNewChannelfor11d, 0x00010001, 0
HKR, , disableP2pLinkSpeedInd, 0x00010001, 1  ; Win10 only
HKR, , AdaptiveSchedulerEnable, 0x00010001, 1 ; Win10 only

[atheros11n.reg]
HKR, Ndi\Params\roamPolicy,         ParamDesc,  0, %RoamAggressive%
HKR, Ndi\Params\roamPolicy,         Type,       0, "enum"
HKR, Ndi\Params\roamPolicy\enum,    "5",        0, %RssiHighest%
HKR, Ndi\Params\roamPolicy\enum,    "4",        0, %RssiMedium-high%
HKR, Ndi\Params\roamPolicy\enum,    "3",        0, %RssiMedium%
HKR, Ndi\Params\roamPolicy\enum,    "2",        0, %RssiMedium-low%
HKR, Ndi\Params\roamPolicy\enum,    "1",        0, %RssiLowest%
HKR, Ndi\Params\roamPolicy,         Default,    0, "3"
HKR, Ndi\params\NetworkAddress,     ParamDesc,  0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,     default,    0,  ""
HKR, Ndi\params\NetworkAddress,     LimitText,  0,  "12"
HKR, Ndi\params\NetworkAddress,     UpperCase,  0,  "1"
HKR, Ndi\params\NetworkAddress,     optional,   0,  "1"
HKR, Ndi\params\NetworkAddress,     type,       0,  "edit"

[qca_utf.reg]
HKR, , UtfMode,       0x10001,  "0"
HKR, , UtfTraceLevel, 0x10001,  "0"

[UtfMode.reg]
HKR, , UtfMode,       0x10001,  "1"
HKR, , UtfTraceLevel, 0x10001,  "0"

[atheros.DelReg]
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,ccode
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,halPcieClockReq
HKR,Ndi\params,radioEnable,0x2000
HKR,Ndi\params,sleepMode,0x2000
HKR,,gpioFunc0ActHi
HKR,,gpioFunc1ActHi
HKR,,gpioLedCustom
HKR,,gpioPinFunc0
HKR,,gpioPinFunc1
HKR, Ndi\params\NetworkAddress
HKR,,NetworkAddress
HKR, Ndi\params\roamPolicy
HKR,,roamPolicy
HKR,,ftEnable
HKR,,wmmacEnable
HKR,,BugCheckOnTargetFailure
HKR,,targetRecoveryEnabled
HKR,,FWFileName
HKR,,BoardDataFileName
HKR,,EnableHardwareRFKill
HKR,,rxChainMask
HKR,,txChainMaskLegacy
HKR,,rxChainMaskLegacy
HKR,,rxChainDetect
HKR,,rxChainDetectRef
HKR,,rxChainDetectThreshA
HKR,,rxChainDetectThreshG
HKR,,rxChainDetectDeltaA
HKR,,rxChainDetectDeltaG
HKR, Ndi\params\smpsDynamic
HKR, Ndi\params\D0PCEnable
HKR,,wmeEnabled
HKR,,halPcieWaen
HKR,,halPcieDetach
HKR,,ampEnable
HKR,,btCoexAntDivEnable
HKR,,translateNullSsid
HKR,,defaultIbssChannel
HKR,,paprdEnable
HKR,,lnaDivUseBtAntEnable
HKR,,antCtrlComm2gSwitchEnable
HKR,,extLnaCtlGpio
HKR,,rateCtrlTxFastDrop
HKR,,antDivLowRssiCfg
HKR,,btCoexDivDefVal
HKR,,antDivFastDivBias
HKR,,extAttenMarginCfg
HKR,,UtfMode
HKR,,UtfTraceLevel,
HKR,,DpcTargetProcessors
HKR,,DpcLockMode
HKR,,gAntennaDiversity
HKR,,ignore11dBeacon
HKR,,smbiosAuthenticationEnable
HKR,,resumeAsyncDlFw
HKR,,BEVOLatencyEnable
HKR,,wowEnable
HKR,,AcerWowOffload
HKR,,Txbfee
HKR,,Txbfeeenable
HKR,,TPCOffset
HKR,,CoexConfig
HKR,,enableTTA
HKR,,TpcProfile
HKR,,enableANI
HKR,,RTSOnANIFlag
HKR,,D3TimingOpEnable
HKR,,BurstDisableOnANIFlag
HKLM,SYSTEM\CurrentControlSet\Services\NativeWifiP\Parameters,EnableWoWLAN
HKR,,dot11acSelection
HKR,,SmUfCfgParaPolicy
HKR,,SIFSBurstEnable
HKR,,AddNewChannelfor11d
HKR,,NetBand
HKR,,wModeSelect
HKR,,VHT40WAR
HKR,,legacyburstenable
HKR,,stbcTxbfWar
HKR,,serviceMonWlan
HKR,,gEnableModulatedDTIM
HKR,,WowEventIgnore
HKR,,BdfExtPerUEFI
HKR,,disableTXBFforBadPerfAPs
HKR,,htamsduEnable
HKR,,disableP2pLinkSpeedInd ; Win10 only
HKR,,*TransmitBuffers       ; Win10 only
HKR,,DBFileName             ; Win10 only
HKR,,MacAddressPerUEFI      ; Win10 only
HKR,,AdaptiveSchedulerEnable; Win10 only
HKR,,ch128_disable          ; Win10 only
HKR,,CtlPerUEFI             ; Win10 only
HKR,,enable2GHzHt40Cap      ; Win10 only
HKR,,AdjustRSSI2            ; Win10 only
HKR,,EnableWowPME           ; Win10 only
HKR,,WarScanAfterRadioOn    ; Win10 only
HKR,,Ch1213_options         ; Win10 only
HKR,,CstateWarEnable        ; Win10 only
HKR,,skipRegAccessInPCIDevReset ; Win10 only
HKR,,WfdPreferred5GPhyMode  ; Win10 only
HKR,,NotifyChannelChangeEnable; Win10 only
HKR,,DisablePCIEWarmReset; Win10 only

[smpsDynamic.reg]
HKR, Ndi\params\smpsDynamic,            ParamDesc,  0,  %smpsDynamic%
HKR, Ndi\params\smpsDynamic,            Base,       0,  "10"
HKR, Ndi\params\smpsDynamic,            default,    0,  "0"
HKR, Ndi\params\smpsDynamic,            type,       0,  "enum"
HKR, Ndi\params\smpsDynamic\enum,       "1",        0,  %Enable%
HKR, Ndi\params\smpsDynamic\enum,       "0",        0,  %Disable%

[D0PC.reg]
HKR, NDI\params\D0PCEnable,ParamDesc,,          %D0PCDesc%
HKR, NDI\params\D0PCEnable,type,,               "enum"
HKR, NDI\params\D0PCEnable,Default,,            "0"
HKR, NDI\params\D0PCEnable\enum,0,,             %Disable%
HKR, NDI\params\D0PCEnable\enum,1,,             %Enable%

[BandPrefer_WirelessMode.reg]
HKR, Ndi\params\StaPreferredBand,      ParamDesc,          0,          "Preferred Band"
HKR, Ndi\params\StaPreferredBand,      default,            0,          "1"
HKR, Ndi\params\StaPreferredBand,      type,               0,          "enum"
HKR, Ndi\params\StaPreferredBand\enum, "1",                0,          "1 - No Preference"
HKR, Ndi\params\StaPreferredBand\enum, "2",                0,          "2 - Prefer 2.4Ghz Band"
HKR, Ndi\params\StaPreferredBand\enum, "3",                0,          "3 - Prefer 5Ghz Band"
HKR, Ndi\params\StaWirelessMode,       ParamDesc,          0,          "Wireless Mode"
HKR, Ndi\params\StaWirelessMode,       default,            0,          "12"
HKR, Ndi\params\StaWirelessMode,       type,               0,          "enum"
HKR, Ndi\params\StaWirelessMode\enum,  "1",                0,          "01 - 11 b"
HKR, Ndi\params\StaWirelessMode\enum,  "2",                0,          "02 - 11 g"
HKR, Ndi\params\StaWirelessMode\enum,  "3",                0,          "03 - 11 b/g"
HKR, Ndi\params\StaWirelessMode\enum,  "4",                0,          "04 - 11 g/n"
HKR, Ndi\params\StaWirelessMode\enum,  "5",                0,          "05 - 11 b/g/n"
HKR, Ndi\params\StaWirelessMode\enum,  "6",                0,          "06 - 11 a"
HKR, Ndi\params\StaWirelessMode\enum,  "7",                0,          "07 - 11 a/n"
HKR, Ndi\params\StaWirelessMode\enum,  "8",                0,          "08 - 11 a/b/g/n"
HKR, Ndi\params\StaWirelessMode\enum,  "9",                0,          "09 - 11 a/g/n"
HKR, Ndi\params\StaWirelessMode\enum,  "10",               0,          "10 - 11 a/n/ac"
HKR, Ndi\params\StaWirelessMode\enum,  "11",               0,          "11 - 11 a/g/n/ac"
HKR, Ndi\params\StaWirelessMode\enum,  "12",               0,          "12 - 11 a/b/g/n/ac"

[WirelessMode_simple.reg]
HKR, Ndi\params\StaWirelessMode,       ParamDesc,          0,          "Wireless Mode Selection"
HKR, Ndi\params\StaWirelessMode,       default,            0,          "12"
HKR, Ndi\params\StaWirelessMode,       type,               0,          "enum"
HKR, Ndi\params\StaWirelessMode\enum,  "5",                0,          "2GHz Only"
HKR, Ndi\params\StaWirelessMode\enum,  "10",               0,          "5GHz Only"
HKR, Ndi\params\StaWirelessMode\enum,  "12",               0,          "Auto"

[MSI.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 8

[ANI_Disable.reg]
HKR, , enableANI, 0x00010001, 0

[ANI_Enable.reg]
HKR, , enableANI, 0x00010001, 1

[DYN_ANI_On_RTS.reg]
HKR, , RTSOnANIFlag, 0x00010001, 1

[roam.reg]
HKR, , ftEnable, 0x00010001, 1

[wmmac.reg]
HKR, , wmmacEnable, 0x00010001, 1

[ignore11denable.reg]
HKR, , ignore11dBeacon, 0x00010001, 1

[wowEnable.reg]
HKR, , wowEnable, 0x00010001, 1

[resumeAsyncDlFw.reg]
HKR, , resumeAsyncDlFw, 0x00010001, 1

[BeLatency.reg]
HKR, , BEVOLatencyEnable, 0x00010001, 1

[11acUefi.reg]
HKR, , dot11acSelection, 0x00010001, 1

[TPC_Profile_NFA435_LE.reg]
HKR, , TpcProfile, 0x00010001, 4

[TPC_Profile_NFA435_AS.reg]
HKR, , TpcProfile, 0x00010001, 6

[enableSmbiosLe.reg]
HKR, , SmUfCfgParaPolicy, 0x00010001, 2

[enableSmbios.reg]
HKR, , SmUfCfgParaPolicy, 0x00010001, 1

[enableSSR.reg]
HKR, , BugCheckOnTargetFailure, 0x00010001, 0x22
HKR, , targetRecoveryEnabled, 0x00010001, 1

[GOTimeQuota.reg]
HKR, , MediaStreamGOTimeQuota, 0x00010001, 0x32

[enableIOACv20.reg]
HKR, , wowEnable, 0x00010001, 1
HKR, , AcerWowOffload, 0x00010001, 0x81

[enableTxbfee.reg]
HKR, , Txbfee, 0x00010001, 0x8D
HKR, , Txbfeeenable, 0x00010001, 1

[CoexConfig_dell.reg]
HKR, , CoexConfig, 0x00010001, 1

[CoexConfig_ss.reg]
HKR, , CoexConfig, 0x00010001, 2

[CoexConfig_le.reg]
HKR, , CoexConfig, 0x00010001, 4

[DPC_2_Cores.reg] ; Win10 no DpcLockMode
HKR, , DpcTargetProcessors, 0x00010001, 3

[DPC_Core_2.reg] ; Win10 only
HKR, , DpcTargetProcessors, 0x00010001, 4

[BURST_le_364A.reg]
HKR, , SIFSBurstEnable, 0x00010001, 0

[TPCOffset_le_344.reg]
HKR, , TPCOffset, 0x00010001, 0x25

[TPCOffset_le_345.reg]
HKR, , TPCOffset, 0x00010001, 0x45

[enableWoWWLAN.reg]
HKLM, SYSTEM\CurrentControlSet\Services\NativeWifiP\Parameters, EnableWoWLAN, 0x00010001, 1

[enableDVS.reg]
HKR, , gAntennaDiversity, 0x00010001, 3

[enableTTA.reg]
HKR, , enableTTA, 0x00010001, 1

[TPC_Profile_SS.reg]
HKR, , TpcProfile, 0x00010001, 1

[TPC_Profile_LE_344.reg]
HKR, , TpcProfile, 0x00010001, 2

[TPC_Profile_LE_000.reg]
HKR, , TpcProfile, 0x00010001, 7

[TPC_Profile_LE_345.reg]
HKR, , TpcProfile, 0x00010001, 3

[TPC_Profile_364A.reg]
HKR, , TpcProfile, 0x00010001, 5

[D3TimingOpEnable_ss.reg]
HKR, , D3TimingOpEnable, 0x00010001, 1

[DYN_ANI.reg]
HKR, , enableANI, 0x00010001, 1
HKR, , RTSOnANIFlag, 0x00010001, 1

[DYN_BURST.reg]
HKR, , BurstDisableOnANIFlag, 0x00010001, 1

[disableTxbfee.reg]
HKR, , Txbfeeenable, 0x00010001, 0

[enableVht2G.reg]
HKR, , NetBand, 0x00010001, 0x6FFFFFF
HKR, , wModeSelect, 0x00010001, 0x6FFFFFF
HKR, , VHT40WAR, 0x00010001, 1

[enableLegacyBurst.reg]
HKR, , legacyburstenable, 0x00010001, 1

[stbcTxbfWar.reg]
HKR, , stbcTxbfWar, 0x00010001, 1

[enableHwRfKill.reg]
HKR, , EnableHardwareRFKill, 0x00010001, 1

[serviceMonWlan.reg]
HKR, , serviceMonWlan, 0x00010001, 1

[EnableModulatedDTIM3.reg]
HKR, , gEnableModulatedDTIM, 0x00010001, 3

[WowEventIgnore.reg]
HKR, , WowEventIgnore, 0x00010001, 0x28

[BdfExtPerUEFI.reg]
HKR, , BdfExtPerUEFI, 0x00010001, 2

[BdfExtPerACPI.reg]
HKR, , BdfExtPerACPI, 0x00010001, 1

[disableTXBFforBadPerfAPs.reg]
HKR, , disableTXBFforBadPerfAPs, 0x00010001, 1

[DisableAmsdu.reg]
HKR, , htamsduEnable, 0x00010001, 0

[Ch1213Option.reg] 
HKR, , Ch1213_options, 0x00010001, 2

[MAX_MSDU.reg] ; Win10 only
HKR, , *TransmitBuffers, 0x00010001, 512

[MacAddressPerUEFI.reg] ; Win10 only
HKR, , MacAddressPerUEFI, 0x00010001, 1

[ch128Disable.reg] ; Win10 only
HKR, , ch128_disable, 0x00010001, 1

[CtlPerUEFI.reg] ; Win10 only
HKR, , CtlPerUEFI, 0x00010001, 1

[disable2gHt40.reg] ; Win10 only
HKR, , enable2GHzHt40Cap, 0x00010001, 0

[AdjustRSSI2.reg] ; Win10 only
HKR, , AdjustRSSI2, 0x00010001, 1

[EnableWowPME.reg] ; Win10 only
HKR, , EnableWowPME, 0x00010001, 1

[WarScanAfterRadioOn.reg] ; Win10 only
HKR, , WarScanAfterRadioOn, 0x00010001, 1

[CstateWarEnable.reg] ; Win10 only
HKR, , CstateWarEnable, 0x00010001, 1

[WfdPreferred5GPhyMode.reg] ; Win10 only
HKR, , WfdPreferred5GPhyMode, 0x00010001, 5

[NotifyChannelChangeEnable.reg] ; Win10 only
HKR, , NotifyChannelChangeEnable, 0x00010001, 1

[PCIEWarmReset.reg] ; Win10 only
HKR, , DisablePCIEWarmReset, 0x00010001, 0

;;End of Customized Section

[atheros.Service]
DisplayName     = %ATHR.Service.DispName%
ServiceType     = 1         ;SERVICE_KERNEL_DRIVER
StartType       = 3         ;SERVICE_DEMAND_START
ErrorControl    = 1         ;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\Qcamain10x86.sys
LoadOrderGroup  = NDIS

[atheros.EventLog]
AddReg = atheros.AddEventLog.reg

[atheros.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[atheros.CopyFiles]
Qcamain10x86.sys,,,2

;;Start of FTM FW and BD files

[FW_FTM.reg]
HKR, , FWFileName, 0x00000000, "qca_fw.bin"

[BD_FTM.reg]
HKR, , BoardDataFileName, 0x00000000, "fakeBoardData.bin"

;;End of FTM FW and BD files

;;Start of Rome 2.x FW and BD files

[FW_20.reg]
HKR, , FWFileName, 0x00000000, "qca61x4_1_1_2.bin"

[BD_NFA324.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_2p1_NFA324i_5.bin"

[BD_NFA344.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_2p1_NFA344i.bin"

[BD_NFA344_le.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_2p1_NFA344i_highTX.bin"

[BD_NFA345.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_2p1_NFA345i.bin"

[BD_NFA345_le.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_2p1_NFA345i_highTX.bin"

[BD_NFA354.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_2p1_NFA354xp.bin"

[BD_NFA355.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_2p1_NFA355i.bin"

[atheros_FW.CopyFiles]
qca61x4_1_1_2.bin,,,2

[atheros_BD_NFA324.CopyFiles]
eeprom_ar6320_2p1_NFA324i_5.bin,,,2

[atheros_BD_NFA344.CopyFiles]
eeprom_ar6320_2p1_NFA344i.bin,,,2

[atheros_BD_NFA344_le.CopyFiles]
eeprom_ar6320_2p1_NFA344i_highTX.bin,,,2

[atheros_BD_NFA345.CopyFiles]
eeprom_ar6320_2p1_NFA345i.bin,,,2

[atheros_BD_NFA345_le.CopyFiles]
eeprom_ar6320_2p1_NFA345i_highTX.bin,,,2

[atheros_BD_NFA354.CopyFiles]
eeprom_ar6320_2p1_NFA354xp.bin,,,2

[atheros_BD_NFA354_SS.CopyFiles]
eeprom_ar6320_2p1_NFA354xp_SS_EU.bin,,,2

[atheros_BD_NFA355.CopyFiles]
eeprom_ar6320_2p1_NFA355i.bin,,,2

;;End of Rome 2.x FW and BD files

;;Start of Tufello FW and BD files

[FW_TF.reg]
HKR, , FWFileName, 0x00000000, "qca9377_2_0.bin"
HKR, , DBFileName, 0x00000000, "Data9377_2_0.msc"

[BD_NFA425_TF.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_qca9377_1p0_NFA425_olpc.bin"

[BD_NFA425_TF11.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_qca9377_1p1_NFA425_olpc.bin"

[BD_NFA425_TF11_A.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_qca9377_1p1_NFA425_olpc_A.bin"

[BD_NFA425_TF11_A_low.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_qca9377_1p1_NFA425_olpc_A_low.bin"

[BD_NFA435_TF.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_qca9377_1p0_NFA435_olpc.bin"

[BD_NFA435_TF_A.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_qca9377_1p0_NFA435_olpc_A.bin"

[BD_NFA435_TF11.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_qca9377_1p1_NFA435_olpc.bin"

[BD_NFA435_TF11_A.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_qca9377_1p1_NFA435_olpc_A.bin"

[BD_NFA455_TF.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_qca9377_1p0_NFA455_olpc.bin"

[atheros_FW_TF.CopyFiles]
qca9377_2_0.bin,,,2
Data9377_2_0.msc,,,2 ; Win10 only

[atheros_BD_NFA425_TF.CopyFiles]
eeprom_qca9377_1p0_NFA425_olpc.bin,,,2

[atheros_BD_NFA425_TF11.CopyFiles]
eeprom_qca9377_1p1_NFA425_olpc.bin,,,2

[atheros_BD_NFA425_TF11_L.CopyFiles]
eeprom_qca9377_1p1_NFA425_olpc_L.bin,,,2

[atheros_BD_NFA425_TF11_A.CopyFiles]
eeprom_qca9377_1p1_NFA425_olpc_A.bin,,,2

[atheros_BD_NFA425_TF11_A_low.CopyFiles]
eeprom_qca9377_1p1_NFA425_olpc_A_low.bin,,,2
eeprom_qca9377_1p1_NFA425_olpc_A_low2.bin,,,2
eeprom_qca9377_1p1_NFA425_olpc_A_TP203NA.bin,,,2
eeprom_qca9377_1p1_NFA425_olpc_A_TP203NAH.bin,,,2
eeprom_qca9377_1p1_NFA425_olpc_A_T103HAF.bin,,,2

[atheros_BD_NFA425_TF11_SS.CopyFiles]
eeprom_qca9377_1p1_NFA425_olpc_SS_N.bin,,,2
eeprom_qca9377_1p1_NFA425_olpc_SS_S.bin,,,2
eeprom_qca9377_1p1_NFA425_olpc_SS_T.bin,,,2
eeprom_qca9377_1p1_NFA425_olpc_SS_V.bin,,,2

[atheros_BD_NFA435_TF.CopyFiles]
eeprom_qca9377_1p0_NFA435_olpc.bin,,,2

[atheros_BD_NFA435_TF_A.CopyFiles]
eeprom_qca9377_1p0_NFA435_olpc_A.bin,,,2
eeprom_qca9377_1p0_NFA435_olpc_A_TP401NA.bin,,,2

[atheros_BD_NFA435_TF_LE.CopyFiles]
eeprom_qca9377_1p0_NFA435_olpc_LE_1.bin,,,2
eeprom_qca9377_1p0_NFA435_olpc_LE_2.bin,,,2

[atheros_BD_NFA435_TF11.CopyFiles]
eeprom_qca9377_1p1_NFA435_olpc.bin,,,2

[atheros_BD_NFA435_TF11_A.CopyFiles]
eeprom_qca9377_1p1_NFA435_olpc_A.bin,,,2
eeprom_qca9377_1p0_NFA435_olpc_A_TP401NA.bin,,,2

[atheros_BD_NFA435_TF11_LE.CopyFiles]
eeprom_qca9377_1p1_NFA435_olpc_LE_1.bin,,,2
eeprom_qca9377_1p1_NFA435_olpc_LE_2.bin,,,2
eeprom_qca9377_1p1_NFA435_olpc_LE_3.bin,,,2

[atheros_BD_NFA455_TF.CopyFiles]
eeprom_qca9377_1p0_NFA455_olpc.bin,,,2

;;End of Tufello FW and BD files

;;Start of Rome 3.x FW and BD files

[FW_3X.reg]
HKR, , FWFileName, 0x00000000, "qca61x4_2_2.bin"
HKR, , DBFileName, 0x00000000, "Data61x4_2_2.msc" ; Win10 only

[BD_NFA324A_1.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_3p0_NFA324i_1.bin"

[BD_SS_COB.reg] ; Win10 only
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_3p0_SS_700.bin"

[BD_SS_COB_1.reg] ; Win10 only
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_3p0_SS_720.bin"

[BD_SS_COB_2.reg] ; Win10 only
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_3p0_SS_620.bin"

[BD_NFA324A_5.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_3p0_NFA324i_5.bin"

[BD_NFA344A.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_3p0_NFA344a.bin"

[BD_NFA344A_H.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_3p0_NFA344a_highTX.bin"

[BD_NFA354A.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_3p0_NFA354xp.bin"

[BD_NFA364A.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_3p0_NFA364xp.bin"

[BD_NFA364A_A.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_3p0_NFA364xp_powerA.bin"

[BD_QCA9008.reg]
HKR, , BoardDataFileName, 0x00000000, "eeprom_ar6320_3p0_QCA9008.bin"

[atheros_FW_3X.CopyFiles]
qca61x4_2_2.bin,,,2
Data61x4_2_2.msc,,,2 ; Win10 only

[atheros_BD_NFA324A_1.CopyFiles]
eeprom_ar6320_3p0_NFA324i_1.bin,,,2

[atheros_BD_SS_COB.CopyFiles] ; Win10 only
eeprom_ar6320_3p0_SS_700.bin,,,2
eeprom_ar6320_3p0_SS_700_K.bin,,,2

[atheros_BD_SS_COB_1.CopyFiles] ; Win10 only
eeprom_ar6320_3p0_SS_720.bin,,,2
eeprom_ar6320_3p0_SS_720_K.bin,,,2

[atheros_BD_SS_COB_2.CopyFiles] ; Win10 only
eeprom_ar6320_3p0_SS_620.bin,,,2
eeprom_ar6320_3p0_SS_620_K.bin,,,2

[atheros_BD_NFA324A_5.CopyFiles]
eeprom_ar6320_3p0_NFA324i_5.bin,,,2

[atheros_BD_NFA324A_SS.CopyFiles]
eeprom_ar6320_3p0_NFA324i_5_SS_N.bin,,,2
eeprom_ar6320_3p0_NFA324i_5_SS_S.bin,,,2
eeprom_ar6320_3p0_NFA324i_5_SS_T.bin,,,2
eeprom_ar6320_3p0_NFA324i_5_SS_V.bin,,,2

[atheros_BD_NFA324A_5_B.CopyFiles] ; Win10 only
eeprom_ar6320_3p0_NFA324i_5_B.bin,,,2

[atheros_BD_NFA344A.CopyFiles]
eeprom_ar6320_3p0_NFA344a.bin,,,2

[atheros_BD_NFA344A_H.CopyFiles]
eeprom_ar6320_3p0_NFA344a_highTX.bin,,,2

[atheros_BD_NFA344A_LE.CopyFiles]
eeprom_ar6320_3p0_NFA344a_highTX_LE_1.bin,,,2
eeprom_ar6320_3p0_NFA344a_highTX_LE_2.bin,,,2
eeprom_ar6320_3p0_NFA344a_highTX_LE_3.bin,,,2
eeprom_ar6320_3p0_NFA344a_highTX_LE_4.bin,,,2
eeprom_ar6320_3p0_NFA344a_highTX_LE_5.bin,,,2
eeprom_ar6320_3p0_NFA344a_highTX_LE_6.bin,,,2
eeprom_ar6320_3p0_NFA344a_highTX_LE_7.bin,,,2
eeprom_ar6320_3p0_NFA344a_highTX_LE_8.bin,,,2

[atheros_BD_NFA344A_AC.CopyFiles]
eeprom_ar6320_3p0_NFA344a_BLP.bin,,,2
eeprom_ar6320_3p0_NFA344a_AC_BRN.bin,,,2

[atheros_BD_NFA354A.CopyFiles]
eeprom_ar6320_3p0_NFA354xp.bin,,,2

[atheros_BD_NFA364A.CopyFiles]
eeprom_ar6320_3p0_NFA364xp.bin,,,2

[atheros_BD_NFA364A_A.CopyFiles]
eeprom_ar6320_3p0_NFA364xp_powerA.bin,,,2

[atheros_BD_NFA364A_1213.CopyFiles]
eeprom_ar6320_3p0_NFA364xp_power1213.bin,,,2

[atheros_BD_NFA364A_RV.CopyFiles]
eeprom_ar6320_3p0_NFA364xp_RV_0519.bin ,,,2
eeprom_ar6320_3p0_NFA364xp_RV_0520.bin ,,,2
eeprom_ar6320_3p0_NFA364xp_LE_1.bin ,,,2
eeprom_ar6320_3p0_NFA364xp_LE_2.bin ,,,2

[atheros_BD_NFA344A_RV.CopyFiles]
eeprom_ar6320_3p0_NFA344A_power1213_RV_0519.bin ,,,2

[atheros_BD_QCA9008.CopyFiles]
eeprom_ar6320_3p0_QCA9008.bin,,,2

;;End of Rome 3.x FW and BD files

[SourceDisksNames]
1 = %DiskDescription%,,,

[SourceDisksFiles]
Qcamain10x86.sys                          = 1,,
qca61x4_1_1_2.bin                         = 1,,
eeprom_ar6320_2p1_NFA324i_5.bin           = 1,,
eeprom_ar6320_2p1_NFA344i.bin             = 1,,
eeprom_ar6320_2p1_NFA344i_highTX.bin      = 1,,
eeprom_ar6320_2p1_NFA345i.bin             = 1,,
eeprom_ar6320_2p1_NFA345i_highTX.bin      = 1,,
eeprom_ar6320_2p1_NFA354xp.bin            = 1,,
eeprom_ar6320_2p1_NFA354xp_SS_EU.bin      = 1,,
eeprom_ar6320_2p1_NFA355i.bin             = 1,,
qca9377_2_0.bin                           = 1,,
Data9377_2_0.msc                          = 1,, ; Win10 only
eeprom_qca9377_1p0_NFA425_olpc.bin        = 1,,
eeprom_qca9377_1p1_NFA425_olpc.bin        = 1,,
eeprom_qca9377_1p1_NFA425_olpc_L.bin      = 1,,
eeprom_qca9377_1p1_NFA425_olpc_A.bin      = 1,,
eeprom_qca9377_1p1_NFA425_olpc_A_low.bin  = 1,,
eeprom_qca9377_1p1_NFA425_olpc_A_low2.bin = 1,,
eeprom_qca9377_1p1_NFA425_olpc_A_TP203NA.bin	= 1,,
eeprom_qca9377_1p1_NFA425_olpc_A_TP203NAH.bin	= 1,,
eeprom_qca9377_1p1_NFA425_olpc_A_T103HAF.bin	= 1,,
eeprom_qca9377_1p0_NFA435_olpc_A_TP401NA.bin	= 1,,
eeprom_qca9377_1p1_NFA425_olpc_SS_N.bin   = 1,,
eeprom_qca9377_1p1_NFA425_olpc_SS_S.bin   = 1,,
eeprom_qca9377_1p1_NFA425_olpc_SS_T.bin   = 1,,
eeprom_qca9377_1p1_NFA425_olpc_SS_V.bin   = 1,,
eeprom_qca9377_1p0_NFA435_olpc.bin        = 1,,
eeprom_qca9377_1p0_NFA435_olpc_A.bin      = 1,,
eeprom_qca9377_1p0_NFA435_olpc_LE_1.bin   = 1,,
eeprom_qca9377_1p0_NFA435_olpc_LE_2.bin   = 1,,
eeprom_qca9377_1p1_NFA435_olpc.bin        = 1,,
eeprom_qca9377_1p1_NFA435_olpc_A.bin      = 1,,
eeprom_qca9377_1p1_NFA435_olpc_LE_1.bin   = 1,,
eeprom_qca9377_1p1_NFA435_olpc_LE_2.bin   = 1,,
eeprom_qca9377_1p1_NFA435_olpc_LE_3.bin   = 1,,
eeprom_qca9377_1p0_NFA455_olpc.bin        = 1,,
qca61x4_2_2.bin                           = 1,,
Data61x4_2_2.msc                          = 1,, ; Win10 only
eeprom_ar6320_3p0_NFA324i_1.bin           = 1,,
eeprom_ar6320_3p0_SS_700.bin              = 1,, ; Win10 only
eeprom_ar6320_3p0_SS_700_K.bin            = 1,, ; Win10 only
eeprom_ar6320_3p0_SS_720.bin              = 1,, ; Win10 only
eeprom_ar6320_3p0_SS_720_K.bin              = 1,, ; Win10 only
eeprom_ar6320_3p0_SS_620.bin              = 1,, ; Win10 only
eeprom_ar6320_3p0_SS_620_K.bin		  	  = 1,, ; Win10 only
eeprom_ar6320_3p0_NFA324i_5.bin           = 1,,
eeprom_ar6320_3p0_NFA324i_5_SS_N.bin      = 1,,
eeprom_ar6320_3p0_NFA324i_5_SS_S.bin      = 1,,
eeprom_ar6320_3p0_NFA324i_5_SS_T.bin      = 1,,
eeprom_ar6320_3p0_NFA324i_5_SS_V.bin      = 1,,
eeprom_ar6320_3p0_NFA324i_5_B.bin         = 1,, ; Win10 only
eeprom_ar6320_3p0_NFA344a.bin             = 1,,
eeprom_ar6320_3p0_NFA344a_highTX.bin      = 1,,
eeprom_ar6320_3p0_NFA344a_highTX_LE_1.bin = 1,,
eeprom_ar6320_3p0_NFA344a_highTX_LE_2.bin = 1,,
eeprom_ar6320_3p0_NFA344a_highTX_LE_3.bin = 1,,
eeprom_ar6320_3p0_NFA344a_highTX_LE_4.bin = 1,,
eeprom_ar6320_3p0_NFA344a_highTX_LE_5.bin = 1,,
eeprom_ar6320_3p0_NFA344a_highTX_LE_6.bin = 1,,
eeprom_ar6320_3p0_NFA344a_highTX_LE_7.bin = 1,,
eeprom_ar6320_3p0_NFA344a_highTX_LE_8.bin = 1,,
eeprom_ar6320_3p0_NFA344a_BLP.bin         = 1,,
eeprom_ar6320_3p0_NFA344a_AC_BRN.bin      = 1,,
eeprom_ar6320_3p0_NFA354xp.bin            = 1,,
eeprom_ar6320_3p0_NFA364xp.bin            = 1,,
eeprom_ar6320_3p0_NFA364xp_powerA.bin     = 1,,
eeprom_ar6320_3p0_NFA364xp_power1213.bin  = 1,,
eeprom_ar6320_3p0_NFA364xp_RV_0519.bin    = 1,,
eeprom_ar6320_3p0_NFA364xp_RV_0520.bin    = 1,,
eeprom_ar6320_3p0_NFA364xp_LE_1.bin 	  = 1,,
eeprom_ar6320_3p0_NFA364xp_LE_2.bin 	  = 1,,
eeprom_ar6320_3p0_QCA9008.bin             = 1,,
eeprom_ar6320_3p0_NFA344A_power1213.bin   = 1,,
eeprom_ar6320_3p0_NFA344A_power1213_DE_5459.bin = 1,,
eeprom_ar6320_3p0_NFA344A_power1213_DE_0410.bin = 1,,
eeprom_ar6320_3p0_NFA344A_power1213_RV_0519.bin = 1,,

[DestinationDirs]
atheros.CopyFiles                  = 12
atheros_FW.CopyFiles               = 12
atheros_BD_NFA324.CopyFiles        = 12
atheros_BD_NFA344.CopyFiles        = 12
atheros_BD_NFA344_le.CopyFiles     = 12
atheros_BD_NFA345.CopyFiles        = 12
atheros_BD_NFA345_le.CopyFiles     = 12
atheros_BD_NFA354.CopyFiles        = 12
atheros_BD_NFA354_SS.CopyFiles     = 12
atheros_BD_NFA355.CopyFiles        = 12
atheros_FW_TF.CopyFiles            = 12
atheros_BD_NFA425_TF.CopyFiles     = 12
atheros_BD_NFA425_TF_L.CopyFiles     = 12
atheros_BD_NFA425_TF11.CopyFiles   = 12
atheros_BD_NFA425_TF11_A.CopyFiles = 12
atheros_BD_NFA425_TF11_A_low.CopyFiles = 12
atheros_BD_NFA425_TF11_SS.CopyFiles    = 12
atheros_BD_NFA435_TF.CopyFiles     = 12
atheros_BD_NFA435_TF_A.CopyFiles   = 12
atheros_BD_NFA435_TF_LE.CopyFiles  = 12
atheros_BD_NFA435_TF11.CopyFiles   = 12
atheros_BD_NFA435_TF11_A.CopyFiles = 12
atheros_BD_NFA435_TF11_LE.CopyFiles= 12
atheros_BD_NFA455_TF.CopyFiles     = 12
atheros_FW_3X.CopyFiles            = 12
atheros_BD_NFA324A_1.CopyFiles     = 12
atheros_BD_SS_COB.CopyFiles        = 12 ; Win10 only
atheros_BD_SS_COB_1.CopyFiles      = 12 ; Win10 only
atheros_BD_SS_COB_2.CopyFiles      = 12 ; Win10 only
atheros_BD_NFA324A_5.CopyFiles     = 12
atheros_BD_NFA324A_SS.CopyFiles    = 12
atheros_BD_NFA324A_5_B.CopyFiles   = 12 ; Win10 only
atheros_BD_NFA344A.CopyFiles       = 12
atheros_BD_NFA344A_H.CopyFiles     = 12
atheros_BD_NFA344A_LE.CopyFiles    = 12
atheros_BD_NFA344A_AC.CopyFiles    = 12
atheros_BD_NFA354A.CopyFiles       = 12
atheros_BD_NFA364A.CopyFiles       = 12
atheros_BD_NFA364A_A.CopyFiles     = 12
atheros_BD_NFA364A_1213.CopyFiles  = 12
atheros_BD_NFA364A_RV.CopyFiles    = 12
atheros_BD_QCA9008.CopyFiles       = 12
atheros_BD_NFA344A_RV.CopyFiles    = 12
DefaultDestDir                     = 11

[Strings]
Msft                         = "Microsoft"
Atheros                      = "Qualcomm Atheros Communications Inc."
ATHR.Service.DispName        = "Qualcomm Atheros Extensible Wireless LAN 11AC device driver"
DiskDescription              = "Qualcomm Atheros Sample Driver Disk 1"
Enable                       = "Enable"
Disable                      = "Disable"
RoamAggressive               = "Roaming aggressiveness"
RssiLowest                   = "1.Lowest"
RssiMedium-low               = "2.Medium-low"   
RssiMedium                   = "3.Medium"
RssiMedium-high              = "4.Medium-high"
RssiHighest                  = "5.Highest"
NetworkAddress               = "Network Address"
bkScanEnable                 = "BackgroundScan On/Off"
radioEnable                  = "Radio On/Off"
smpsDynamic                  = "Dynamic MIMO Power Save"
D0PCDesc                     = "D0 PacketCoalescing"
ATHR.DeviceDesc.6320         = "Qualcomm Atheros QCA61x4 Wireless Network Adapter"
ATHR.DeviceDesc.6320_2       = "Qualcomm Atheros QCA61x4 Wireless Network Adapter"
ATHR.DeviceDesc.6320_3       = "Qualcomm Atheros QCA61x4A Wireless Network Adapter"
ATHR.DeviceDesc.2582         = "Killer Wireless-n/a/ac 1525 Wireless Network Adapter"
ATHR.DeviceDesc.2582_2       = "Killer Wireless-n/a/ac 1435 Wireless Network Adapter"
ATHR.DeviceDesc.2582_3       = "Killer Wireless-n/a/ac 1535 Wireless Network Adapter"
ATHR.DeviceDesc.9377         = "Qualcomm Atheros QCA9377 Wireless Network Adapter"

