;; netrtwlanu.inf 
;;
;; Realtek Wireless 802.11b/g/n USB 2.0 Network Adapter
;;
;; Copyright (C) 2012 Realtek Semiconductor Corp.
;;
;; This release is primarily for WHQL test.
;;

;; FOR XP/Vista/Win7/Win8

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %DLink%
CatalogFile.NT	= netrtwlanu.cat		;; for WHQL certified
DriverVer = 02/25/2013,1024.0.0218.2013

[Manufacturer]
%DLink% = DLink,NTx86

[ControlFlags]
ExcludeFromSelect = *

[DLink.NTx86]
;; For 8821A DLINK			================================================================
%DLink-DWA171.DeviceDesc% 			= RTL8821au.ndi, 	USB\VID_2001&PID_3314
;;----------------------------------------------------------------------------
;; Realtek 8821AU default installation
;;----------------------------------------------------------------------------



[RTL8821au.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, RTL8811AU_COMMON.reg, TcpReorderEnable.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8821au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8821au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration




[RTL8821auEdimax.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, RTL8811AU_COMMON.reg, TcpReorderEnable.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8821auEdimax.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8821auEdimax.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration


;;
;; OS relative registry.
;;
[NDIS_62.reg]
HKR, Ndi\Interfaces,	UpperRange, 0, "ndis5,mdcwifi"
HKR, Ndi\Interfaces,	LowerRange, 0, "wlan, ethernet, vwifi"
HKR, Ndi,				Service,    0, "RtlWlanu"
;;
;; OS relative service.
;;
[RtlWlanu.Service]
DisplayName    	= %DLink-DWA171.DeviceDesc.DispName%
ServiceType    	= 1		; %SERVICE_KERNEL_DRIVER%
StartType      	= 3		; %SERRVICE_DEMAND_START%
ErrorControl   	= 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  	= %12%\rtwlanu.sys
LoadOrderGroup 	= NDIS

;;
;; OS relative event log.
;;
[RtlWlanu.EventLog]
AddReg 			= RtlWlanu.AddEventLog.reg

[RtlWlanu.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

;*******************************************************************************
; USB common paramters
;*******************************************************************************
[UsbCommon.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For PDN mode switch.
HKR,,PDNMode,0,"0"

;; For PDN mode switch.
HKR,,DongleSS,0,"1"

;; For Different selective suspend power save level. Now support 1 and 2. 2 is better.
HKR,,SSPwrLvl,0,"2"

;; For wake on WLAN mode enable.
;;HKR,,WoWLANMode,0,"0"

;; For Different AC mode Rx parameters.
HKR,,AcUsbDmaTime,0,"10"
HKR,,AcUsbDmaSize,0,"5"

;; For Different Tx power limit.
;;HKR,,TxPwrLimit,0x00010001,"0xFFFFFFFF"		// Define as DW

;; For Different Tx power limit control registry test.
;;HKR,,TxPwrCtrl, 0x00010001 ,"0x12345678"

;; For IO mode switch.
HKR,,NByteAccess,0,"2"

;; For Init mode
HKR,,FWOffload,0,"2"

;; RFE Enable
HKR,,EnRFEType,0,"1"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation OS Relative
;-------------------------------------------------------------------------------

[Ndis6UsbRxAgg.reg]
HKR,defaults,UsbRxAggMode,0,"2"
HKR,,UsbRxAggMode,0,"2"
HKR,defaults,UsbRxAggPageCount,0,"16"
HKR,,UsbRxAggPageCount,0,"16"


[Ndis6UsbRxAgg_Jaguar.reg]
HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"
HKR,defaults,UsbRxAggPageCount,0,"16"
HKR,,UsbRxAggPageCount,0,"16"

;-------------------------------------------------------------------------------
;	WoWlanMode
;-------------------------------------------------------------------------------
[WowlanEnable.reg]
HKR,,WoWLANMode,0,"3"
HKR,,WoWLANLPSLevel,0,"1"
[WowlanDisable.reg]
HKR,,WoWLANMode,0,"0"
HKR,,WoWLANLPSLevel,0,"0"

;-------------------------------------------------------------------------------
;	USB selective suspend.
;-------------------------------------------------------------------------------
[RtlSsOnn.reg]
HKR,,EnableUsbSS,0,"1"
[RtlSsOff.reg]
HKR,,EnableUsbSS,0,"0"

;-------------------------------------------------------------------------------
;	TX path selection.
;-------------------------------------------------------------------------------
[TxByTimerOnn.reg]
HKR,,SendPacketByTimer,0,"1"
[TxByTimerOff.reg]
HKR,,SendPacketByTimer,0,"0"


;-------------------------------------------------------------------------------
;     Timer GPIO.
;-------------------------------------------------------------------------------
[TimerGPIOSettingCommon.reg]
;; For GPIO detect setting.
HKR,,TimerGPIO,0,"0"
HKR,,GPIODelay,0,"2000"
HKR,,GPIOBack,0,"2000"

[TimerGPIOSetting8723A.reg]
;; For GPIO detect setting.
HKR,,TimerGPIO,0,"0"
HKR,,GPIODelay,0,"1000"
HKR,,GPIOBack,0,"1000"

[TimerGPIOSetting8812AU.reg]
;; For GPIO detect setting.
HKR,,TimerGPIO,0,"1"
HKR,,GPIODelay,0,"500"
HKR,,GPIOBack,0,"250"

;---------------------------------------------------------------------------------
;    Customer ID
;---------------------------------------------------------------------------------
[CustomerID_Belkin.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"22"

[CustomerID_DLink.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"44"

[CustomerID_NEC.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"45"

[CustomerID_ASUS.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"35"

;;----------------------------------------------------------------------------
;; TCP Reorder Control Parameters
;;----------------------------------------------------------------------------
[TcpReorderEnable.reg]
HKR,,TcpReorder,0,"1"
[TcpReorderDisable.reg]
HKR,,TcpReorder,0,"0"

;;----------------------------------------------------------------------------
;; Earlymode Control Parameters
;;----------------------------------------------------------------------------
[EarlyModeEnable.reg]
HKR,,bEarlymodeEnable,0,"1"
[EarlyModeDisable.reg]
HKR,,bEarlymodeEnable,0,"0"

;-------------------------------------------------------------------------------
;	Custom Tx Power Limit And Power By Rate Parameters
;-------------------------------------------------------------------------------
[CustomTxPwrConfigFile.reg]
HKR,,PwrByRateFile,0,""
HKR,,PwrLimitFile,0,""

;-------------------------------------------------------------------------------
; Intel Soft AP Mode Reg
;-------------------------------------------------------------------------------
[Intel.reg]
HKR,Ndi\params\ForcedBstDataRate,        ParamDesc,  0, "Broadcast/Multicast Data Rate"
HKR,Ndi\params\ForcedBstDataRate,        type,       0, "enum"
HKR,Ndi\params\ForcedBstDataRate,        default,    0, "0"
HKR,Ndi\params\ForcedBstDataRate\enum,   "0",        0, "Auto"
HKR,Ndi\params\ForcedBstDataRate\enum,   "2",        0, "1Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "4",        0, "2Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "11",      0, "5.5Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "22",     0, "11Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "12",      0, "6Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "18",     0, "9Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "24",     0, "12Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "36",     0, "18Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "48",     0, "24Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "72",     0, "36Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "96",     0, "48Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "108",     0, "54Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "128",     0, "MCS0"
HKR,Ndi\params\ForcedBstDataRate\enum,   "129",     0, "MCS1"
HKR,Ndi\params\ForcedBstDataRate\enum,   "130",     0, "MCS2"
HKR,Ndi\params\ForcedBstDataRate\enum,   "131",     0, "MCS3"
HKR,Ndi\params\ForcedBstDataRate\enum,   "132",     0, "MCS4"
HKR,Ndi\params\ForcedBstDataRate\enum,   "133",     0, "MCS5"
HKR,Ndi\params\ForcedBstDataRate\enum,   "134",     0, "MCS6"
HKR,Ndi\params\ForcedBstDataRate\enum,   "135",     0, "MCS7"
HKR,Ndi\params\ForcedBstDataRate\enum,   "136",     0, "MCS8"
HKR,Ndi\params\ForcedBstDataRate\enum,   "137",     0, "MCS9"
HKR,Ndi\params\ForcedBstDataRate\enum,   "138",     0, "MCS10"
HKR,Ndi\params\ForcedBstDataRate\enum,   "139",     0, "MCS11"
HKR,Ndi\params\ForcedBstDataRate\enum,   "140",     0, "MCS12"
HKR,Ndi\params\ForcedBstDataRate\enum,   "141",     0, "MCS13"
HKR,Ndi\params\ForcedBstDataRate\enum,   "142",     0, "MCS14"
HKR,Ndi\params\ForcedBstDataRate\enum,   "143",     0, "MCS15"

;;----------------------------------------------------------------------------
;; Realtek WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,defaults,SSID,0,"ANY"
HKR,,SSID,0,"ANY"

HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"

;; Antenna Diversity Type
HKR,Ndi\params\AntennaDivType, 	default, 	0, "0"
HKR,Ndi\params\AntennaDivType,	ParamDesc, 	0, "Antenna Diversity Type"
HKR,Ndi\params\AntennaDivType, 		    type, 		    0, "enum"
HKR,Ndi\params\AntennaDivType\enum,   	"0",        	0, "Auto"
HKR,Ndi\params\AntennaDivType\enum,   	"1",        	0, "T/Rx Diversity"
HKR,Ndi\params\AntennaDivType\enum,   	"2",        	0, "2R Diversity"
HKR,Ndi\params\AntennaDivType\enum,   	"3",        	0, "Fixed"  

;;HKR,Ndi\params\NetworkType,			ParamDesc,  0, %NETWORK_TYPE_STR%
;;HKR,Ndi\params\NetworkType,			type,       0, "enum"
;;HKR,Ndi\params\NetworkType,			default,    0, "1"
;;HKR,Ndi\params\NetworkType\enum,		"0",        0, %AD_HOC_STR%
;;HKR,Ndi\params\NetworkType\enum,		"1",        0, %INFRASTRUCTURE_STR%
;;HKR,Ndi\params\NetworkType\enum,		"2",        0, %AUTO_SELECT%
;;HKR,defaults,NetworkType,0,"1"
;;HKR,,NetworkType,0,"1"

HKR,defaults,StaUapsd,0,"0"
HKR,,StaUapsd,0,"0"

;; For WiFi test, 1: WiFi Config and 0: Performance Config
HKR,Ndi\params\WiFiConfg,        ParamDesc,  0, "WiFi Config"
HKR,Ndi\params\WiFiConfg,        type,       0, "enum"
HKR,Ndi\params\WiFiConfg,        default,    0, "0"
HKR,Ndi\params\WiFiConfg\enum,   "0",        0, "Performance"
HKR,Ndi\params\WiFiConfg\enum,   "1",        0, "WiFi"
HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"
HKR,,WiFiConfg,,"0"

;; For LDPC test, config
;;// BIT0: Enable VHT LDPC Rx, BIT1: Enable VHT LDPC Tx, BIT4: Enable HT LDPC Rx, BIT5: Enable HT LDPC Tx
HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
HKR,Ndi\params\LdpcCap,        type,       0, "enum"
HKR,Ndi\params\LdpcCap,        default,    0, "51"
HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
HKR,Ndi\params\LdpcCap\enum,   "1",        0, "VHT LDPC RX"
HKR,Ndi\params\LdpcCap\enum,   "2",        0, "VHT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
HKR,,LdpcCap,,"51"

;; For STBC test, config
;;// BIT0: Enable VHT STBC Rx, BIT1: Enable VHT STBC Tx, BIT4: Enable HT STBC Rx, BIT5: Enable HT STBC Tx
HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
HKR,Ndi\params\StbcCap,        type,       0, "enum"
HKR,Ndi\params\StbcCap,        default,    0, "51"
HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
HKR,Ndi\params\StbcCap\enum,   "1",        0, "VHT STBC RX"
HKR,Ndi\params\StbcCap\enum,   "2",        0, "VHT STBC TX"
HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
HKR,,StbcCap,,"51"

;; For AMfactor test, config
;;// AMDPU factor from 0 to 7
;;HKR,Ndi\params\AMfactor,        ParamDesc,  0, "VHT AMPDU Factor"
;;HKR,Ndi\params\AMfactor,        type,       0, "enum"
;;HKR,Ndi\params\AMfactor,        default,    0, "7"
;;HKR,Ndi\params\AMfactor\enum,   "0",        0, "VHT AMPDU Factor 0"
;;HKR,Ndi\params\AMfactor\enum,   "1",        0, "VHT AMPDU Factor 1"
;;HKR,Ndi\params\AMfactor\enum,   "2",        0, "VHT AMPDU Factor 2"
;;HKR,Ndi\params\AMfactor\enum,   "3",        0, "VHT AMPDU Factor 3"
;;HKR,Ndi\params\AMfactor\enum,   "4",       0, "VHT AMPDU Factor 4"
;;HKR,Ndi\params\AMfactor\enum,   "5",       0, "VHT AMPDU Factor 5"
;;HKR,Ndi\params\AMfactor\enum,   "6",       0, "VHT AMPDU Factor 6"
;;HKR,Ndi\params\AMfactor\enum,   "7",       0, "VHT AMPDU Factor 7"
;;HKR,defaults,AMfactor,0,"7"
;;HKR,,AMfactor,0,"7"
;;HKR,,AMfactor,,"7"

;; For VHTRSec test, config
;;// VHTRSec factor from 0 to 7
;;HKR,Ndi\params\VHTRSec,        ParamDesc,  0, "VHT Support Rate"
;;HKR,Ndi\params\VHTRSec,        type,       0, "enum"
;;HKR,Ndi\params\VHTRSec,        default,    0, "0"
;;HKR,Ndi\params\VHTRSec\enum,   "0",        0, "Defau Setting"
;;HKR,Ndi\params\VHTRSec\enum,   "1",        0, "Support 1SS MCS0-7"
;;HKR,Ndi\params\VHTRSec\enum,   "2",        0, "Support 1SS MCS0-8"
;;HKR,Ndi\params\VHTRSec\enum,   "3",        0, "Support 1SS MCS0-9"
;;HKR,Ndi\params\VHTRSec\enum,   "4",       0, "Support 1SS/2SS MCS0-7"
;;HKR,Ndi\params\VHTRSec\enum,   "5",       0, "Support 1SS/2SS MCS0-8"
;;HKR,Ndi\params\VHTRSec\enum,   "6",       0, "Support 1SS/2SS MCS0-9"
;;HKR,Ndi\params\VHTRSec\enum,   "7",       0, "Support 1SS MCS0-7 2SS MCS0-9"
;;HKR,Ndi\params\VHTRSec\enum,   "8",       0, "Support 1SS MCS0-8 2SS MCS0-9"
;;HKR,Ndi\params\VHTRSec\enum,   "9",       0, "Support 1SS MCS0-7 2SS MCS0-8"
;;HKR,defaults,VHTRSec,0,"0"
;;HKR,,VHTRSec,0,"0"
;;HKR,,VHTRSec,,"0"

;; For RxReorder_WinSize test, config
;;// RxReorder_WinSize factor from 0 to 7
;;HKR,Ndi\params\RxReorder_WinSize,        ParamDesc,  0, "RxReorder_WinSize"
;;HKR,Ndi\params\RxReorder_WinSize,        type,       0, "enum"
;;HKR,Ndi\params\RxReorder_WinSize,        default,    0, "64"
;;HKR,Ndi\params\RxReorder_WinSize\enum,   "64",        0, "Defau Setting"
;;HKR,Ndi\params\RxReorder_WinSize\enum,   "4",        0, "RxReorder_WinSize 4"
;;HKR,Ndi\params\RxReorder_WinSize\enum,   "8",        0, "RxReorder_WinSize 8"
;;HKR,Ndi\params\RxReorder_WinSize\enum,   "16",        0, "RxReorder_WinSize 16"
;;HKR,Ndi\params\RxReorder_WinSize\enum,   "32",       0, "RxReorder_WinSize 32"
;;HKR,Ndi\params\RxReorder_WinSize\enum,   "64",       0, "RxReorder_WinSize 64"
;;HKR,Ndi\params\RxReorder_WinSize\enum,   "128",       0, "RxReorder_WinSize 128"
;;HKR,Ndi\params\RxReorder_WinSize\enum,   "256",       0, "RxReorder_WinSize 256"
;;HKR,defaults,RxReorder_WinSize,0,"64"
;;HKR,,RxReorder_WinSize,0,"64"
;;HKR,,RxReorder_WinSize,,"64"

;; For RxReorder_PendTime test, config
;;// RxReorder_PendTime factor from 0 to 7
;;HKR,Ndi\params\RxReorder_PendTime,        ParamDesc,  0, "RxReorder_PendTime"
;;HKR,Ndi\params\RxReorder_PendTime,        type,       0, "enum"
;;HKR,Ndi\params\RxReorder_PendTime,        default,    0, "30"
;;HKR,Ndi\params\RxReorder_PendTime\enum,   "30",        0, "Defau Setting"
;;HKR,Ndi\params\RxReorder_PendTime\enum,   "0",        0, "RxReorder_PendTime 0"
;;HKR,Ndi\params\RxReorder_PendTime\enum,   "10",        0, "RxReorder_PendTime 10"
;;HKR,Ndi\params\RxReorder_PendTime\enum,   "20",        0, "RxReorder_PendTime 20"
;;HKR,Ndi\params\RxReorder_PendTime\enum,   "30",       0, "RxReorder_PendTime 30"
;;HKR,Ndi\params\RxReorder_PendTime\enum,   "50",       0, "RxReorder_PendTime 50"
;;HKR,Ndi\params\RxReorder_PendTime\enum,   "100",       0, "RxReorder_PendTime 100"
;;HKR,Ndi\params\RxReorder_PendTime\enum,   "500",       0, "RxReorder_PendTime 500"
;;HKR,Ndi\params\RxReorder_PendTime\enum,   "1000",       0, "RxReorder_PendTime 1000"
;;HKR,Ndi\params\RxReorder_PendTime\enum,   "10000",       0, "RxReorder_PendTime 10000"
;;HKR,defaults,RxReorder_PendTime,0,"30"
;;HKR,,RxReorder_PendTime,0,"30"
;;HKR,,RxReorder_PendTime,,"30"

;;HKR,Ndi\params\BWSetting,        ParamDesc,  0, "Bandwisth"     
;;HKR,Ndi\params\BWSetting,        type,       0, "enum"                  
;;HKR,Ndi\params\BWSetting,        default,    0, "2"                    
;;HKR,Ndi\params\BWSetting\enum,   "2",        0, "Defau Setting"        
;;HKR,Ndi\params\BWSetting\enum,   "0",        0, "20 MHz only"   
;;HKR,Ndi\params\BWSetting\enum,   "1",        0, "20_40 MHz only"   
;;HKR,Ndi\params\BWSetting\enum,   "2",        0, "20_40_80 MHz" 
;;HKR,defaults,BWSetting,0,"2"                                           
;;HKR,,BWSetting,0,"2"                                                   
;;HKR,,BWSetting,,"2"                                                    


;;HKR,Ndi\params\RFType,        ParamDesc,  0, "RfType"
;;HKR,Ndi\params\RFType,        type,       0, "enum"
;;HKR,Ndi\params\RFType,        default,    0, "5"
;;HKR,Ndi\params\RFType\enum,   "5",        0, "Default Setting"
;;HKR,Ndi\params\RFType\enum,   "3",        0, "RF_1T1R"
;;HKR,Ndi\params\RFType\enum,   "2",        0, "RF_2T2R"
;;HKR,defaults,RfType,0,"5"
;;HKR,,RFType,0,"5"
;;HKR,,RFType,,"5"

;;HKR,,UsbCurMode,0,"0"
;;HKR,,UsbCurMode,,"0"

;;HKR,,UsbMode3To2Cnt,0,"0"
;;HKR,,UsbMode3To2Cnt,,"0"

;;HKR,,UsbMode2To3Cnt,0,"0"
;;HKR,,UsbMode2To3Cnt,,"0"

;;Tx power limit
HKR,,EnableTxPowerLimit,0,"0"

;; For QoS test, 1: WiFi Config and 0: Performance Config
HKR,Ndi\params\QoS,        ParamDesc,  0, "QoS Support"
HKR,Ndi\params\QoS,        type,       0, "enum"
HKR,Ndi\params\QoS,        default,    0, "0"
HKR,Ndi\params\QoS\enum,   "0",        0, "Not Support QoS"
HKR,Ndi\params\QoS\enum,   "1",        0, "Support QoS"
HKR,Ndi\params\QoS\enum,   "2",        0, "Auto"
HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"
HKR,,QoS,,"1"

;; For TX pwoer control test,
;;// Value = 0-15 power = 0-7.5dBm
;;HKR,Ndi\params\TPCLvl,        ParamDesc,  	0, "TxPowerLvl Increase"
;;HKR,Ndi\params\TPCLvl,        type,       	0, "enum"
;;HKR,Ndi\params\TPCLvl,        default,    	0, "0"
;;HKR,Ndi\params\TPCLvl\enum,   "0",        	0, "0 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "1",        	0, "0.5 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "2",        	0, "1.0 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "3",        	0, "1.5 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "4",       		0, "2.0 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "5",       		0, "2.5 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "6",       		0, "3.0 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "7",       		0, "3.5 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "8",       		0, "4.0 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "9",       		0, "4.5 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "10",       	0, "5.0 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "11",       	0, "5.5 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "12",       	0, "6.0 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "13",       	0, "6.5 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "14",       	0, "7.0 dBm"
;;HKR,Ndi\params\TPCLvl\enum,   "15",       	0, "7.5 dBm"
;;HKR,defaults,TPCLvl,0,"0"
;;HKR,,TPCLvl,0,"0"
;;HKR,,TPCLvl,,"0"

HKR,defaults,RxReorder,0,"1"
HKR,,RxReorder,0,"1"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"0"
HKR,,bLeisurePs,0,"0"

;Fw Control LPS
HKR,defaults,bFwCtrlLPS,0,"1"
HKR,,bFwCtrlLPS,0,"1"

;; LPS Interval
;HKR,defaults,LPSIntvl,0,"5"
HKR,,LPSIntvl,0,"5"

;BTmode
HKR,,bBTMode,0,"1"

; Reset Tx Hang
HKR,defaults,USBResetTxHang,0,"1"
HKR,,USBResetTxHang,0,"1"

HKR,,WEPinNmode,0,"0"

; OS protocol offload detection and decision
HKR,,ProtocolOffloadDecision,0,"1"

; Win8 FSS mode detection mechanism
HKR,,FSSDetection,0,"1"

;-------------------------------------------------------------------------------
;	Some function ability setting
;-------------------------------------------------------------------------------
HKR,defaults,UPDMEnable,0,"1"
HKR,,UPDMEnable,0,"1"

HKR,defaults,LinkSpeedLevel,0,"0"
HKR,,LinkSpeedLevel,0,"0"

HKR,defaults,AutoConnect,0,"1"
HKR,,AutoConnect,0,"1"

HKR,defaults,RWRetry,0,"0"
HKR,,RWRetry,0,"0"

HKR,defaults,MultiMode,0,"1"
HKR,,MultiMode,0,"1"

HKR,defaults,TxMode,0,"0"
HKR,,TxMode,0,"0"

HKR,defaults,PwrTblSel,0,"0"
HKR,,PwrTblSel,0,"0"
HKR,defaults,PwrByRate,0,"0"
HKR,,PwrByRate,0,"0"
HKR,defaults,PwrRaTbl1,0,"0"
HKR,,PwrRaTbl1,0,"0"
HKR,defaults,PwrRaTbl2,0,"0"
HKR,,PwrRaTbl2,0,"0"
HKR,defaults,PwrRaTbl3,0,"0"
HKR,,PwrRaTbl3,0,"0"
HKR,defaults,PwrRaTbl4,0,"0"
HKR,,PwrRaTbl4,0,"0"
HKR,defaults,PwrRaTbl5,0,"0"
HKR,,PwrRaTbl5,0,"0"
HKR,defaults,PwrRaTbl6,0,"0"
HKR,,PwrRaTbl6,0,"0"
HKR,defaults,PwrRaTbl7,0,"0"
HKR,,PwrRaTbl7,0,"0"
HKR,defaults,PwrRaTbl8,0,"0"
HKR,,PwrRaTbl8,0,"0"
HKR,defaults,PwrRaTbl9,0,"0"
HKR,,PwrRaTbl9,0,"0"
HKR,defaults,PwrRaTbl10,0,"0"
HKR,,PwrRaTbl10,0,"0"
HKR,defaults,PwrRaTbl11,0,"0"
HKR,,PwrRaTbl11,0,"0"
HKR,defaults,PwrRaTbl12,0,"0"
HKR,,PwrRaTbl12,0,"0"
HKR,defaults,PwrRaTbl13,0,"0"
HKR,,PwrRaTbl13,0,"0"
HKR,defaults,PwrRaTbl14,0,"0"
HKR,,PwrRaTbl14,0,"0"
HKR,defaults,PwrRaTbl15,0,"0"
HKR,,PwrRaTbl15,0,"0"
HKR,defaults,PwrRaTbl16,0,"0"
HKR,,PwrRaTbl16,0,"0"

HKR,defaults,GainOffsetFCCLow,0,"0"
HKR,,GainOffsetFCCLow,0,"0"
HKR,defaults,GainOffsetFCC,0,"0"
HKR,,GainOffsetFCC,0,"0"
HKR,defaults,GainOffsetFCCHigh,0,"0"
HKR,,GainOffsetFCCHigh,0,"0"

HKR,defaults,GainOffsetMKKLow,0,"0"
HKR,,GainOffsetMKKLow,0,"0"
HKR,defaults,GainOffsetMKK,0,"0"
HKR,,GainOffsetMKK,0,"0"
HKR,defaults,GainOffsetMKKHigh,0,"0"
HKR,,GainOffsetMKKHigh,0,"0"

HKR,defaults,GainOffsetETSILow,0,"0"
HKR,,GainOffsetETSILow,0,"0"
HKR,defaults,GainOffsetETSI,0,"0"
HKR,,GainOffsetETSI,0,"0"
HKR,defaults,GainOffsetETSIHigh,0,"0"
HKR,,GainOffsetETSIHigh,0,"0"

HKR,defaults,RxSC,0,"0"
HKR,,RxSC,0,"0"

HKR,defaults,TxSC,0,"0"
HKR,,TxSC,0,"0"

;Dynamic batch indication
HKR,defaults,DynamicBatchEnable,0,"1"
HKR,,DynamicBatchEnable,0,"1"

HKR,defaults,BINumber,0,"10"
HKR,,BINumber,0,"10"

[Ndis5Set.reg]
HKR,Ndi\params\PSPXlinkMode,			ParamDesc,  0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode,			type,       0, "enum"
HKR,Ndi\params\PSPXlinkMode,			default,    0, "0"
HKR,Ndi\params\PSPXlinkMode\enum,		"0",        0, %DISABLE_STR%
HKR,Ndi\params\PSPXlinkMode\enum,		"1",        0, %ENABLE_STR%
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"

; Hw Beacon Max Error
HKR,,bBcnMaxErrorRegEnable,0,"0"

;Inactive Power Save
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"

HKR,defaults,AggDMEnable,0,"0"
HKR,,AggDMEnable,0,"0"

[Ndis6Set.reg]
;Inactive Power Save
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"

HKR,defaults,AggDMEnable,0,"1"
HKR,,AggDMEnable,0,"1"

; /****************************************************************************
; ** IHV Service Reg for CCX
; ****************************************************************************/
[CIHVS.reg]
HKR, Ndi\IHVExtensions, ExtensibilityDLL,       0,  "%SystemRoot%\system32\Rtlihvs.dll"
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID,   0,  "{6C2A8CCA-B2A2-4d81-A3B2-4E15F445C312}"
HKR, Ndi\IHVExtensions, GroupName,              0,  "Realtek CCX SDK IHV Service"
HKR, Ndi\IHVExtensions, AdapterOUI,             0x00010001, 0x00e04c

;;----------------------------------------------------------------------------
;; Wireless Mode Related Parameters
;;----------------------------------------------------------------------------
[11nWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

;; 40MHz Support in 11n
HKR,Ndi\params\BWSetting,        ParamDesc,  0, "Bandwidth"
HKR,Ndi\params\BWSetting,        type,       0, "enum"
HKR,Ndi\params\BWSetting,        default,    0, "1"
HKR,Ndi\params\BWSetting\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BWSetting\enum,   "1",        0, "20_40MHz"
HKR,defaults,BWSetting,0,"1"
HKR,,BWSetting,0,"1"
HKR,,BWSetting,,"1"

HKR,,Channel,0,"10"

[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"

HKR,,BWSetting,0,"0"

HKR,,Channel,0,"10"

[11acWirelessMode.reg]
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

HKR,,Channel,0,"36"
HKR,,RFType,0,"5"

HKR,defaults,BWSetting,0,"2"
HKR,,BWSetting,0,"2"

;;----------------------------------------------------------------------------
;; Wake on Wlan mode option parameters
;;----------------------------------------------------------------------------
[WoWModeOnn.reg]
;;HKR,Ndi\params\WoWLANMode, 		ParamDesc, 	0, %WOW_MODE_STR%
;;HKR,Ndi\params\WoWLANMode, 		type, 		0, "enum"
;;HKR,Ndi\params\WoWLANMode, 		default, 	0, "1"
;;HKR,Ndi\params\WoWLANMode\enum, 	"0", 		0, %WOW_DISABLE%
;;HKR,Ndi\params\WoWLANMode\enum, 	"1", 		0, %WOW_ENABLE_MAGIC_PKT%
;;HKR,Ndi\params\WoWLANMode\enum, 	"2", 		0, %WOW_ENABLE_PATTERN_PKT%
;;HKR,Ndi\params\WoWLANMode\enum, 	"3", 		0, %WOW_ENABLE_MAGIC_PATTERN_PKT%
HKR,defaults,WoWLANMode, 0, "1"
HKR,,WoWLANMode, 0, "1"

; ARP Offload
HKR,,ARPOffloadEnable, 0, "1"

; GTK Offload
HKR,,GTKOffloadEnable, 0, "1"

[WoWModeOff.reg]
;;HKR,Ndi\params\WoWLANMode, 		ParamDesc, 	0, %WOW_MODE_STR%
;;HKR,Ndi\params\WoWLANMode, 		type, 		0, "enum"
;;HKR,Ndi\params\WoWLANMode, 		default, 	0, "0"
;;HKR,Ndi\params\WoWLANMode\enum, 	"0", 		0, %WOW_DISABLE%
;;HKR,Ndi\params\WoWLANMode\enum, 	"1", 		0, %WOW_ENABLE_MAGIC_PKT%
;;HKR,Ndi\params\WoWLANMode\enum, 	"2", 		0, %WOW_ENABLE_PATTERN_PKT%
;;HKR,Ndi\params\WoWLANMode\enum, 	"3", 		0, %WOW_ENABLE_MAGIC_PATTERN_PKT%
HKR,defaults,WoWLANMode, 0, "0"
HKR,,WoWLANMode, 0, "0"


;;----------------------------------------------------------------------------
;; Usb selective suspend parameters
;;----------------------------------------------------------------------------
[NdisSS.reg]
HKR,Ndi\params\*SelectiveSuspend,	    ParamDesc,  0, %SelectiveSuspend%
HKR,Ndi\params\*SelectiveSuspend,	    default,    0, "1"
HKR,Ndi\params\*SelectiveSuspend,	    type,       0, "enum"
HKR,Ndi\params\*SelectiveSuspend\enum,   "0",        0, "Disabled"
HKR,Ndi\params\*SelectiveSuspend\enum,   "1",        0, "Enabled"

HKR,Ndi\params\*SSIdleTimeout,	    ParamDesc,  0, %SSIdleTimeout%
HKR,Ndi\params\*SSIdleTimeout,	    type,       0, "int"
HKR,Ndi\params\*SSIdleTimeout,	    default,    0, "10"
HKR,Ndi\Params\*SSIdleTimeout,      Max,        0, "60"
HKR,Ndi\Params\*SSIdleTimeout,      Min,        0, "5"
HKR,Ndi\Params\*SSIdleTimeout,      Step,       0, "1"


;*******************************************************************************
; Two STA Concurrent Mode Reg
;*******************************************************************************
[ConcurrentMode.reg]
HKR,Ndi\params\TwoStaConcurrentMode,		ParamDesc,  0, %TWO_STA_CONCURRENT_MODE%
HKR,Ndi\params\TwoStaConcurrentMode,		type,       0, "enum"
HKR,Ndi\params\TwoStaConcurrentMode,			default,    0, "1"
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"0",        0, %SECONDARY_DISABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"1",        0, %SECONDARY_ENABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"2",        0, %SECONDARY_AUTO%
HKR,defaults,TwoStaConcurrentMode,0,"0"
HKR,,TwoStaConcurrentMode,0,"0"

;*******************************************************************************
; bandwidth setting
;*******************************************************************************
[2G40MHzAnd5G40MHz.reg]
HKR,Ndi\params\BW40MHzFor2G,        ParamDesc,  0, "Bandwidth_2.4G"
HKR,Ndi\params\BW40MHzFor2G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor2G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor2G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor2G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,,"1"

HKR,Ndi\params\BW40MHzFor5G,        ParamDesc,  0, "Bandwidth_5G"
HKR,Ndi\params\BW40MHzFor5G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor5G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor5G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor5G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,,"1"

[2G20MHzAnd5G40MHz.reg]
HKR,defaults,BW40MHzFor2G,0,"0"
HKR,,BW40MHzFor2G,0,"0"

HKR,Ndi\params\BW40MHzFor5G,        ParamDesc,  0, "Bandwidth_5G"
HKR,Ndi\params\BW40MHzFor5G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor5G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor5G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor5G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,,"1"

[2G20MHzAnd5G20MHz.reg]
HKR,defaults,BW40MHzFor2G,0,"0"
HKR,,BW40MHzFor2G,0,"0"

HKR,defaults,BW40MHzFor5G,0,"0"
HKR,,BW40MHzFor5G,0,"0"

[BandWidthSetting.reg]
;; 40MHz Support in 11n
HKR,Ndi\params\BWSetting,        ParamDesc,  0, "Bandwidth"
HKR,Ndi\params\BWSetting,        type,       0, "enum"
HKR,Ndi\params\BWSetting,        default,    0, "1"
HKR,Ndi\params\BWSetting\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BWSetting\enum,   "1",        0, "20_40MHz"
HKR,defaults,BWSetting,0,"1"
HKR,,BWSetting,0,"1"
HKR,,BWSetting,,"1"

[BelkinCustomId.reg]
HKR,,CustomerID,0,"21"
HKR,,CustomerID,,"21"

[BandSet.reg]
HKR,Ndi\params\WirelessBand,			ParamDesc,  0, "Disable Bands"
HKR,Ndi\params\WirelessBand,			type,       0, "enum"
HKR,Ndi\params\WirelessBand,			default,    0, "0"
HKR,Ndi\params\WirelessBand\enum,		"0",        0, "Disable 11A"
HKR,Ndi\params\WirelessBand\enum,		"1",        0, "Disable 11B/G"
HKR,Ndi\params\WirelessBand\enum,		"2",        0, "None"
HKR,defaults,WirelessBand,0,"2"
HKR,,WirelessBand,0,"2"

[BandOnly5G.reg]
HKR,defaults,WirelessBand,0,"1"
HKR,,WirelessBand,0,"1"

;*****************************************************************************
; 92DU VS open EDCCA 
;*****************************************************************************
[EDCCASupport.reg]
HKR,defaults,EdccaSupport,0,"0"
HKR,,EdccaSupport,0,"0"

;;----------------------------------------------------------------------------
;; 8811AU/8821AU WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTL8811AU_COMMON.reg]
HKR,,EnableTxPowerLimit,0,"0"
HKR,,RFPathS1,0,"0"
HKR,,StbcCap,0,"17"

HKR,defaults,UsbTxAggDescNum,0,"10"
HKR,,UsbTxAggDescNum,0,"10"
HKR,,PwrByRateFile,0,"PHY_REG_PG.txt"
HKR,,PwrLimitFile,0,"TXPWR_LMT.txt"

HKR,defaults,LdpcCap,0,"0"
HKR,,LdpcCap,0,"0"
HKR,,LdpcCap,,"0"

;; Antenna Diversity Type
HKR,Ndi\params\Ant5GSelect, 	default, 	0, "0"
HKR,Ndi\params\Ant5GSelect,	ParamDesc, 	0, "5G Antenna Select"
HKR,Ndi\params\Ant5GSelect, 		    type, 		    0, "enum"
HKR,Ndi\params\Ant5GSelect\enum,   	"0",        	0, "Auto"
HKR,Ndi\params\Ant5GSelect\enum,   	"1",        	0, "Main"
HKR,Ndi\params\Ant5GSelect\enum,   	"2",        	0, "Aux"

;*******************************************************************************
; Destination Directory
;*******************************************************************************
[RTWlanU.CopyFiles]
RTWlanU.sys,,,2

[DestinationDirs]
DefaultDestDir     	= 11
RTWlanU.CopyFiles	= 12


;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksFiles]
RTWlanU.sys = 1

[SourceDisksNames]
1=%DISKNAME%,,,


;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
SSID_STR					= "SSID"
CHANNEL_STR					= "Channel"
NETWORK_TYPE_STR			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR						= "QoS"
WiFiConfg_STR	  			= "WiFiConfg"
WMM_APSD					= "WMM APSD"
CCX_RM_STR					= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR			= "Forced Priority"
HW_PARA_STR					= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR						= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
DISABLE_STR					= "Disable"
ENABLE_STR					= "Enable"
AD_HOC_STR					= "Ad Hoc"
INFRASTRUCTURE_STR			= "Infrastructure"
AUTO_SELECT					= "Auto select"
WL_MODE_STR					= "Wireless Mode"
RX_REORDER_STR				= "Rx Reorder"
CAM_STR						= "CAM"
MAX_PSP_STR					= "MAX_PSP"
Fast_PSP_STR				= "Fast_PSP"
NO_AC_STR					= "No AC (Disable)"
ALL_AC_STR					= "ALL AC"
AUTO_STR 				= "Auto"
IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
SelectiveSuspend               		= "Selective suspend"
SSIdleTimeout                  		= "Selective suspend Timeout"

TX_PWR_CONTROL_STR		= "送信出力"
TX_PWR_PERCENTAGE_1_STR 	= "12.5%"
TX_PWR_PERCENTAGE_2_STR 	= "25%"
TX_PWR_PERCENTAGE_3_STR 	= "50%"
TX_PWR_PERCENTAGE_4_STR 	= "100%"
STREAM_MODE_STR			= "ストリーミングモード"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation strings
;-------------------------------------------------------------------------------
RX_AGG_MODE_STR				= "Rx Aggregation Mode"
RX_AGG_MODE_BLOCK_STR		= "Rx Agg USB Block Mode"
RX_AGG_MODE_PAGE_STR		= "Rx Agg DMA Page Mode"
RX_AGG_MODE_MIXED_STR		= "Rx Agg USB and Page Mixed Mode"
RX_AGG_USB_BLOCK_STR		= "Rx Agg USB Block Threshold"
RX_AGG_USB_TIMEOUT_STR		= "Rx Agg USB Timeout"
RX_AGG_DMA_PAGE_STR			= "Rx Agg DMA Page Threshold"
RX_AGG_DMA_TIMEOUT_STR		= "Rx Agg DMA Timeout"
TX_AGG_MODE_STR				= "Tx Aggregation Mode"
TX_AGG_DESC_PER_OUT_STR		= "Tx Agg Number of descriptor per bulk out"

;-------------------------------------------------------------------------------
;	Two STA Concurrent Mode
;-------------------------------------------------------------------------------
TWO_STA_CONCURRENT_MODE		= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"


;*******************************************************************************
; manufacture description
;*******************************************************************************
DLink					= "D-Link Corporation"

;*******************************************************************************
;	Source disk name
;*******************************************************************************
;DISKNAME							= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
DISKNAME							= "Realtek Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
DLink-DWA171.DeviceDesc                      	= "D-Link DWA-171 Wireless AC Dual Band Adapter"
DLink-DWA171.DeviceDesc.DispName               = "D-Link DWA-171 Wireless AC Dual Band Adapter"