;; net8187b.inf (For Win 7)
;;
;; Realtek RTL8187B Wireless 802.11g 54Mbps USB 2.0 Network Adapter
;;
;; Copyright (C) 2010 Realtek Semiconductor Corp.
;;
;; this release is primarily for WHQL test.
;;

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %Realtek%
CatalogFile.NT	= net8187b.cat		;; for WHQL certified
DriverVer	= 03/31/2010,62.1182.0331.2010

[Manufacturer]
%Realtek% = Realtek,NTx86.6.1

[ControlFlags]
ExcludeFromSelect = USB\VID_0BDA&PID_8187&REV_0200

;;****************************************************************************
;; IDs for X86
;;****************************************************************************
[Realtek.NTx86.6.1]
%RTL8187B.DeviceDesc% = RTL8187B.ndi, USB\VID_0BDA&PID_8187&REV_0200
%RTL8187B.DeviceDesc% = RTL8187B.ndi, USB\VID_0BDA&PID_8189&REV_0200
%RTL8187B.DeviceDesc% = RTL8187B.ndi, USB\VID_0BDA&PID_8197&REV_0200
%RTL8187B.DeviceDesc% = RTL8187B.ndi, USB\VID_0BDA&PID_8198&REV_0200
%RTL8187B.DeviceDesc% = RTL8187B.ndi, USB\VID_0BDA&PID_8199&REV_0200

;;****************************************************************************
;; IDs for X64
;;****************************************************************************
[Realtek.NTamd64.6.1]
%RTL8187B.DeviceDesc% = RTL8187B.ndi, USB\VID_0BDA&PID_8187&REV_0200
%RTL8187B.DeviceDesc% = RTL8187B.ndi, USB\VID_0BDA&PID_8189&REV_0200
%RTL8187B.DeviceDesc% = RTL8187B.ndi, USB\VID_0BDA&PID_8197&REV_0200
%RTL8187B.DeviceDesc% = RTL8187B.ndi, USB\VID_0BDA&PID_8198&REV_0200
%RTL8187B.DeviceDesc% = RTL8187B.ndi, USB\VID_0BDA&PID_8199&REV_0200

;;****************************************************************************
;; Windows 2000/XP
;;****************************************************************************
[RTL8187B.ndi.NT]
AddReg          	= RTL8187B.common.reg, RTLWLAN.reg, RTL8187B_os61.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTL8187B.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8187B.ndi.NT.Services]
AddService		= RTL8187B, 2, RTL8187B.nt61.Service, RTL8187B.nt61.EventLog

[RTL8187B.ndi.NT.HW]
AddReg = RTL8187B_os61.vwifi.reg

;;****************************************************************************
;; register for both Win 7 x86 and x64              			**
;;****************************************************************************
[RTL8187B_os61.reg]
HKR, Ndi,				Service,    0, "RTL8187B"
HKR, Ndi\Interfaces,                	UpperRange, 0, "ndis5,mdcwifi,wifipro"
HKR, Ndi\Interfaces,                	LowerRange, 0, "wlan,ethernet,vwifi"

[RTL8187B.nt61.Service]
DisplayName     = %RTL8187B.DeviceDesc.DispName%
ServiceType     = 1 		;SERVICE_KERNEL_DRIVER
StartType       = 3 		;SERVICE_DEMAND_START
ErrorControl    = 1 		;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\rtl8187B.sys
LoadOrderGroup  = NDIS

[RTL8187B.nt61.EventLog]
AddReg = RTL8187B.nt61.AddEventLog.reg

[RTL8187B.nt61.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

;; Adds the VWiFi PNP filter
[RTL8187B_os61.vwifi.reg]
HKR,,"UpperFilters",0x00010000,"vwifibus"


;*******************************************************************************
; RTL8187B common paramters
;*******************************************************************************
[RTL8187B.common.reg]
;HKR,Ndi\params\LedCtrl,        ParamDesc,  0, %LED_CONTROL_STR%
;HKR,Ndi\params\LedCtrl,        type,       0, "enum"
;HKR,Ndi\params\LedCtrl,        default,    0, "1"
;HKR,Ndi\params\LedCtrl\enum,   "0",        0, %Disable_STR%
;HKR,Ndi\params\LedCtrl\enum,   "1",        0, %ENABLE_STR%
;HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

;HKR,NDI\params\PowerSaveMode,      ParamDesc,  0, %POWER_SAVE_STR%
;HKR,NDI\params\PowerSaveMode,      type,       0, "enum"
;HKR,Ndi\params\PowerSaveMode,      default,    0, "0"
;HKR,NDI\params\PowerSaveMode\enum, "0",        0, %CAM_STR%
;HKR,NDI\params\PowerSaveMode\enum, "1",        0, %MAX_PSP_STR%
;HKR,NDI\params\PowerSaveMode\enum, "2",        0, %FAST_PSP_STR%
;HKR,defaults,PowerSaveMode,0,"0"
HKR,,PowerSaveMode,0,"0"

;HKR,Ndi\params\WiFi11bIbss,        ParamDesc,  0, %WIFI_IBSS_STR%
;HKR,Ndi\params\WiFi11bIbss,        type,       0, "enum"
;HKR,Ndi\params\WiFi11bIbss,        default,    0, "0"
;HKR,Ndi\params\WiFi11bIbss\enum,   "0",        0, %DISABLE_STR%
;HKR,Ndi\params\WiFi11bIbss\enum,   "1",        0, %ENABLE_STR%
;HKR,defaults,WiFi11bIbss,0,"0"
HKR,,WiFi11bIbss,0,"0"

;HKR,Ndi\params\bRateAdaptive,        ParamDesc,  0, %RATE_ADAPTIVE_STR%
;HKR,Ndi\params\bRateAdaptive,        type,       0, "enum"
;HKR,Ndi\params\bRateAdaptive,        default,    0, "1"
;HKR,Ndi\params\bRateAdaptive\enum,   "0",        0, %DISABLE_STR%
;HKR,Ndi\params\bRateAdaptive\enum,   "1",        0, %ENABLE_STR%
;HKR,defaults,bRateAdaptive,0,"1"
HKR,,bRateAdaptive,0,"1"

;HKR,Ndi\params\QoS,        ParamDesc,  0, %QOS_STR%
;HKR,Ndi\params\QoS,        type,       0, "enum"
;HKR,Ndi\params\QoS,        default,    0, "0"
;HKR,Ndi\params\QoS\enum,   "0",        0, %DISABLE_STR%
;HKR,Ndi\params\QoS\enum,   "1",        0, %ENABLE_STR%
;HKR,defaults,QoS,0,"0"
HKR,,QoS,0,"0"

HKR,,CcxRm,0,"0"

;;----------------------------------------------------------------------------
;; Realtek WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,,SSID,0,""

;HKR,Ndi\params\Channel,       ParamDesc,  0, %CHANNEL_STR%
;HKR,Ndi\params\Channel,       type,       0, "int"
;HKR,Ndi\params\Channel,       default,    0, "1"
;HKR,Ndi\params\Channel,       Min,        0, "1"
;HKR,Ndi\params\Channel,       Max,        0, "14"
;HKR,Ndi\params\Channel,       Step,       0, "1"
;HKR,Ndi\params\Channel,       Base,       0, "10"
;HKR,defaults,Channel,0,"10"
HKR,,Channel,0,"10"

;HKR,Ndi\params\NetworkType,        ParamDesc,  0, %NETWORK_TYPE_STR%
;HKR,Ndi\params\NetworkType,        type,       0, "enum"
;HKR,Ndi\params\NetworkType,        default,    0, "1"
;HKR,Ndi\params\NetworkType\enum,   "0",        0, %AD_HOC_STR%
;HKR,Ndi\params\NetworkType\enum,   "1",        0, %INFRA_STR%
;HKR,Ndi\params\NetworkType\enum,   "2",        0, %AUTO_SELECT_STR%
;HKR,defaults,NetworkType,0,"1"
HKR,,NetworkType,0,"1"

;HKR,Ndi\params\WirelessMode, ParamDesc, 0, %WL_MODE_STR%
;HKR,Ndi\params\WirelessMode, type, 0, "enum"
;HKR,Ndi\params\WirelessMode, default, 0, "4"
;HKR,Ndi\params\WirelessMode\enum, "1", 0, %11A_STR%
;HKR,Ndi\params\WirelessMode\enum, "2", 0, %11B_STR%
;HKR,Ndi\params\WirelessMode\enum, "4", 0, %11BG_STR%
;HKR,Ndi\params\WirelessMode\enum, "8", 0, %AUTO_STR%
;HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"

; Preamble mode, 2006.11.30, by shien chang.
;HKR,Ndi\params\PreambleMode, ParamDesc, 0, %PREAMBLE_MODE_STR%
;HKR,Ndi\params\PreambleMode, type, 0, "enum"
;HKR,Ndi\params\PreambleMode, default, 0, "2"
;HKR,Ndi\params\PreambleMode\enum, "1", 0, %LONG_PREAMBLE_STR%
;HKR,Ndi\params\PreambleMode\enum, "2", 0, %AUTO_STR%
;HKR,Ndi\params\PreambleMode\enum, "3", 0, %SHORT_PREAMBLE_STR%
;HKR,defaults,PreambleMode, 0, "2"
HKR,,PreambleMode, 0, "2"

HKR,Ndi\params\FragThresh, ParamDesc, 0, %FRAGTHRESH_STR%
HKR,Ndi\params\FragThresh, default, 0, "2346"
HKR,Ndi\params\FragThresh, type, 0, "int"
HKR,Ndi\params\FragThresh, min, 0, "256"
HKR,Ndi\params\FragThresh, max, 0, "2346"
HKR,Ndi\params\FragThresh, step, 0, "1"
HKR,defaults,FragThresh, 0, "2346"
HKR,,FragThresh, 0, "2346"

HKR,Ndi\params\RTSThresh, ParamDesc, 0, %RTSTHRESH_STR%
HKR,Ndi\params\RTSThresh, default, 0, "2347"
HKR,Ndi\params\RTSThresh, type, 0, "int"
HKR,Ndi\params\RTSThresh, min, 0, "0"
HKR,Ndi\params\RTSThresh, max, 0, "2347"
HKR,Ndi\params\RTSThresh, step, 0, "1"
HKR,defaults,RTSThresh, 0, "2347"
HKR,,RTSThresh, 0, "2347"

HKR,Ndi\params\Dot11dEnable,        ParamDesc,  0, %DOT11_ENABLE_STR%
HKR,Ndi\params\Dot11dEnable,        type,       0, "enum"
HKR,Ndi\params\Dot11dEnable,        default,    0, "0"
HKR,Ndi\params\Dot11dEnable\enum,   "0",        0, %Disable_STR%
HKR,Ndi\params\Dot11dEnable\enum,   "1",        0, %Enable_STR%
HKR,defaults,Dot11dEnable,0,"0"
HKR,,Dot11dEnable,0,"0"

;Inactive Power Save
HKR,,bInactivePs,0,"1"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;*******************************************************************************
; Destination Directory
;*******************************************************************************
[RTL8187B.CopyFiles]
RTL8187B.sys,,,2

[DestinationDirs]
DefaultDestDir     = 11
RTL8187B.CopyFiles		= 12

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksFiles]
RTL8187B.sys = 1

[SourceDisksNames]
1=%DISKNAME%,,,

;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
Realtek 			= "Realtek Semiconductor Corp."
SSID_STR			= "SSID"
CHANNEL_STR			= "Channel"
NETWORK_TYPE_STR		= "Network Type"
LED_CONTROL_STR			= "LED Control" 
POWER_SAVE_STR			= "Power Save Mode"
WIFI_IBSS_STR			= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR		= "Rate Adaptive"
QOS_STR				= "QoS"
TransmitBuffers              	= "Transmit Buffers"
ReceiveBuffers               	= "Receive Buffers"
FORCE_PRIORITY_STR		= "Forced Priority"
HW_PARA_STR			= "Init from HwParaFile"
THREE_WIRE_MODE_STR		= "Three Wire Programming Mode"
BOARD_TYPE_STR			= "Board Type"
PROTECTION_MODE_STR		= "Protection Mode"
TPC_STR				= "Transmit Power Control"
TPC_POLARITY_STR		= "TPC Polarity Select"
HIGH_POWER_STR			= "High Power Mechanism"
INIT_GAIN_STR			= "Initial Gain State"
CW_MAX_MIN_STR			= "Contention Window"
PSP_XLINK_STR			= "PSP XLink Mode"
ANTENNA_DIVERSITY_STR		= "SW Antenna Diversity"
INACTIVE_POWER_SAVE		= "Inactive Power Save"
B_MODE_INIT_GAIN_STR		= "B Mode Initial Gain"
WL_MODE_STR			= "Wireless Mode"
PREAMBLE_MODE_STR		= "Preamble Mode"
FRAGTHRESH_STR			= "Fragmentation Threshold"
RTSTHRESH_STR			= "RTS Threshold"
DOT11_ENABLE_STR		= "802.11d"
CAM_STR				= "CAM"
MAX_PSP_STR			= "MAX_PSP"
FAST_PSP_STR			= "Fast_PSP"
DISABLE_STR			= "Disable"
ENABLE_STR			= "Enable"
AD_HOC_STR			= "Ad Hoc"
INFRA_STR			= "Infrastructure"
AUTO_SELECT_STR			= "Auto select"
11A_STR				= "IEEE 802.11 a"
11B_STR				= "IEEE 802.11 b"
11BG_STR			= "IEEE 802.11 b/g"
LONG_PREAMBLE_STR		= "Long Preamble"
SHORT_PREAMBLE_STR		= "Short Preamble"
AUTO_STR			= "Auto"

;; Source disk name
DISKNAME			= "Realtek RTL8187B Wireless 802.11b/g 54Mbps USB 2.0 Network Adapter Driver Disk"
RTL8187B.DeviceDesc 		= "Realtek RTL8187B Wireless 802.11b/g 54Mbps USB 2.0 Network Adapter"
RTL8187B.DeviceDesc.DispName	= "Realtek RTL8187B Wireless 802.11b/g 54Mbps USB 2.0 Network Adapter"

