;****************************************************************************************************
; Netwbn02.INF
;
;Mini PCI Express INF
;
; Intel Wireless WiFi Link Adapters
; Installation Script for Windows Blue 32 bit
;
; Copyright (C) 1997-2011 Intel Corporation. All rights reserved.
;
; The information and source code contained herein is the exclusive
; property of Intel Corporation and may not be disclosed, examined
; or reproduced in whole or in part without explicit written authorization
; from the company.
;
;------------------------------------------------------------------------------

;******************************************************************************
; Version Section
;------------------------------------------------------------------------------
[version]
Signature   = "$Windows NT$"
Compatible  = 1
Class       = net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %PROVIDER_NAME%
DriverVer   = 08/23/2015,18.20.0.9 ;DATE HAS TO BE IN FOLLOWING FORMAT MM/DD/YYYY

CatalogFile = Netwbn02.cat


;****************************************************************************************************
; Manufacturer
;----------------------------------------------------------------------------------------------------

[Manufacturer]
%COMPANY_NAME% = Device, NTx86.6.3

;[ControlFlags]
;ExcludeFromSelect = \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_40208086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_402A8086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_40608086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_40628086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_406A8086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_40708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_40728086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_41608086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_41628086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_41708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_44208086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_44608086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_44628086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_446A8086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_44708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_44728086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_45608086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_45708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_486E8086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_48708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_4A6C8086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_4A6E8086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_4A708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_4C608086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_4C708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_50708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_50728086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_51708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_57708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C0208086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C02A8086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C0608086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C0628086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C06A8086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C0708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C0728086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C1608086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C1628086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C1708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C3608086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C4208086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C4608086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C4628086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C4708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C4728086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C5608086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C5708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C7608086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_C7708086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_CC608086 , \ 
;        PCI\VEN_8086&DEV_08B1&SUBSYS_CC708086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_42208086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_42608086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_42628086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_426A8086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_42708086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_42728086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_43608086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_43708086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_C2208086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_C2608086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_C2628086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_C26A8086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_C2708086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_C2728086 , \ 
;        PCI\VEN_8086&DEV_08B2&SUBSYS_C3708086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_00608086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_00628086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_00708086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_00728086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_01708086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_01728086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_04708086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_04728086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_10708086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_11708086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_80608086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_80628086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_80708086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_80728086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_81708086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_81728086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_84708086 , \ 
;        PCI\VEN_8086&DEV_08B3&SUBSYS_85708086 , \ 
;        PCI\VEN_8086&DEV_08B4&SUBSYS_02608086 , \ 
;        PCI\VEN_8086&DEV_08B4&SUBSYS_02708086 , \ 
;        PCI\VEN_8086&DEV_08B4&SUBSYS_02728086 , \ 
;        PCI\VEN_8086&DEV_08B4&SUBSYS_03708086 , \ 
;        PCI\VEN_8086&DEV_08B4&SUBSYS_82608086 , \ 
;        PCI\VEN_8086&DEV_08B4&SUBSYS_82708086 , \ 
;        PCI\VEN_8086&DEV_08B4&SUBSYS_82728086 , \ 
;        PCI\VEN_8086&DEV_08B4&SUBSYS_83708086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_10108086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50008086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50028086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_500A8086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50108086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50128086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50208086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_502A8086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_50908086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_51008086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_51028086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_51108086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_51908086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54008086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54108086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54128086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54208086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_54908086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_55108086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_55908086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_5C108086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_5F108086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_90008086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_900A8086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_90108086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_90128086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_91108086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_94008086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_94108086 , \ 
;        PCI\VEN_8086&DEV_095A&SUBSYS_95108086 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52008086 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52028086 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_520A8086 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52108086 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52128086 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_52908086 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_53028086 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_53108086 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_92008086 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_92108086 , \ 
;        PCI\VEN_8086&DEV_095B&SUBSYS_93108086 , \ 
;        PCI\VEN_8086&DEV_3165&SUBSYS_40108086 , \ 
;        PCI\VEN_8086&DEV_3165&SUBSYS_40128086 , \ 
;        PCI\VEN_8086&DEV_3165&SUBSYS_41108086 , \ 
;        PCI\VEN_8086&DEV_3165&SUBSYS_44108086 , \ 
;        PCI\VEN_8086&DEV_3165&SUBSYS_45108086 , \ 
;        PCI\VEN_8086&DEV_3165&SUBSYS_80108086 , \ 
;        PCI\VEN_8086&DEV_3165&SUBSYS_81108086 , \ 
;        PCI\VEN_8086&DEV_3166&SUBSYS_42108086 , \ 
;        PCI\VEN_8086&DEV_3166&SUBSYS_42128086 , \ 
;        PCI\VEN_8086&DEV_3166&SUBSYS_43108086 , \ 

;****************************************************************************************************
;Device
;****************************************************************************************************

;****************************************************************************************************
;Device WINB
;----------------------------------------------------------------------------------------------------
[Device.NTx86.6.3]

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENNBT_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_40208086 ; AGN

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENNBT_7260_AGN_2x2_HMC_WINB_AGN15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_402A8086 ; AGN15

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GEN_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_40608086 ; AGN

%NIC_7260BGN_2x2_HMC% = Install_MPCIEX_GEN_7260_BGN_2x2_HMC_WINB_BGN15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_40628086 ; BGN15

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GEN_7260_AGN_2x2_HMC_WINB_AGN15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_406A8086 ; AGN15

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GEN_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_40708086 ; AC

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GEN_7260_AC_2x2_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_40728086 ; AC15

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENSAR_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_41608086 ; AGN

%NIC_7260BGN_2x2_HMC% = Install_MPCIEX_GENSAR_7260_BGN_2x2_HMC_WINB_BGN15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_41628086 ; BGN15

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GENSAR_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_41708086 ; AC

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_DELLNBT_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_44208086 ; AGN

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_DELL_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_44608086 ; AGN

%NIC_7260BGN_2x2_HMC% = Install_MPCIEX_DELL_7260_BGN_2x2_HMC_WINB_BGN15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_44628086 ; BGN15

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_DELL_7260_AGN_2x2_HMC_WINB_AGN15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_446A8086 ; AGN15

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_DELL_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_44708086 ; AC

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_DELL_7260_AC_2x2_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_44728086 ; AC15

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_DELLSAR_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_45608086 ; AGN

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_DELLSAR_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_45708086 ; AC

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_IM1_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_486E8086 ; AC

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_IM2_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_48708086 ; AC

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_AUTO_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_4A6C8086 ; AC

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_AUTO1_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_4A6E8086 ; AC

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_AUTO2_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_4A708086 ; AC

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_ASUS_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_4C608086 ; AGN

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_ASUS_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_4C708086 ; AC

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GENSD_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_50708086 ; AC

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GENSD_7260_AC_2x2_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_50728086 ; AC15

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GENSARSD_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_51708086 ; AC

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_SAMSARSD_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_57708086 ; AC

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENNGFFNBT_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C0208086 ; AGN

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENNGFFNBT_7260_AGN_2x2_HMC_WINB_AGN15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C02A8086 ; AGN15

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENNGFF_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C0608086 ; AGN

%NIC_7260BGN_2x2_HMC% = Install_MPCIEX_GENNGFF_7260_BGN_2x2_HMC_WINB_BGN15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C0628086 ; BGN15

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENNGFF_7260_AGN_2x2_HMC_WINB_AGN15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C06A8086 ; AGN15

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GENNGFF_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C0708086 ; AC

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GENNGFF_7260_AC_2x2_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C0728086 ; AC15

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENSARNGFF_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C1608086 ; AGN

%NIC_7260BGN_2x2_HMC% = Install_MPCIEX_GENSARNGFF_7260_BGN_2x2_HMC_WINB_BGN15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C1628086 ; BGN15

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GENSARNGFF_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C1708086 ; AC

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENUISARNGFF_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C3608086 ; AGN

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_DELLNGFFNBT_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C4208086 ; AGN

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_DELLNGFF_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C4608086 ; AGN

%NIC_7260BGN_2x2_HMC% = Install_MPCIEX_DELLNGFF_7260_BGN_2x2_HMC_WINB_BGN15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C4628086 ; BGN15

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_DELLNGFF_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C4708086 ; AC

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_DELLNGFF_7260_AC_2x2_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C4728086 ; AC15

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_DELLSARNGFF_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C5608086 ; AGN

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_DELLSARNGFF_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C5708086 ; AC

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_SAMSARNGFF_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C7608086 ; AGN

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_SAMSARNGFF_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_C7708086 ; AC

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_ASUSNGFF_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_CC608086 ; AGN

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_ASUSNGFF_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B1&SUBSYS_CC708086 ; AC

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENUINBT_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_42208086 ; AGN

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENUI_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_42608086 ; AGN

%NIC_7260BGN_2x2_HMC% = Install_MPCIEX_GENUI_7260_BGN_2x2_HMC_WINB_BGN15    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_42628086 ; BGN15

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENUI_7260_AGN_2x2_HMC_WINB_AGN15    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_426A8086 ; AGN15

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GENUI_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_42708086 ; AC

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GENUI_7260_AC_2x2_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_42728086 ; AC15

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENUISAR_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_43608086 ; AGN

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GENUISAR_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_43708086 ; AC

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENUINGFFNBT_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_C2208086 ; AGN

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENUINGFF_7260_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_C2608086 ; AGN

%NIC_7260BGN_2x2_HMC% = Install_MPCIEX_GENUINGFF_7260_BGN_2x2_HMC_WINB_BGN15    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_C2628086 ; BGN15

%NIC_7260AGN_2x2_HMC% = Install_MPCIEX_GENUINGFF_7260_AGN_2x2_HMC_WINB_AGN15    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_C26A8086 ; AGN15

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GENUINGFF_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_C2708086 ; AC

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GENUINGFF_7260_AC_2x2_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_C2728086 ; AC15

%NIC_7260AC_2x2_HMC% = Install_MPCIEX_GENUISARNGFF_7260_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B2&SUBSYS_C3708086 ; AC

%NIC_3160AGN_HMC% = Install_MPCIEX_GEN_3160_AGN_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_00608086 ; AGN

%NIC_3160BGN_HMC% = Install_MPCIEX_GEN_3160_BGN_HMC_WINB_BGN15    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_00628086 ; BGN15

%NIC_3160AC_HMC% = Install_MPCIEX_GEN_3160_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_00708086 ; AC

%NIC_3160AC_HMC% = Install_MPCIEX_GEN_3160_AC_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_00728086 ; AC15

%NIC_3160AC_HMC% = Install_MPCIEX_GENSAR_3160_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_01708086 ; AC

%NIC_3160AC_HMC% = Install_MPCIEX_GENSAR_3160_AC_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_01728086 ; AC15

%NIC_3160AC_HMC% = Install_MPCIEX_DELL_3160_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_04708086 ; AC

%NIC_3160AC_HMC% = Install_MPCIEX_DELL_3160_AC_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_04728086 ; AC15

%NIC_3160AC_HMC% = Install_MPCIEX_GENSD_3160_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_10708086 ; AC

%NIC_3160AC_HMC% = Install_MPCIEX_GENSARSD_3160_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_11708086 ; AC

%NIC_3160AGN_HMC% = Install_MPCIEX_GENNGFF_3160_AGN_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_80608086 ; AGN

%NIC_3160BGN_HMC% = Install_MPCIEX_GENNGFF_3160_BGN_HMC_WINB_BGN15    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_80628086 ; BGN15

%NIC_3160AC_HMC% = Install_MPCIEX_GENNGFF_3160_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_80708086 ; AC

%NIC_3160AC_HMC% = Install_MPCIEX_GENNGFF_3160_AC_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_80728086 ; AC15

%NIC_3160AC_HMC% = Install_MPCIEX_GENSARNGFF_3160_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_81708086 ; AC

%NIC_3160AC_HMC% = Install_MPCIEX_GENSARNGFF_3160_AC_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_81728086 ; AC15

%NIC_3160AC_HMC% = Install_MPCIEX_DELLNGFF_3160_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_84708086 ; AC

%NIC_3160AC_HMC% = Install_MPCIEX_DELLSARNGFF_3160_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B3&SUBSYS_85708086 ; AC

%NIC_3160AGN_HMC% = Install_MPCIEX_GENUI_3160_AGN_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B4&SUBSYS_02608086 ; AGN

%NIC_3160AC_HMC% = Install_MPCIEX_GENUI_3160_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B4&SUBSYS_02708086 ; AC

%NIC_3160AC_HMC% = Install_MPCIEX_GENUI_3160_AC_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_08B4&SUBSYS_02728086 ; AC15

%NIC_3160AC_HMC% = Install_MPCIEX_GENUISAR_3160_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B4&SUBSYS_03708086 ; AC

%NIC_3160AGN_HMC% = Install_MPCIEX_GENUINGFF_3160_AGN_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_08B4&SUBSYS_82608086 ; AGN

%NIC_3160AC_HMC% = Install_MPCIEX_GENUINGFF_3160_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B4&SUBSYS_82708086 ; AC

%NIC_3160AC_HMC% = Install_MPCIEX_GENUINGFF_3160_AC_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_08B4&SUBSYS_82728086 ; AC15

%NIC_3160AC_HMC% = Install_MPCIEX_GENUISARNGFF_3160_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_08B4&SUBSYS_83708086 ; AC

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GEN_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_10108086 ; AC

%NIC_7265AGN_2x2_HMC% = Install_MPCIEX_GENM2_7265_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50008086 ; AGN

%NIC_7265BGN_2x2_HMC% = Install_MPCIEX_GENM2_7265_BGN_2x2_HMC_WINB_BGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50028086 ; BGN15

%NIC_7265AGN_2x2_HMC% = Install_MPCIEX_GENM2_7265_AGN_2x2_HMC_WINB_AGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_500A8086 ; AGN15

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GENM2_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50108086 ; AC

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GENM2_7265_AC_2x2_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50128086 ; AC15

%NIC_7265AGN_2x2_HMC% = Install_MPCIEX_GENM2NBT_7265_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50208086 ; AGN

%NIC_7265AGN_2x2_HMC% = Install_MPCIEX_GENM2NBT_7265_AGN_2x2_HMC_WINB_AGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_502A8086 ; AGN15

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GENM2WG_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_50908086 ; AC

%NIC_7265AGN_2x2_HMC% = Install_MPCIEX_GENSARM2_7265_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_51008086 ; AGN

%NIC_7265BGN_2x2_HMC% = Install_MPCIEX_GENSARM2_7265_BGN_2x2_HMC_WINB_BGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_51028086 ; BGN15

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GENSARM2_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_51108086 ; AC

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GENSARM2WG_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_51908086 ; AC

%NIC_7265AGN_2x2_HMC% = Install_MPCIEX_DELLM2_7265_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54008086 ; AGN

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_DELLM2_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54108086 ; AC

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_DELLM2_7265_AC_2x2_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54128086 ; AC15

%NIC_7265AGN_2x2_HMC% = Install_MPCIEX_DELLM2NBT_7265_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54208086 ; AGN

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_DELLM2WG_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_54908086 ; AC

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_DELLSARM2_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_55108086 ; AC

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_DELLSARM2WG_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_55908086 ; AC

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_ASUSM2_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_5C108086 ; AC

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_SKLSARM2_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_5F108086 ; AC

%NIC_7265AGN_2x2_HMC% = Install_MPCIEX_GENSD_7265_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_90008086 ; AGN

%NIC_7265AGN_2x2_HMC% = Install_MPCIEX_GENSD_7265_AGN_2x2_HMC_WINB_AGN15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_900A8086 ; AGN15

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GENSD_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_90108086 ; AC

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GENSD_7265_AC_2x2_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_095A&SUBSYS_90128086 ; AC15

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GENSARSD_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_91108086 ; AC

%NIC_7265AGN_2x2_HMC% = Install_MPCIEX_DELLSD_7265_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_095A&SUBSYS_94008086 ; AGN

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_DELLSD_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_94108086 ; AC

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_DELLSARSD_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095A&SUBSYS_95108086 ; AC

%NIC_7265AGN_2x2_HMC% = Install_MPCIEX_GENUIM2_7265_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52008086 ; AGN

%NIC_7265BGN_2x2_HMC% = Install_MPCIEX_GENUIM2_7265_BGN_2x2_HMC_WINB_BGN15    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52028086 ; BGN15

%NIC_7265AGN_2x2_HMC% = Install_MPCIEX_GENUIM2_7265_AGN_2x2_HMC_WINB_AGN15    ,   PCI\VEN_8086&DEV_095B&SUBSYS_520A8086 ; AGN15

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GENUIM2_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52108086 ; AC

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GENUIM2_7265_AC_2x2_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52128086 ; AC15

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GENUIM2WG_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_52908086 ; AC

%NIC_7265BGN_2x2_HMC% = Install_MPCIEX_GENUISARM2_7265_BGN_2x2_HMC_WINB_BGN15    ,   PCI\VEN_8086&DEV_095B&SUBSYS_53028086 ; BGN15

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GENUISARM2_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_53108086 ; AC

%NIC_7265AGN_2x2_HMC% = Install_MPCIEX_GENUISD_7265_AGN_2x2_HMC_WINB_AGN    ,   PCI\VEN_8086&DEV_095B&SUBSYS_92008086 ; AGN

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GENUISD_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_92108086 ; AC

%NIC_7265AC_2x2_HMC% = Install_MPCIEX_GENUISARSD_7265_AC_2x2_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_095B&SUBSYS_93108086 ; AC

%NIC_3165AC_HMC% = Install_MPCIEX_GENM2_3165_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_3165&SUBSYS_40108086 ; AC

%NIC_3165AC_HMC% = Install_MPCIEX_GENM2_3165_AC_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_3165&SUBSYS_40128086 ; AC15

%NIC_3165AC_HMC% = Install_MPCIEX_GENSARM2_3165_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_3165&SUBSYS_41108086 ; AC

%NIC_3165AC_HMC% = Install_MPCIEX_DELLM2_3165_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_3165&SUBSYS_44108086 ; AC

%NIC_3165AC_HMC% = Install_MPCIEX_DELLSARM2_3165_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_3165&SUBSYS_45108086 ; AC

%NIC_3165AC_HMC% = Install_MPCIEX_GENSD_3165_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_3165&SUBSYS_80108086 ; AC

%NIC_3165AC_HMC% = Install_MPCIEX_GENSARSD_3165_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_3165&SUBSYS_81108086 ; AC

%NIC_3165AC_HMC% = Install_MPCIEX_GENUIM2_3165_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_3166&SUBSYS_42108086 ; AC

%NIC_3165AC_HMC% = Install_MPCIEX_GENUIM2_3165_AC_HMC_WINB_AC15    ,   PCI\VEN_8086&DEV_3166&SUBSYS_42128086 ; AC15

%NIC_3165AC_HMC% = Install_MPCIEX_GENUISARM2_3165_AC_HMC_WINB_AC    ,   PCI\VEN_8086&DEV_3166&SUBSYS_43108086 ; AC



;****************************************************************************************************
;INSTALL WINB
;----------------------------------------------------------------------------------------------------

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENNBT_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENNBT_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENNBT_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENNBT_7260_AGN_2x2_HMC_WINB_AGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENNBT_7260_AGN_2x2_HMC_WINB_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENNBT_7260_AGN_2x2_HMC_WINB_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GEN_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GEN_7260_BGN_2x2_HMC_WINB_BGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_BGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_BGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_7260_BGN_2x2_HMC_WINB_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_7260_BGN_2x2_HMC_WINB_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GEN_7260_AGN_2x2_HMC_WINB_AGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_7260_AGN_2x2_HMC_WINB_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_7260_AGN_2x2_HMC_WINB_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GEN_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GEN_7260_AC_2x2_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_7260_AC_2x2_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_7260_AC_2x2_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSAR_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSAR_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSAR_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSAR_7260_BGN_2x2_HMC_WINB_BGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_BGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_BGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSAR_7260_BGN_2x2_HMC_WINB_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSAR_7260_BGN_2x2_HMC_WINB_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSAR_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSAR_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSAR_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLNBT_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLNBT_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLNBT_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELL_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELL_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELL_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELL_7260_BGN_2x2_HMC_WINB_BGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_BGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_BGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELL_7260_BGN_2x2_HMC_WINB_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELL_7260_BGN_2x2_HMC_WINB_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELL_7260_AGN_2x2_HMC_WINB_AGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELL_7260_AGN_2x2_HMC_WINB_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELL_7260_AGN_2x2_HMC_WINB_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELL_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELL_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELL_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELL_7260_AC_2x2_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELL_7260_AC_2x2_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELL_7260_AC_2x2_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSAR_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSAR_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSAR_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSAR_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSAR_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSAR_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_IM1_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_IM1_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_IM1_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_IM2_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_IM2_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_IM2_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_AUTO_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_AUTO_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_AUTO_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_AUTO1_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_AUTO1_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_AUTO1_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_AUTO2_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_AUTO2_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_AUTO2_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_ASUS_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_ASUS_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_ASUS_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_ASUS_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_ASUS_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_ASUS_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_7260_AC_2x2_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_7260_AC_2x2_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_7260_AC_2x2_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARSD_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARSD_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARSD_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_SAMSARSD_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_SAMSARSD_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_SAMSARSD_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENNGFFNBT_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENNGFFNBT_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENNGFFNBT_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENNGFFNBT_7260_AGN_2x2_HMC_WINB_AGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENNGFFNBT_7260_AGN_2x2_HMC_WINB_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENNGFFNBT_7260_AGN_2x2_HMC_WINB_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENNGFF_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENNGFF_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENNGFF_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENNGFF_7260_BGN_2x2_HMC_WINB_BGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_BGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_BGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENNGFF_7260_BGN_2x2_HMC_WINB_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENNGFF_7260_BGN_2x2_HMC_WINB_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENNGFF_7260_AGN_2x2_HMC_WINB_AGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENNGFF_7260_AGN_2x2_HMC_WINB_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENNGFF_7260_AGN_2x2_HMC_WINB_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENNGFF_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENNGFF_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENNGFF_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENNGFF_7260_AC_2x2_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENNGFF_7260_AC_2x2_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENNGFF_7260_AC_2x2_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARNGFF_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARNGFF_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARNGFF_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARNGFF_7260_BGN_2x2_HMC_WINB_BGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_BGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_BGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARNGFF_7260_BGN_2x2_HMC_WINB_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARNGFF_7260_BGN_2x2_HMC_WINB_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARNGFF_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARNGFF_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARNGFF_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISARNGFF_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISARNGFF_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISARNGFF_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLNGFFNBT_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLNGFFNBT_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLNGFFNBT_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLNGFF_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLNGFF_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLNGFF_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLNGFF_7260_BGN_2x2_HMC_WINB_BGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_BGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_BGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLNGFF_7260_BGN_2x2_HMC_WINB_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLNGFF_7260_BGN_2x2_HMC_WINB_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLNGFF_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLNGFF_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLNGFF_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLNGFF_7260_AC_2x2_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLNGFF_7260_AC_2x2_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLNGFF_7260_AC_2x2_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARNGFF_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARNGFF_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARNGFF_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARNGFF_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARNGFF_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARNGFF_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_SAMSARNGFF_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_SAMSARNGFF_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_SAMSARNGFF_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_SAMSARNGFF_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_SAMSARNGFF_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_SAMSARNGFF_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_ASUSNGFF_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_ASUSNGFF_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_ASUSNGFF_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_ASUSNGFF_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_ASUSNGFF_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_ASUSNGFF_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUINBT_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUINBT_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUINBT_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUI_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUI_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUI_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUI_7260_BGN_2x2_HMC_WINB_BGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_BGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_BGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUI_7260_BGN_2x2_HMC_WINB_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUI_7260_BGN_2x2_HMC_WINB_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUI_7260_AGN_2x2_HMC_WINB_AGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUI_7260_AGN_2x2_HMC_WINB_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUI_7260_AGN_2x2_HMC_WINB_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUI_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUI_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUI_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUI_7260_AC_2x2_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUI_7260_AC_2x2_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUI_7260_AC_2x2_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISAR_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISAR_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISAR_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISAR_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISAR_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISAR_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUINGFFNBT_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUINGFFNBT_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUINGFFNBT_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUINGFF_7260_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUINGFF_7260_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUINGFF_7260_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUINGFF_7260_BGN_2x2_HMC_WINB_BGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_BGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_BGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUINGFF_7260_BGN_2x2_HMC_WINB_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUINGFF_7260_BGN_2x2_HMC_WINB_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUINGFF_7260_AGN_2x2_HMC_WINB_AGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUINGFF_7260_AGN_2x2_HMC_WINB_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUINGFF_7260_AGN_2x2_HMC_WINB_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUINGFF_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUINGFF_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUINGFF_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUINGFF_7260_AC_2x2_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUINGFF_7260_AC_2x2_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUINGFF_7260_AC_2x2_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISARNGFF_7260_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7260_AC_2x2_HMC, Reg_NDIS_WINB, Reg_WP2, Reg_NDI, Reg_NDI_WP2, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISARNGFF_7260_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISARNGFF_7260_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GEN_3160_AGN_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AGN_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3160_AGN_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_3160_AGN_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GEN_3160_BGN_HMC_WINB_BGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_BGN_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_BGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3160_BGN_HMC_WINB_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_3160_BGN_HMC_WINB_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GEN_3160_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3160_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_3160_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GEN_3160_AC_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_3160_AC_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_3160_AC_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSAR_3160_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSAR_3160_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSAR_3160_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSAR_3160_AC_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSAR_3160_AC_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSAR_3160_AC_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELL_3160_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELL_3160_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELL_3160_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELL_3160_AC_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELL_3160_AC_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELL_3160_AC_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_3160_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_3160_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_3160_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARSD_3160_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARSD_3160_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARSD_3160_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENNGFF_3160_AGN_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AGN_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENNGFF_3160_AGN_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENNGFF_3160_AGN_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENNGFF_3160_BGN_HMC_WINB_BGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_BGN_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_BGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENNGFF_3160_BGN_HMC_WINB_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENNGFF_3160_BGN_HMC_WINB_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENNGFF_3160_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENNGFF_3160_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENNGFF_3160_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENNGFF_3160_AC_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENNGFF_3160_AC_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENNGFF_3160_AC_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARNGFF_3160_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARNGFF_3160_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARNGFF_3160_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARNGFF_3160_AC_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARNGFF_3160_AC_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARNGFF_3160_AC_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLNGFF_3160_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLNGFF_3160_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLNGFF_3160_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARNGFF_3160_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARNGFF_3160_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARNGFF_3160_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUI_3160_AGN_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AGN_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUI_3160_AGN_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUI_3160_AGN_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUI_3160_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUI_3160_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUI_3160_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUI_3160_AC_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUI_3160_AC_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUI_3160_AC_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISAR_3160_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISAR_3160_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISAR_3160_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUINGFF_3160_AGN_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AGN_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUINGFF_3160_AGN_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUINGFF_3160_AGN_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUINGFF_3160_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUINGFF_3160_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUINGFF_3160_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUINGFF_3160_AC_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUINGFF_3160_AC_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUINGFF_3160_AC_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISARNGFF_3160_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3160_AC_HMC, Reg_NDIS_WINB, Reg_WP1, Reg_NDI, Reg_NDI_WP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISARNGFF_3160_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISARNGFF_3160_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GEN_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GEN_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GEN_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_7265_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_7265_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_7265_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_7265_BGN_2x2_HMC_WINB_BGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_BGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_BGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_7265_BGN_2x2_HMC_WINB_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_7265_BGN_2x2_HMC_WINB_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_7265_AGN_2x2_HMC_WINB_AGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_7265_AGN_2x2_HMC_WINB_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_7265_AGN_2x2_HMC_WINB_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_7265_AC_2x2_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_7265_AC_2x2_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_7265_AC_2x2_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2NBT_7265_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2NBT_7265_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2NBT_7265_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2NBT_7265_AGN_2x2_HMC_WINB_AGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2NBT_7265_AGN_2x2_HMC_WINB_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2NBT_7265_AGN_2x2_HMC_WINB_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2WG_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2WG_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2WG_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2_7265_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2_7265_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2_7265_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2_7265_BGN_2x2_HMC_WINB_BGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_BGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_BGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2_7265_BGN_2x2_HMC_WINB_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2_7265_BGN_2x2_HMC_WINB_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2WG_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2WG_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2WG_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2_7265_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2_7265_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2_7265_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2_7265_AC_2x2_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2_7265_AC_2x2_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2_7265_AC_2x2_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2NBT_7265_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2NBT_7265_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2NBT_7265_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2WG_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2WG_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2WG_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARM2_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARM2_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARM2_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARM2WG_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARM2WG_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARM2WG_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_ASUSM2_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_ASUSM2_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_ASUSM2_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_SKLSARM2_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_SKLSARM2_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_SKLSARM2_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_7265_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_7265_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_7265_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_7265_AGN_2x2_HMC_WINB_AGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_7265_AGN_2x2_HMC_WINB_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_7265_AGN_2x2_HMC_WINB_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_7265_AC_2x2_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_7265_AC_2x2_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_7265_AC_2x2_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARSD_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARSD_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARSD_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSD_7265_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSD_7265_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSD_7265_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSD_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSD_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSD_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARSD_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARSD_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARSD_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_7265_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_7265_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_7265_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_7265_BGN_2x2_HMC_WINB_BGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_BGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_BGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_7265_BGN_2x2_HMC_WINB_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_7265_BGN_2x2_HMC_WINB_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_7265_AGN_2x2_HMC_WINB_AGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_7265_AGN_2x2_HMC_WINB_AGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_7265_AGN_2x2_HMC_WINB_AGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_7265_AC_2x2_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_7265_AC_2x2_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_7265_AC_2x2_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2WG_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2WG_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2WG_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISARM2_7265_BGN_2x2_HMC_WINB_BGN15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_BGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_BGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISARM2_7265_BGN_2x2_HMC_WINB_BGN15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISARM2_7265_BGN_2x2_HMC_WINB_BGN15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISARM2_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISARM2_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISARM2_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISD_7265_AGN_2x2_HMC_WINB_AGN]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AGN_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AGN, Reg_NDI_11N, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISD_7265_AGN_2x2_HMC_WINB_AGN.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISD_7265_AGN_2x2_HMC_WINB_AGN.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISD_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISD_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISD_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISARSD_7265_AC_2x2_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_7265_AC_2x2_HMC, Reg_NDIS_WINB, Reg_STP, Reg_NDI, Reg_NDI_STP, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISARSD_7265_AC_2x2_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISARSD_7265_AC_2x2_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_3165_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3165_AC_HMC, Reg_NDIS_WINB, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_3165_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_3165_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENM2_3165_AC_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3165_AC_HMC, Reg_NDIS_WINB, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENM2_3165_AC_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENM2_3165_AC_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARM2_3165_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3165_AC_HMC, Reg_NDIS_WINB, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARM2_3165_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARM2_3165_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLM2_3165_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3165_AC_HMC, Reg_NDIS_WINB, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLM2_3165_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLM2_3165_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_DELLSARM2_3165_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3165_AC_HMC, Reg_NDIS_WINB, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_DELLSARM2_3165_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_DELLSARM2_3165_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSD_3165_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3165_AC_HMC, Reg_NDIS_WINB, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSD_3165_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSD_3165_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENSARSD_3165_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3165_AC_HMC, Reg_NDIS_WINB, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENSARSD_3165_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENSARSD_3165_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_3165_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3165_AC_HMC, Reg_NDIS_WINB, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_3165_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_3165_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUIM2_3165_AC_HMC_WINB_AC15]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3165_AC_HMC, Reg_NDIS_WINB, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUIM2_3165_AC_HMC_WINB_AC15.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUIM2_3165_AC_HMC_WINB_AC15.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

;----------------------------------------------------------------------------------------------------

[Install_MPCIEX_GENUISARM2_3165_AC_HMC_WINB_AC]
FeatureScore    = 0xFD
Include         = netvwifibus.inf
Needs           = VWiFiBus.CopyFiles
DelReg          = DelReg_Common
AddReg          = Reg_Common, Reg_Common_WINB, Reg_3165_AC_HMC, Reg_NDIS_WINB, Reg_STP1, Reg_NDI, Reg_NDI_STP1, Reg_NDI_AC, Reg_NDI_BTHS
Characteristics = 0x84; NCF_HAS_UI, NCF_PHYSICAL
BusType         = 5; PCI bus
CopyFiles       = CopyFiles_Driver_WINB
*IfType = 71             	; IF_TYPE_IEEE80211
*MediaType = 16          	; NdisMediumNative802_11
*PhysicalMediaType = 9   	; NdisPhysicalMediumNative802_11

[Install_MPCIEX_GENUISARM2_3165_AC_HMC_WINB_AC.HW]
Include         = netvwifibus.inf
Needs           = VWiFiBus.PnPFilterRegistration
AddReg          = MSI_NDIS.reg

[Install_MPCIEX_GENUISARM2_3165_AC_HMC_WINB_AC.Services]
Include         = netvwifibus.inf
Needs           = VWiFiBus.Services
AddService      = NETwNb32, 2, NIC_Service_WINB, Common_EventLog_WINB

[Reg_NDI_BTHS]
[DelReg_Common]
HKR,,ChannelWidth24
HKR,,ChannelWidth52
HKR,,TGeEnableBits
HKR,,uAPSDSupport
HKR,,CtsToItself
HKR, Ndi\

[Reg_Common]
HKR,,ApsdTriggerQueues,0x10001,0x0
HKR,,CardType,0x00010001,2
HKR,,CCXv4FeatureSet,0x10001,0x0
HKR,,CcxSdkActive,0x10003,0x1
HKR,,CcxVersion,0x10003,0x4
HKR,,ConfigurationName,0,"PR0W1RELE55"
HKR,,ConnectionPriority,0,"2"
HKR,,DesiredAuthenticationMode,0x10003,0x0
HKR,,DesiredCipher,0x10003,0x1
HKR,,DesiredDefaultKeyId,0x10003,0x1
HKR,,DesiredPortType,0x10003,0x1
HKR,,DesiredPSKey1,0x2,""
HKR,,DesiredPSKey2,0x2,""
HKR,,DesiredPSKey3,0x2,""
HKR,,DesiredPSKey4,0x2,""
HKR,,ExternalImage,0x10001,0x0
HKR,,FixedLongPreamble,0x10001,0x0
HKR,,FixedSupportedRates,0x10001,0xFFF
HKR,,ModulationType,2,"2"
HKR,,NdisEnvironment,0x10001,0
HKR,,NetType,0,"WLAN"
HKR,,PibssShortSlot,0x10001,0x1
HKR,,Provider,0,%PROVIDER_NAME%
HKR,,RadioEnable,0x10003,0x1
HKR,,RecommendedBeaconInterval,0x10001,0x64
HKR,,BTOnThreshold,0x10001,0x4
HKR,,APMMode,0x10001,0x0
HKR,,AtomMaxDpcTime,0x10001,0x14
HKR,,MaxDpcTime,0x10001,0x1E
HKR,,DuplicateRateSupported,0x10001,0x0
HKR,,BaEnable,0x10001,0x0
HKR,,PanTimeoutForResetTxFailCnt,0x10001,0x64
HKR,,ChannelWidth24,0,"1"
HKR,,ChannelWidth52,0,"1"
HKR,,CtsToItself,0,"0"
HKR,,*MiracastSupported,0x10001,0x1

; following registry keys define the Advanced Property Page (NDI) values. they are common, and the defult values vary between the different reg sections.
[Reg_NDI_BGN]
HKR, Ndi\Params\WirelessMode,			ParamDesc,  0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode, 			Type, 	    0, "enum",
HKR, Ndi\params\WirelessMode, 			Default,    0, "32" ;bg
HKR, Ndi\Params\WirelessMode, 			Optional,   0, "0"
HKR, Ndi\params\WirelessMode\enum, 		"0",  	    0, "1. 802.11b"
HKR, Ndi\params\WirelessMode\enum, 		"16", 	    0, "2. 802.11g"
HKR, Ndi\params\WirelessMode\enum, 		"32", 	    0, "3. 802.11b/g"

[Reg_NDI_AGN]                                               
HKR, Ndi\Params\WirelessMode,               	ParamDesc,  0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode,               	Type,       0, "enum",
HKR, Ndi\params\WirelessMode,      		Default,    0, "34" ;abg
HKR, Ndi\Params\WirelessMode,               	Optional,   0, "0"
HKR, Ndi\params\WirelessMode\enum, 		"17",       0, "1. 802.11a"
HKR, Ndi\params\WirelessMode\enum, 		"0",        0, "2. 802.11b"
HKR, Ndi\params\WirelessMode\enum, 		"16",       0, "3. 802.11g"
HKR, Ndi\params\WirelessMode\enum, 		"32",       0, "4. 802.11b/g"
HKR, Ndi\params\WirelessMode\enum,              "18",       0, "5. 802.11a/g"
HKR, Ndi\params\WirelessMode\enum, 		"34",       0, "6. 802.11a/b/g"

HKR, Ndi\params\RoamingPreferredBandType,     	ParamDesc,  0x00000000, %PREFERRED_BAND_STR%
HKR, Ndi\params\RoamingPreferredBandType,     	Type,       0x00000002, "enum"
HKR, Ndi\params\RoamingPreferredBandType,     	Default,    0x00000002, "0"
HKR, Ndi\params\RoamingPreferredBandType,     	Optional,   0x00000002, "0"
HKR, Ndi\params\RoamingPreferredBandType\enum,	"0",        0x00000000, "1. "%NO_PREFERECE_STR%
HKR, Ndi\params\RoamingPreferredBandType\enum,	"1",        0x00000000, "2. "%PREFER_24_BAND_STR%
HKR, Ndi\params\RoamingPreferredBandType\enum,  "2",        0x00000000, "3. "%PREFER_52_BAND_STR%

HKR, Ndi\params\ChannelWidth52,			ParamDesc,  0,  %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,			Type,       0,  "enum"
HKR, Ndi\params\ChannelWidth52,			Default,    0,  "1"
HKR, Ndi\params\ChannelWidth52,			Optional,   0,  "0"
HKR, Ndi\params\ChannelWidth52\enum, 		"0",        0,  %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 		"1",        0,  %CHANNELWIDTHAUTO%

[Reg_NDI_AC]                                                
HKR, Ndi\Params\WirelessMode,               	ParamDesc,  0, %WIRELESS_MODE_STR%
HKR, Ndi\Params\WirelessMode,               	Type,       0, "enum",
HKR, Ndi\params\WirelessMode,      		Default,    0, "34" ;abg
HKR, Ndi\Params\WirelessMode,               	Optional,   0, "0"
HKR, Ndi\params\WirelessMode\enum, 		"17",       0, "1. 802.11a"
HKR, Ndi\params\WirelessMode\enum, 		"0",        0, "2. 802.11b"
HKR, Ndi\params\WirelessMode\enum, 		"16",       0, "3. 802.11g"
HKR, Ndi\params\WirelessMode\enum, 		"32",       0, "4. 802.11b/g"
HKR, Ndi\params\WirelessMode\enum,              "18",       0, "5. 802.11a/g"
HKR, Ndi\params\WirelessMode\enum, 		"34",       0, "6. 802.11a/b/g"

HKR, Ndi\params\RoamingPreferredBandType,     	ParamDesc,  0x00000000, %PREFERRED_BAND_STR%
HKR, Ndi\params\RoamingPreferredBandType,     	Type,       0x00000002, "enum"
HKR, Ndi\params\RoamingPreferredBandType,     	Default,    0x00000002, "0"
HKR, Ndi\params\RoamingPreferredBandType,     	Optional,   0x00000002, "0"
HKR, Ndi\params\RoamingPreferredBandType\enum,	"0",        0x00000000, "1. "%NO_PREFERECE_STR%
HKR, Ndi\params\RoamingPreferredBandType\enum,	"1",        0x00000000, "2. "%PREFER_24_BAND_STR%
HKR, Ndi\params\RoamingPreferredBandType\enum,  "2",        0x00000000, "3. "%PREFER_52_BAND_STR%

HKR, Ndi\params\ChannelWidth52,			ParamDesc,  0,  %CHANNELWIDTH52%
HKR, Ndi\params\ChannelWidth52,			Type,       0,  "enum"
HKR, Ndi\params\ChannelWidth52,			Default,    0,  "1"
HKR, Ndi\params\ChannelWidth52,			Optional,   0,  "0"
HKR, Ndi\params\ChannelWidth52\enum, 		"0",        0,  %CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth52\enum, 		"1",        0,  %CHANNELWIDTHAUTO%

HKR, Ndi\params\IEEE11nMode,			ParamDesc,  0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,			Type,       0, "enum"
HKR, Ndi\params\IEEE11nMode,			Default,    0, "2"
HKR, Ndi\params\IEEE11nMode,			Optional,   0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 		"0",        0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 		"1",        0, %HT_ENABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 		"2",        0, %VHT_ENABLED_STR%

[Reg_NDI]                                       
HKR, Ndi\params\ThroughputBoosterEnabled,	ParamDesc,  0x00000000, %THROUGHPUTBOOSTER_STR%
HKR, Ndi\params\ThroughputBoosterEnabled,	Type,  	    0x00000002, "enum"
HKR, Ndi\params\ThroughputBoosterEnabled,	Default,    0x00000002, "0"
HKR, Ndi\params\ThroughputBoosterEnabled,	Optional,   0x00000002, "0"
HKR, Ndi\params\ThroughputBoosterEnabled\enum,  "0",  	    0x00000000, %DISABLED_STR%
HKR, Ndi\params\ThroughputBoosterEnabled\enum,  "1",  	    0x00000000, %ENABLED_STR%

HKR, Ndi\params\RecommendedChannel24,      	ParamDesc,  0x00000000, %RECOMMENDED_CHANNEL24_STR%
HKR, Ndi\params\RecommendedChannel24,      	Type,       0x00000002, "int"
HKR, Ndi\params\RecommendedChannel24,      	Optional,   0x00000002, "0"
HKR, Ndi\params\RecommendedChannel24,      	Min,	    0x00000002, "1"
HKR, Ndi\params\RecommendedChannel24,      	Step,	    0x00000002, "1"
HKR, Ndi\params\RecommendedChannel24,      	Max,	    0x00000002, "11"    		      

HKR, Ndi\params\ChannelWidth24,			ParamDesc,  0, 	%CHANNELWIDTH24%
HKR, Ndi\params\ChannelWidth24,			Type,       0, 	"enum"
HKR, Ndi\params\ChannelWidth24,			Default,    0, 	"1"
HKR, Ndi\params\ChannelWidth24,			Optional,   0, 	"0"
HKR, Ndi\params\ChannelWidth24\enum, 		"0",        0, 	%CHANNELWIDTH20ONLY%
HKR, Ndi\params\ChannelWidth24\enum, 		"1",        0, 	%CHANNELWIDTHAUTO%

HKR, Ndi\params\IbssTxPower,      	     	ParamDesc,  0x00000000, %IBSS_TX_POWER_STR%
HKR, Ndi\params\IbssTxPower,      	     	Type,       0x00000002, "enum"
HKR, Ndi\params\IbssTxPower,      	     	Default,    0x00000002, "100"
HKR, Ndi\params\IbssTxPower,      	     	Optional,   0x00000002, "0"
HKR, Ndi\params\IbssTxPower\enum, 	     	"0",        0x00000000, "1. "%LOWEST_STR%
HKR, Ndi\params\IbssTxPower\enum, 	     	"25",       0x00000000, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\params\IbssTxPower\enum, 	     	"50",       0x00000000, "3. "%MEDIUM_STR%
HKR, Ndi\params\IbssTxPower\enum, 	     	"75",       0x00000000, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\params\IbssTxPower\enum, 	     	"100",      0x00000000, "5. "%HIGHEST_STR%

HKR, Ndi\params\RoamAggressiveness,     	ParamDesc,  0x00000000, %ROAMING_AGGRESSIVENESS_STR%
HKR, Ndi\params\RoamAggressiveness,     	Type,       0x00000002, "enum"
HKR, Ndi\params\RoamAggressiveness,     	Default,    0x00000002, "2"
HKR, Ndi\params\RoamAggressiveness,     	Optional,   0x00000002, "0"
HKR, Ndi\params\RoamAggressiveness\enum,	"0",        0x00000000, "1. "%LOWEST_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	"1",        0x00000000, "2. "%MEDIUM_LOW_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	"2",        0x00000000, "3. "%MEDIUM_STR%
HKR, Ndi\params\RoamAggressiveness\enum,	"3", 	    0x00000000, "4. "%MEDIUM_HIGH_STR%
HKR, Ndi\params\RoamAggressiveness\enum,    	"4",        0x00000000, "5. "%HIGHEST_STR%

HKR, Ndi\params\IbssQosEnabled,			ParamDesc,  0x00000000, %ADHOC_QOS_MODE_STR%
HKR, Ndi\params\IbssQosEnabled,			Type,  	    0x00000002, "enum"
HKR, Ndi\params\IbssQosEnabled,			Default,    0x00000002, "0"
HKR, Ndi\params\IbssQosEnabled,			Optional,   0x00000002, "0"
HKR, Ndi\params\IbssQosEnabled\enum,  		"0",  	    0x00000000, %WMM_DISABLED_STR%
HKR, Ndi\params\IbssQosEnabled\enum,  		"1",  	    0x00000000, %WMM_ENABLED_STR%

HKR, Ndi\params\CtsToItself,			ParamDesc,  0x00000000, %MIXED_MODE_PROTECTION_STR%
HKR, Ndi\params\CtsToItself,			Type,  	    0x00000002, "enum"
HKR, Ndi\params\CtsToItself,			Default,    0x00000002, "0"
HKR, Ndi\params\CtsToItself,			Optional,   0x00000002, "0"
HKR, Ndi\params\CtsToItself\enum, 		"0",  	    0x00000000, %RTS_CTS_ENABLED_STR%
HKR, Ndi\params\CtsToItself\enum, 		"1",  	    0x00000000, %CTS_TO_SELF_ENABLED_STR%

HKR, Ndi\params\FatChannelIntolerant, 	    	ParamDesc,  0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	    0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,    0, "0"
HKR, Ndi\params\FatChannelIntolerant, 		Optional,   0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	    0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	    0, %ENABLED_STR%

HKR, Ndi\params\uAPSDSupport, 	    		ParamDesc,  0, %U_APSD_SUPPORT%
HKR, Ndi\params\uAPSDSupport, 			Type,	    0, "enum"
HKR, Ndi\params\uAPSDSupport, 			Optional,   0, "0"
HKR, Ndi\params\uAPSDSupport,			Default,    0, "0"
HKR, Ndi\params\uAPSDSupport\enum,  		"0",	    0, %DISABLED_STR%
HKR, Ndi\params\uAPSDSupport\enum,  		"1",	    0, %ENABLED_STR%


HKR, Ndi\Params\*WakeOnPattern,                 ParamDesc,  0, %WAKE_ON_PATTERN_MATCH%
HKR, Ndi\Params\*WakeOnPattern\Enum,            "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnPattern\Enum,            "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnPattern,                 type,       0, "enum"
HKR, Ndi\Params\*WakeOnPattern,                 default,    0, "1"

HKR, Ndi\Params\*WakeOnMagicPacket,             ParamDesc,  0, %WAKE_ON_MAGIC_PACKET%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,        "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket\Enum,        "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*WakeOnMagicPacket,             type,       0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket,             default,    0, "1"

HKR, Ndi\Params\*PMWiFiRekeyOffload,            ParamDesc,  0, %PM_WIFI_REKEY_OFFLOAD%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload\Enum,       "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMWiFiRekeyOffload,            type,       0, "enum"
HKR, Ndi\Params\*PMWiFiRekeyOffload,            default,    0, "1"

HKR, Ndi\Params\*PMARPOffload,                  ParamDesc,  0, %PM_ARP_OFFLOAD%
HKR, Ndi\Params\*PMARPOffload\Enum,             "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMARPOffload\Enum,             "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMARPOffload,                  type,       0, "enum"
HKR, Ndi\Params\*PMARPOffload,                  default,    0, "1"

HKR, Ndi\Params\*PMNSOffload,                   ParamDesc,  0, %PM_NS_OFFLOAD%
HKR, Ndi\Params\*PMNSOffload\Enum,              "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*PMNSOffload\Enum,              "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*PMNSOffload,                   type,       0, "enum"
HKR, Ndi\Params\*PMNSOffload,                   default,    0, "1"

HKR, Ndi\Params\*DeviceSleepOnDisconnect,       ParamDesc,  0, %DEVICE_SLEEP_ON_DISCONNECT%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  "0",        0, %DISABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect\Enum,  "1",        0, %ENABLED_STR%
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       type,       0, "enum"
HKR, Ndi\Params\*DeviceSleepOnDisconnect,       default,    0, "0"

[Reg_NDI_WP1]
HKR,,CLSGUID,0,"{6DB92573-C061-11E1-A839-441EA15FCEDE}"

HKR, Ndi\params\BT3HSMode,			ParamDesc, 	0, %BTHSMode%
HKR, Ndi\params\BT3HSMode,			Type,      	0, "enum"
HKR, Ndi\params\BT3HSMode,			Default,   	0, "0"
HKR, Ndi\params\BT3HSMode,			Optional,  	0, "0"
HKR, Ndi\params\BT3HSMode\enum,			"0",        	0, %DISABLED_STR%
HKR, Ndi\params\BT3HSMode\enum,			"1",        	0, %ENABLED_STR%
HKR, Ndi\Interfaces,				UpperRange,	0, "ndis5,wifipro,intel_amp,intel_psm"

[Reg_NDI_WP2]
HKR,,CLSGUID,0,"{6DB92573-C061-11E1-A839-441EA15FCEDE}"

HKR, Ndi\params\BT3HSMode,			ParamDesc, 	0, %BTHSMode%
HKR, Ndi\params\BT3HSMode,			Type,      	0, "enum"
HKR, Ndi\params\BT3HSMode,			Default,   	0, "0"
HKR, Ndi\params\BT3HSMode,			Optional,  	0, "0"
HKR, Ndi\params\BT3HSMode\enum,			"0",        	0, %DISABLED_STR%
HKR, Ndi\params\BT3HSMode\enum,			"1",        	0, %ENABLED_STR%
HKR, Ndi\Interfaces,				UpperRange,	0, "ndis5,wifipro,intel_amp,intel_psm"

[Reg_NDI_STP]
HKR,,CLSGUID,0,"{15520CF2-F2F6-44eb-97D4-039BC10BEA1D}"

HKR, Ndi\params\BT3HSMode,			ParamDesc, 	0, %BTHSMode%
HKR, Ndi\params\BT3HSMode,			Type,      	0, "enum"
HKR, Ndi\params\BT3HSMode,			Default,   	0, "0"
HKR, Ndi\params\BT3HSMode,			Optional,  	0, "0"
HKR, Ndi\params\BT3HSMode\enum,			"0",        	0, %DISABLED_STR%
HKR, Ndi\params\BT3HSMode\enum,			"1",        	0, %ENABLED_STR%
HKR, Ndi\Interfaces,				UpperRange,	0, "ndis5,wifipro,intel_amp,intel_psm"

[Reg_NDI_STP1]
HKR,,CLSGUID,0,"{15520CF2-F2F6-44eb-97D4-039BC10BEA1D}"

HKR, Ndi\params\BT3HSMode,			ParamDesc, 	0, %BTHSMode%
HKR, Ndi\params\BT3HSMode,			Type,      	0, "enum"
HKR, Ndi\params\BT3HSMode,			Default,   	0, "0"
HKR, Ndi\params\BT3HSMode,			Optional,  	0, "0"
HKR, Ndi\params\BT3HSMode\enum,			"0",        	0, %DISABLED_STR%
HKR, Ndi\params\BT3HSMode\enum,			"1",        	0, %ENABLED_STR%
HKR, Ndi\Interfaces,				UpperRange,	0, "ndis5,wifipro,intel_amp,intel_psm"

[Reg_NDI_11N]                                   
HKR, Ndi\params\IEEE11nMode,			ParamDesc, 	0, %TGnMode%
HKR, Ndi\params\IEEE11nMode,			Type,      	0, "enum"
HKR, Ndi\params\IEEE11nMode,			Default,   	0, "1"
HKR, Ndi\params\IEEE11nMode,			Optional,  	0, "0"
HKR, Ndi\params\IEEE11nMode\enum, 		"0",        	0, %DISABLED_STR%
HKR, Ndi\params\IEEE11nMode\enum, 		"1",        	0, %HT_ENABLED_STR%

HKR, Ndi\params\FatChannelIntolerant, 	    	ParamDesc,	0, %FAT_CHANNEL_TOLERANT%
HKR, Ndi\params\FatChannelIntolerant, 		Type,	 	0, "enum"
HKR, Ndi\params\FatChannelIntolerant, 		Default,	0, "0" ;Disable
HKR, Ndi\params\FatChannelIntolerant, 		Optional, 	0, "0"
HKR, Ndi\params\FatChannelIntolerant\enum,  	"0",	  	0, %DISABLED_STR%
HKR, Ndi\params\FatChannelIntolerant\enum,  	"1",	  	0, %ENABLED_STR%


[Reg_NDIS_WINB]
HKR, Ndi\Interfaces,  UpperRange,   0, "ndis5,wifipro"
HKR, Ndi\Interfaces,  LowerRange,   0, "ethernet,wlan,vwifi"
HKR, Ndi,             Service,      0, "NETwNb32"

; =========================
; Registry settings by HW
; =========================
[Reg_WP1]
HKR,,uAPSDSupport,0,0
HKR,,TGeEnableBits,0x10001,0x00000027
HKR,,FixedSupportedHtRates,0x10001,0x000000FF
HKR,,VhtSupportedRxMcs,0x10001,0x1FFFFFFE
HKR,,VhtsupportedTxMcs,0x10001,0x1FFFFFFE
HKR,,GoVhtSupportedRxMcs,0x10001,0x1FFFFFFE
HKR,,GoVhtSupportedTxMcs,0x10001,0x1FFFFFFE
HKR,,rlcChainSettings,0x10001,0x2
HKR,,tlcValidAntenna,0x10001,0x1
HKR,,SystemAllowedAntennas,0x10001,0x101
HKR,,vhtCapabilities,0x10001,0x03807121
HKR,,RxStbc,0x10001,0x1
HKR,,tlcTpcAllowMCS9,0x10001,0x0
HKR,,OtpMode,0x00010001,0x0

[Reg_WP2]
HKR, Ndi\Params\*PacketCoalescing,                 ParamDesc,              0, %PACKET_COALESCING%
HKR, Ndi\Params\*PacketCoalescing,                 type,                   0, "enum"
HKR, Ndi\Params\*PacketCoalescing,                 default,                0, "1"
HKR, Ndi\Params\*PacketCoalescing\Enum,            "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PacketCoalescing\Enum,            "1",                    0, %ENABLED_STR%
HKR,,uAPSDSupport,0,0
HKR,,TGeEnableBits,0x10001,0x00000037
HKR,,BTDuration,0x10001,0xFFFFFFFF
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,vhtCapabilities,0x10001,0x3807122
HKR,,RxStbc,0x10001,0x1
HKR,,tlcTpcAllowMCS9,0x10001,0x0
HKR,,OtpMode,0x00010001,0x0

[Reg_STP]
HKR, Ndi\Params\*PacketCoalescing,                 ParamDesc,              0, %PACKET_COALESCING%
HKR, Ndi\Params\*PacketCoalescing,                 type,                   0, "enum"
HKR, Ndi\Params\*PacketCoalescing,                 default,                0, "1"
HKR, Ndi\Params\*PacketCoalescing\Enum,            "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PacketCoalescing\Enum,            "1",                    0, %ENABLED_STR%
HKR, Ndi\Interfaces,				UpperRange,                0, "ndis5,wifipro,intel_psm"
HKR,,uAPSDSupport,0,0
HKR,,TGeEnableBits,0x10001,0x00000037
HKR,,BTDuration,0x10001,0xFFFFFFFF
HKR,,FixedSupportedHtRates,0x10001,0x0000FFFF
HKR,,RxStbc,0x10001,0x1
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,vhtCapabilities,0x00010001,0x038171B1
HKR,,HtTxStbc,0x10001,1
HKR,,TxLdpc,0x10001,1
HKR,,HtRxLdpc,0x10001,1
HKR,,CtdpSupported,0x10001,1
HKR,,LowLinearitySupported,0x10001,1
HKR,,OtpMode,0x00010001,0x0

[Reg_STP1]
;This section is full copy from STP, if you think it should be changed, go ahead
HKR, Ndi\Params\*PacketCoalescing,                 ParamDesc,              0, %PACKET_COALESCING%
HKR, Ndi\Params\*PacketCoalescing,                 type,                   0, "enum"
HKR, Ndi\Params\*PacketCoalescing,                 default,                0, "1"
HKR, Ndi\Params\*PacketCoalescing\Enum,            "0",                    0, %DISABLED_STR%
HKR, Ndi\Params\*PacketCoalescing\Enum,            "1",                    0, %ENABLED_STR%
HKR, Ndi\Interfaces,				UpperRange,                0, "ndis5,wifipro,intel_psm"
HKR,,uAPSDSupport,0,0
HKR,,TGeEnableBits,0x10001,0x00000037
HKR,,BTDuration,0x10001,0xFFFFFFFF
HKR,,FixedSupportedHtRates,0x10001,0x000000FF
HKR,,RxStbc,0x10001,0x1
HKR,,SystemAllowedAntennas,0x10001,0x303
HKR,,vhtCapabilities,0x00010001,0x03817131
HKR,,HtTxStbc,0x10001,0
HKR,,TxLdpc,0x10001,1
HKR,,HtRxLdpc,0x10001,1
HKR,,CtdpSupported,0x10001,1
HKR,,LowLinearitySupported,0x10001,1
HKR,,VhtSupportedRxMcs,0x10001,0x1FFFFFFE
HKR,,VhtsupportedTxMcs,0x10001,0x1FFFFFFE
HKR,,GoVhtSupportedRxMcs,0x10001,0x1FFFFFFE
HKR,,GoVhtSupportedTxMcs,0x10001,0x1FFFFFFE
HKR,,OtpMode,0x00010001,0x0

; =========================
; Registry settings by OS
; =========================

[Reg_Common_WINB]
HKR,,SkipOverDtimEnable,0x10001,0x1
HKR,,LprxEnable,0x10001,0x1
HKR,,GreenFieldCapable,0x10001,0x0
HKR,,PanEnabled,0x10001,0x1
HKR,,BaEnable,0x10001,0x1
HKR,,CalibrationActive,0x10001,0x0
HKR,,CalibrationActiveUcode,0x10001,0x0


; =========================
; Registry settings by SKU
; =========================
[Reg_7260_AC_2x2_HMC]
HKR,,AdapterModel,0,%NIC_AdapterModel_7260AC_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_7260AC_2x2%
HKR,,SKU_CAP,0x10001,0xf

[Reg_7260_AGN_2x2_HMC]
HKR,,AdapterModel,0,%NIC_AdapterModel_7260AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_7260AGN_2x2%
HKR,,SKU_CAP,0x10001,0x7

[Reg_7260_BGN_2x2_HMC]
HKR,,AdapterModel,0,%NIC_AdapterModel_7260BGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_7260BGN_2x2%
HKR,,SKU_CAP,0x10001,0x5

[Reg_3160_AC_HMC]
HKR,,AdapterModel,0,%NIC_AdapterModel_3160AC_HMC%
HKR,,DriverDesc,0,%NIC_DriverDesc_3160AC_HMC%
HKR,,SKU_CAP,0x10001,0xf

[Reg_3160_AGN_HMC]
HKR,,AdapterModel,0,%NIC_AdapterModel_3160AGN_HMC%
HKR,,DriverDesc,0,%NIC_DriverDesc_3160AGN_HMC%
HKR,,SKU_CAP,0x10001,0x7

[Reg_3160_BGN_HMC]
HKR,,AdapterModel,0,%NIC_AdapterModel_3160BGN_HMC%
HKR,,DriverDesc,0,%NIC_DriverDesc_3160BGN_HMC%
HKR,,SKU_CAP,0x10001,0x5

[Reg_7265_AC_2x2_HMC]
HKR,,AdapterModel,0,%NIC_AdapterModel_7265AC_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_7265AC_2x2%
HKR,,SKU_CAP,0x10001,0xf

[Reg_7265_AGN_2x2_HMC]
HKR,,AdapterModel,0,%NIC_AdapterModel_7265AGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_7265AGN_2x2%
HKR,,SKU_CAP,0x10001,0x7

[Reg_7265_BGN_2x2_HMC]
HKR,,AdapterModel,0,%NIC_AdapterModel_7265BGN_2x2%
HKR,,DriverDesc,0,%NIC_DriverDesc_7265BGN_2x2%
HKR,,SKU_CAP,0x10001,0x5

[Reg_3165_AC_HMC]
HKR,,AdapterModel,0,%NIC_AdapterModel_3165AC_HMC%
HKR,,DriverDesc,0,%NIC_DriverDesc_3165AC_HMC%
HKR,,SKU_CAP,0x10001,0xf

; =============================
; Registry settings for Binding
; =============================

[MSI_NDIS.reg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1

; ===============================
; Registry settings for EventLogs
; ===============================

[Reg_CommonAddEventLog_WINB]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\Drivers\Netwbn02.sys"
HKR,, TypesSupported,   0x00010001, 7



[NIC_Service_WINB]
DisplayName = "___" %NIC_Service_DispName_WINB%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary = %12%\Netwbn02.sys
LoadOrderGroup  = NDIS

[Common_EventLog_WINB]
AddReg = Reg_CommonAddEventLog_WINB

;----------------------------------------------------------------------------------------------------
; DestinationDirs
;----------------------------------------------------------------------------------------------------

[CopyFiles_Driver_WINB]
Netwbn02.sys,,,2
Netwfw02.dat,,,2

[SourceDisksNames]
1=%SOURCEDISK1%,,

[SourceDisksFiles]
Netwbn02.sys = 1,,
Netwfw02.dat = 1,,

[DestinationDirs]
DefaultDestDir = 11 ; Windows\System32
CopyFiles_Driver_WINB=12;Windows\System32\Drivers

[Strings]
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Intel(R) Wireless Adapter Driver for Windows 8.1 - 32 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	= "Ad Hoc Channel 802.11b/g"
IBSS_TX_POWER_STR           	= "Transmit Power"
ROAMING_AGGRESSIVENESS_STR	= "Roaming Aggressiveness"
ADHOC_QOS_MODE_STR          	= "Ad Hoc QoS Mode"
MIXED_MODE_PROTECTION_STR   	= "Mixed Mode Protection"
WIRELESS_MODE_STR           	= "Wireless Mode"
PREFERRED_BAND_STR          	= "Preferred Band"
CHANNELWIDTH52              	= "802.11n Channel Width for 5.2GHz"
CHANNELWIDTH24              	= "802.11n Channel Width for 2.4GHz"
TGnMode                     	= "HT Mode"
VHT_ENABLED_STR			= "VHT Mode"
HT_ENABLED_STR			= "HT Mode"
BTHSMode                    	= "Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		= "Fat Channel Intolerant"
LOWEST_STR			= "Lowest"
MEDIUM_LOW_STR			= "Medium-low"
MEDIUM_STR			= "Medium"
MEDIUM_HIGH_STR			= "Medium-High"
HIGHEST_STR			= "Highest"
DISABLED_STR			= "Disabled"
ENABLED_STR 			= "Enabled"
CTS_TO_SELF_ENABLED_STR     	= "CTS-to-self Enabled"
RTS_CTS_ENABLED_STR         	= "RTS/CTS Enabled"
CHANNELWIDTH20ONLY          	= "20 MHz Only"
CHANNELWIDTHAUTO            	= "Auto"
WMM_DISABLED_STR            	= "WMM Disabled"
WMM_ENABLED_STR             	= "WMM Enabled"
NO_PREFERECE_STR            	= "No Preference"
PREFER_24_BAND_STR          	= "Prefer 2.4GHz band"
PREFER_52_BAND_STR          	= "Prefer 5.2GHz band"
WAKE_ON_MAGIC_PACKET        	= "Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH       	= "Wake on Pattern Match"
PM_WIFI_REKEY_OFFLOAD	    	= "GTK rekeying for WoWLAN"
PM_ARP_OFFLOAD			= "ARP offload for WoWLAN"
PM_NS_OFFLOAD			= "NS offload for WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	= "Sleep on WoWLAN Disconnect"
PACKET_COALESCING               = "Packet Coalescing"
U_APSD_SUPPORT			= "U-APSD support"
THROUGHPUTBOOSTER_STR   	= "Throughput Booster"

SOURCEDISK1                     = "Intel(R) Wireless Install Disk"

[Strings.0401] ; Arabic (Saudi Arabia)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="برنامج تشغيل محول Intel(R) Wireless لنظام Windows 8.1 32 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="قناة الأقران 802.11b/g"
IBSS_TX_POWER_STR           	="طاقة الإرسال"
ROAMING_AGGRESSIVENESS_STR	="نشاط التجوال"
ADHOC_QOS_MODE_STR          	="الوضع QoS للأقران"
MIXED_MODE_PROTECTION_STR   	="حماية الوضع المختلط"
WIRELESS_MODE_STR           	="وضع اللاسلكي"
PREFERRED_BAND_STR          	="مدى الموجات المفضل"
CHANNELWIDTH52              	="عرض القناة 802.11n ‏5.2 غيغا هرتز"
CHANNELWIDTH24              	="عرض القناة 802.11n ‏2.4 غيغا هرتز"
TGnMode                     	="وضع HT"
VHT_ENABLED_STR			="وضع VHT"
HT_ENABLED_STR			="وضع HT"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="غير متوافق مع قناة 40 ميجاهيرتز"
LOWEST_STR			="الأدنى"
MEDIUM_LOW_STR			="متوسط-منخفض"
MEDIUM_STR			="متوسط"
MEDIUM_HIGH_STR			="متوسط-مرتفع"
HIGHEST_STR			="الأعلى"
DISABLED_STR			="معطل"
ENABLED_STR 			="ممكَّن"
CTS_TO_SELF_ENABLED_STR     	="تمكين CTS الذاتي"
RTS_CTS_ENABLED_STR         	="تمكين RTS/CTS"
CHANNELWIDTH20ONLY          	="20 ميجاهيرتز"
CHANNELWIDTHAUTO            	="تلقائي"
WMM_DISABLED_STR            	="WMM معطل"
WMM_ENABLED_STR             	="WMM ممكَّن"
NO_PREFERECE_STR            	="بلا تفضيل"
PREFER_24_BAND_STR          	="يفضل مدى موجات 2.4 جيجاهيرتز"
PREFER_52_BAND_STR          	="يفضل مدى موجات 5.2 جيجاهيرتز"
WAKE_ON_MAGIC_PACKET        	="التنبيه عند الحزمة السحرية"
WAKE_ON_PATTERN_MATCH       	="التنبيه عند مطابقة النقش"
PM_WIFI_REKEY_OFFLOAD	    	="إعادة إنشاء مفتاح GTK لتنبيه WLAN"
PM_ARP_OFFLOAD			="توزيع نقل البيانات باستخدام ARP لتنبيه WLAN"
PM_NS_OFFLOAD			="توزيع نقل البيانات باستخدام NS لتنبيه WLAN"
DEVICE_SLEEP_ON_DISCONNECT	="السكون عند فصل تنبيه WLAN"
PACKET_COALESCING               ="إدماج الحزمة"
U_APSD_SUPPORT			="دعم U-APSD"
THROUGHPUTBOOSTER_STR   	="معزز معدل النقل"

SOURCEDISK1                     ="قرص تثبيت مجموعة Intel(R) Wireless"

[Strings.0804] ; Chinese (Simplified)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Intel(R) Wireless 适配器驱动程序（适用于 Windows 8.1 32 位）"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad Hoc 信道 802.11b/g"
IBSS_TX_POWER_STR           	="传输电源"
ROAMING_AGGRESSIVENESS_STR	="漫游主动性"
ADHOC_QOS_MODE_STR          	="Ad Hoc QoS 模式"
MIXED_MODE_PROTECTION_STR   	="混合模式保护"
WIRELESS_MODE_STR           	="无线模式"
PREFERRED_BAND_STR          	="首选频带"
CHANNELWIDTH52              	="5.2 GHz 802.11n 信道宽度"
CHANNELWIDTH24              	="2.4 GHz 802.11n 信道宽度"
TGnMode                     	="HT 模式"
VHT_ENABLED_STR			="VHT 模式"
HT_ENABLED_STR			="HT 模式"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="与 40Mhz 信道不兼容"
LOWEST_STR			="最低值"
MEDIUM_LOW_STR			="中低"
MEDIUM_STR			="中间"
MEDIUM_HIGH_STR			="中高"
HIGHEST_STR			="最高值"
DISABLED_STR			="已禁用"
ENABLED_STR 			="已启用"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self 已启用"
RTS_CTS_ENABLED_STR         	="RTS/CTS 已启用"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="自动"
WMM_DISABLED_STR            	="WMM 已禁用"
WMM_ENABLED_STR             	="WMM 已启用"
NO_PREFERECE_STR            	="无首选项"
PREFER_24_BAND_STR          	="首选 2.4 GHz 频带"
PREFER_52_BAND_STR          	="首选 5.2 GHz 频带"
WAKE_ON_MAGIC_PACKET        	="唤醒幻数据包"
WAKE_ON_PATTERN_MATCH       	="唤醒模式匹配"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN 的 GTK 重新生成密钥"
PM_ARP_OFFLOAD			="WoWLAN 的 ARP 卸载"
PM_NS_OFFLOAD			="WoWLAN 的 NS 卸载"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN 断开连接时睡眠"
PACKET_COALESCING               ="数据包合并"
U_APSD_SUPPORT			="支持 U-APSD "
THROUGHPUTBOOSTER_STR   	="吞吐量助推器"

SOURCEDISK1                     ="Intel(R) Wireless 系列安装盘"

[Strings.0404] ; Chinese (Traditional)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="用於 Windows 8.1 32 Bit 的 Intel(R) Wireless 介面卡驅動程式"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="點對點 (ad hoc) 通道 802.11b/g"
IBSS_TX_POWER_STR           	="傳輸電源"
ROAMING_AGGRESSIVENESS_STR	="漫遊積極度"
ADHOC_QOS_MODE_STR          	="點對點 (ad hoc) QoS 模式"
MIXED_MODE_PROTECTION_STR   	="混合模式保護"
WIRELESS_MODE_STR           	="無線模式"
PREFERRED_BAND_STR          	="偏好的頻帶"
CHANNELWIDTH52              	="802.11n 通道寬度 (5.2 GHz)"
CHANNELWIDTH24              	="802.11n 通道寬度 (2.4 GHz)"
TGnMode                     	="HT 模式"
VHT_ENABLED_STR			="VHT 模式"
HT_ENABLED_STR			="HT 模式"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="不容大量通道"
LOWEST_STR			="最低"
MEDIUM_LOW_STR			="中低"
MEDIUM_STR			="中"
MEDIUM_HIGH_STR			="中高"
HIGHEST_STR			="最高"
DISABLED_STR			="停用"
ENABLED_STR 			="啟用"
CTS_TO_SELF_ENABLED_STR     	="啟用 CTS-to-self"
RTS_CTS_ENABLED_STR         	="啟用 RTS/CTS"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="自動"
WMM_DISABLED_STR            	="WMM 停用"
WMM_ENABLED_STR             	="WMM 啟用"
NO_PREFERECE_STR            	="無偏好設定"
PREFER_24_BAND_STR          	="喜好 2.4 GHz 頻帶"
PREFER_52_BAND_STR          	="喜好 5.2 GHz 頻帶"
WAKE_ON_MAGIC_PACKET        	="收到 Magic 封包時喚醒"
WAKE_ON_PATTERN_MATCH       	="收到模式對應時喚醒"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN GTK 金鑰重建"
PM_ARP_OFFLOAD			="WoWLAN ARP 卸載"
PM_NS_OFFLOAD			="WoWLAN NS 卸載"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN 中斷連線時睡眠"
PACKET_COALESCING               ="封包聯合"
U_APSD_SUPPORT			="U-APSD 支援"
THROUGHPUTBOOSTER_STR   	="傳輸加速"

SOURCEDISK1                     ="Intel(R) Wireless 系列安裝磁碟"

[Strings.0C04] ; Chinese (Hong Kong)

PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="用於 Windows 8.1 32 Bit 的 Intel(R) Wireless 介面卡驅動程式"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="點對點 (ad hoc) 通道 802.11b/g"
IBSS_TX_POWER_STR           	="傳輸電源"
ROAMING_AGGRESSIVENESS_STR	="漫遊積極度"
ADHOC_QOS_MODE_STR          	="點對點 (ad hoc) QoS 模式"
MIXED_MODE_PROTECTION_STR   	="混合模式保護"
WIRELESS_MODE_STR           	="無線模式"
PREFERRED_BAND_STR          	="偏好的頻帶"
CHANNELWIDTH52              	="802.11n 通道寬度 (5.2 GHz)"
CHANNELWIDTH24              	="802.11n 通道寬度 (2.4 GHz)"
TGnMode                     	="HT 模式"

VHT_ENABLED_STR			="VHT 模式"
HT_ENABLED_STR			="HT 模式"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="不容大量通道"
LOWEST_STR			="最低"
MEDIUM_LOW_STR			="中低"
MEDIUM_STR			="中"
MEDIUM_HIGH_STR			="中高"
HIGHEST_STR			="最高"
DISABLED_STR			="停用"
ENABLED_STR 			="啟用"
CTS_TO_SELF_ENABLED_STR     	="啟用 CTS-to-self"
RTS_CTS_ENABLED_STR         	="啟用 RTS/CTS"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="自動"
WMM_DISABLED_STR            	="WMM 停用"
WMM_ENABLED_STR             	="WMM 啟用"
NO_PREFERECE_STR            	="無偏好設定"
PREFER_24_BAND_STR          	="喜好 2.4 GHz 頻帶"
PREFER_52_BAND_STR          	="喜好 5.2 GHz 頻帶"
WAKE_ON_MAGIC_PACKET        	="收到 Magic 封包時喚醒"
WAKE_ON_PATTERN_MATCH       	="收到模式對應時喚醒"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN GTK 金鑰重建"
PM_ARP_OFFLOAD			="WoWLAN ARP 卸載"
PM_NS_OFFLOAD			="WoWLAN NS 卸載"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN 中斷連線時睡眠"
PACKET_COALESCING               ="封包聯合"
U_APSD_SUPPORT			="U-APSD 支援"
THROUGHPUTBOOSTER_STR   	="傳輸加速"

SOURCEDISK1                     ="Intel(R) Wireless 系列安裝磁碟"

[Strings.0405] ; Czech (Czech Republic)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Ovladač adaptéru Intel(R) Wireless pro systém Windows 8.1 32 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Kanál ad hoc 802.11b/g"
IBSS_TX_POWER_STR           	="Vysílací energie"
ROAMING_AGGRESSIVENESS_STR	="Agresivita roamingu"
ADHOC_QOS_MODE_STR          	="Režim Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   	="Ochrana smíšeného režimu"
WIRELESS_MODE_STR           	="Bezdrátový režim"
PREFERRED_BAND_STR          	="Upřednostňované pásmo"
CHANNELWIDTH52              	="Šířka kanálu 802.11n pro 5,2 GHz"
CHANNELWIDTH24              	="Šířka kanálu 802.11n pro 2,4 GHz"
TGnMode                     	="Režim HT"
VHT_ENABLED_STR			="Režim VHT"
HT_ENABLED_STR			="Režim HT"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Nekompatibilní s šířkou kanálu 40 MHz"
LOWEST_STR			="Nejnižší"
MEDIUM_LOW_STR			="Středně nízký"
MEDIUM_STR			="Střední"
MEDIUM_HIGH_STR			="Středně vysoký"
HIGHEST_STR			="Nejvyšší"
DISABLED_STR			="Zakázáno"
ENABLED_STR 			="Povoleno"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self povoleno"
RTS_CTS_ENABLED_STR         	="RTS/CTS povoleno"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automaticky"
WMM_DISABLED_STR            	="WMM zakázáno"
WMM_ENABLED_STR             	="WMM povoleno"
NO_PREFERECE_STR            	="Žádná předvolba"
PREFER_24_BAND_STR          	="Upřednostňovat pásmo 2,4 GHz"
PREFER_52_BAND_STR          	="Upřednostňovat pásmo 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Probuzení paketem Magic"
WAKE_ON_PATTERN_MATCH       	="Probuzení porovnávacím vzorkem"
PM_WIFI_REKEY_OFFLOAD	    	="Vystavování nových klíčů GTK pro technologii WoWLAN"
PM_ARP_OFFLOAD			="Snižování zatížení ARP pro technologii WoWLAN"
PM_NS_OFFLOAD			="Snižování zatížení NS pro technologii WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Režim spánku při odpojení technologie WoWLAN"
PACKET_COALESCING               ="Slučování paketů"
U_APSD_SUPPORT			="Podpora U-APSD"
THROUGHPUTBOOSTER_STR   	="Podpora průchodnosti"

SOURCEDISK1                     ="Instalační disk adaptéru řady Intel(R) Wireless"

[Strings.0406] ; Danish (Denmark)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Intel(R) Wireless adapter driver til Windows 8.1 32 Bit "

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad hoc-kanal 802.11b/g"
IBSS_TX_POWER_STR           	="Sendeeffekt"
ROAMING_AGGRESSIVENESS_STR	="Roaming-aggressivitet"
ADHOC_QOS_MODE_STR          	="Ad Hoc QoS-tilstand"
MIXED_MODE_PROTECTION_STR   	="Beskyttelse til blandet miljø"
WIRELESS_MODE_STR           	="Trådløs tilstand"
PREFERRED_BAND_STR          	="Foretrukket bånd"
CHANNELWIDTH52              	="802.11n kanalbredde for 5,2 GHz"
CHANNELWIDTH24              	="802.11n kanalbredde for 2,4 GHz"
TGnMode                     	="HT tilstand"
VHT_ENABLED_STR			="VHT tilstand"
HT_ENABLED_STR			="HT tilstand"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="40Mhz kanal intolerant"
LOWEST_STR			="Laveste"
MEDIUM_LOW_STR			="Mellem-lav"
MEDIUM_STR			="Mellem"
MEDIUM_HIGH_STR			="Mellem-høj"
HIGHEST_STR			="Højeste"
DISABLED_STR			="Deaktiveret"
ENABLED_STR 			="Aktiveret"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self aktiveret "
RTS_CTS_ENABLED_STR         	="RTS/CTS aktiveret "
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM deaktiveret"
WMM_ENABLED_STR             	="WMM aktiveret"
NO_PREFERECE_STR            	="Ingen indstilling"
PREFER_24_BAND_STR          	="Foretræk 2,4 GHz bånd"
PREFER_52_BAND_STR          	="Foretræk 5,2 GHz bånd"
WAKE_ON_MAGIC_PACKET        	="Vækning ved magisk pakke"
WAKE_ON_PATTERN_MATCH       	="Vækning ved mønstermatch"
PM_WIFI_REKEY_OFFLOAD	    	="GTK-nøglefornyelse til WoWLAN"
PM_ARP_OFFLOAD			="ARP-aflastning til WoWLAN"
PM_NS_OFFLOAD			="NS-aflastning til WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Slumring ved afbrydelse af WoWLAN"
PACKET_COALESCING               ="Pakke-samling"
U_APSD_SUPPORT			="U-APSD Support"
THROUGHPUTBOOSTER_STR   	="Gennemløbsforstærker"

SOURCEDISK1                     ="Intel(R) Wireless installationsdisk"

[Strings.0407] ; German (Germany)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Intel(R) Wireless Adaptertreiber für Windows 8.1 32-Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad-Hoc-Kanal 802.11b/g"
IBSS_TX_POWER_STR           	="Übertragungsleistung"
ROAMING_AGGRESSIVENESS_STR	="Roaming-Dynamik"
ADHOC_QOS_MODE_STR          	="Ad-Hoc QoS-Modus"
MIXED_MODE_PROTECTION_STR   	="Schutz f. gemischte Umgebungen"
WIRELESS_MODE_STR           	="Drahtloser Modus"
PREFERRED_BAND_STR          	="Bevorzugtes Band"
CHANNELWIDTH52              	="802.11n Kanalbreite für 5.2 GHz"
CHANNELWIDTH24              	="802.11n Kanalbreite für 2.4 GHz"
TGnMode                     	="HT Modus"
VHT_ENABLED_STR			="VHT Modus"
HT_ENABLED_STR			="HT Modus"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Fat Kanal Intolerant"
LOWEST_STR			="Am niedrigsten"
MEDIUM_LOW_STR			="Mittel-niedrig"
MEDIUM_STR			="Mittel"
MEDIUM_HIGH_STR			="Mittel-hoch"
HIGHEST_STR			="Am höchsten"
DISABLED_STR			="Deaktiviert"
ENABLED_STR 			="Aktiviert"
CTS_TO_SELF_ENABLED_STR     	="'CTS-to-self' aktiviert"
RTS_CTS_ENABLED_STR         	="RTS/CTS aktiviert"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM deaktiviert"
WMM_ENABLED_STR             	="WMM aktiviert"
NO_PREFERECE_STR            	="Keine Einstellung"
PREFER_24_BAND_STR          	="2,4-GHz-Band bevorzugen"
PREFER_52_BAND_STR          	="5,2-GHz-Band bevorzugen"
WAKE_ON_MAGIC_PACKET        	="Aktivierung durch Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Aktivierung durch Musterübereinstimmung"
PM_WIFI_REKEY_OFFLOAD	    	="GTK führt Neuverschlüsselung für WoWLAN durch"
PM_ARP_OFFLOAD			="ARP-Offload für WoWLAN"
PM_NS_OFFLOAD			="NS-Offload für WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Medientrennung beim Aufrechterhalten des Energiesparmodus von WoWLAN"
PACKET_COALESCING               ="Paketzusammenfügung"
U_APSD_SUPPORT			="U-APSD-Unterstützung"
THROUGHPUTBOOSTER_STR   	="Durchsatzbooster"

SOURCEDISK1                     ="Intel(R) Wireless - Installationsdiskette"

[Strings.0408] ; Greek (Greece)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Πρόγραμμα οδήγησης προσαρμογέα Intel(R) Wireless για Windows 8.1 32 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Κανάλι ad hoc 802.11b/g"
IBSS_TX_POWER_STR           	="Ισχύς μετάδοσης"
ROAMING_AGGRESSIVENESS_STR	="Δυναμικότητα περιαγωγής"
ADHOC_QOS_MODE_STR          	="Τρόπος λειτουργίας Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   	="Προστασία μεικτής λειτουργίας"
WIRELESS_MODE_STR           	="Ασύρματη κατάσταση"
PREFERRED_BAND_STR          	="Προτιμώμενη ζώνη"
CHANNELWIDTH52              	="Εύρος καναλιού 802.11n για 5.2 GHz"
CHANNELWIDTH24              	="Εύρος καναλιού 802.11n για 2.4 GHz"
TGnMode                     	="Λειτουργία HT"
VHT_ENABLED_STR			="Λειτουργία VHT"
HT_ENABLED_STR			="Λειτουργία HT"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Μη συμβατό με ισχυρά κανάλια"
LOWEST_STR			="Χαμηλότερη"
MEDIUM_LOW_STR			="Μεσαία-Χαμηλή"
MEDIUM_STR			="Μεσαία"
MEDIUM_HIGH_STR			="Μεσαία-Υψηλή"
HIGHEST_STR			="Υψηλότερη"
DISABLED_STR			="Απενεργοποιημένη"
ENABLED_STR 			="Ενεργοποιημένη"
CTS_TO_SELF_ENABLED_STR     	="Ενεργοποιημένο CTS-to-self"
RTS_CTS_ENABLED_STR         	="Ενεργοποιημένο RTS/CTS"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Αυτόματα"
WMM_DISABLED_STR            	="Απενεργοποιημένη WMM"
WMM_ENABLED_STR             	="Ενεργοποιημένη WMM"
NO_PREFERECE_STR            	="Καμία προτίμηση"
PREFER_24_BAND_STR          	="Προτίμηση ζώνη 2,4 GHz"
PREFER_52_BAND_STR          	="Προτίμηση ζώνη 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Ενεργοποίηση με Μαγικό πακέτο"
WAKE_ON_PATTERN_MATCH       	="Ενεργοποίηση με αντιστοίχιση μοτίβου"
PM_WIFI_REKEY_OFFLOAD	    	="Το GTK ζητά τη δημιουργία νέου κλειδιού για WoWLAN"
PM_ARP_OFFLOAD			="Μείωση φόρτου ARP για WoWLAN"
PM_NS_OFFLOAD			="Μείωση φόρτου NS για WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Αναστολή λειτουργίας κατά την αποσύνδεση του WoWLAN"
PACKET_COALESCING               ="Ενοποίηση πακέτων"
U_APSD_SUPPORT			="Υποστήριξη U-APSD"
THROUGHPUTBOOSTER_STR   	="Ενισχυτής μετάδοσης"

SOURCEDISK1                     ="Δισκέτα εγκατάστασης Intel(R) Wireless"

[Strings.0C0A] ; Spanish (Spain)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Controlador del adaptador Intel(R) Wireless para Windows 8.1 de 32 bits"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Canal Ad Hoc 802.11b/g"
IBSS_TX_POWER_STR           	="Potencia de transmisión"
ROAMING_AGGRESSIVENESS_STR	="Agresividad de itinerancia"
ADHOC_QOS_MODE_STR          	="Modo QoS Ad Hoc"
MIXED_MODE_PROTECTION_STR   	="Protección de modo mixto"
WIRELESS_MODE_STR           	="Modo inalámbrico"
PREFERRED_BAND_STR          	="Banda preferida"
CHANNELWIDTH52              	="Ancho de canal 802.11n para 5,2 GHz"
CHANNELWIDTH24              	="Ancho de canal 802.11n para 2,4 GHz"
TGnMode                     	="Modo HT"
VHT_ENABLED_STR			="Modo VHT"
HT_ENABLED_STR			="Modo HT"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="No compatible con canal de 40 MHz"
LOWEST_STR			="Mínimo"
MEDIUM_LOW_STR			="Bajo"
MEDIUM_STR			="Mediano"
MEDIUM_HIGH_STR			="Alto"
HIGHEST_STR			="Máximo"
DISABLED_STR			="Desactivado"
ENABLED_STR 			="Activado"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self activado"
RTS_CTS_ENABLED_STR         	="RTS/CTS activado"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automático"
WMM_DISABLED_STR            	="WMM desactivado"
WMM_ENABLED_STR             	="WMM activado"
NO_PREFERECE_STR            	="Sin preferencias"
PREFER_24_BAND_STR          	="Preferir la banda de 2,4 GHz"
PREFER_52_BAND_STR          	="Preferir la banda de 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Magic Packet de reactivación"
WAKE_ON_PATTERN_MATCH       	="Coincidencia de patrones de reactivación"
PM_WIFI_REKEY_OFFLOAD	    	="Regeneración de clave GTK para WoWLAN"
PM_ARP_OFFLOAD			="Descarga ARP para WoWLAN"
PM_NS_OFFLOAD			="Descarga NS para WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Suspensión al desconectar WoWLAN"
PACKET_COALESCING               ="Fusión de paquetes"
U_APSD_SUPPORT			="Soporte de U-APSD"
THROUGHPUTBOOSTER_STR   	="Impulsar la capacidad de proceso"

SOURCEDISK1                     ="Disco de instalación de Intel(R) Wireless"

[Strings.040B] ; Finnish (Finland)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Intel(R) Wireless -sovitinohjain Windows 8.1 32-bit -käyttöjärjestelmään"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad Hoc -kanava 802.11b/g"
IBSS_TX_POWER_STR           	="Lähetysteho"
ROAMING_AGGRESSIVENESS_STR	="Solukonpäivitysaktiivisuus"
ADHOC_QOS_MODE_STR          	="Ad Hoc QoS -tila"
MIXED_MODE_PROTECTION_STR   	="Sekatilan Suojaus"
WIRELESS_MODE_STR           	="Langaton tila"
PREFERRED_BAND_STR          	="Ensisijainen kaista"
CHANNELWIDTH52              	="802.11n-kanavaleveys 5,2 GHz"
CHANNELWIDTH24              	="802.11n-kanavaleveys 2,4 GHz"
TGnMode                     	="HT-tila"
VHT_ENABLED_STR			="VHT-tila"
HT_ENABLED_STR			="HT-tila"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Fat Channel -esto"
LOWEST_STR			="Pienin"
MEDIUM_LOW_STR			="Kohtalainen-pieni"
MEDIUM_STR			="Kohtalainen"
MEDIUM_HIGH_STR			="Kohtalainen-suuri"
HIGHEST_STR			="Suurin"
DISABLED_STR			="Poissa käytöstä"
ENABLED_STR 			="Käytössä"
CTS_TO_SELF_ENABLED_STR     	="CTS itselle käytössä"
RTS_CTS_ENABLED_STR         	="RTS/CTS käytössä"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automaattinen"
WMM_DISABLED_STR            	="WMM poissa käytöstä"
WMM_ENABLED_STR             	="WMM käytössä"
NO_PREFERECE_STR            	="Ei ensisijaisuutta"
PREFER_24_BAND_STR          	="2,4 GHz:n kaista ensisijainen"
PREFER_52_BAND_STR          	="5,2 GHz:n kaista ensisijainen"
WAKE_ON_MAGIC_PACKET        	="Aktivointi Magic-paketilla"
WAKE_ON_PATTERN_MATCH       	="Aktivointi mallivastaavuudella"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN-toiminnon GTK-uudelleenavainnus "
PM_ARP_OFFLOAD			="WoWLAN-toiminnon ARP-purku"
PM_NS_OFFLOAD			="WoWLAN-toiminnon NS-purku"
DEVICE_SLEEP_ON_DISCONNECT	="Lepotilaan, kun WoWLAN-yhteys katkaistu"
PACKET_COALESCING               ="Pakettien yhdistäminen"
U_APSD_SUPPORT			="U-APSD-tuki"
THROUGHPUTBOOSTER_STR   	="Siirtomäärän tehostus"

SOURCEDISK1                     ="Intel(R) Wireless asennuslevy"

[Strings.040C] ; French (France)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Pilote de carte Intel(R) Wireless pour Windows 8.1 32 bits "

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Canal ad hoc 802.11b/g"
IBSS_TX_POWER_STR           	="Puissance de transmission"
ROAMING_AGGRESSIVENESS_STR	="Agressivité de l’itinérance"
ADHOC_QOS_MODE_STR          	="Mode Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   	="Protection en mode mixte"
WIRELESS_MODE_STR           	="Mode Sans fil"
PREFERRED_BAND_STR          	="Bande privilégiée"
CHANNELWIDTH52              	="Largeur de canal 802.11n - 5,2 GHz"
CHANNELWIDTH24              	="Largeur de canal 802.11n - 2,4 GHz"
TGnMode                     	="Mode HT"
VHT_ENABLED_STR			="Mode VHT"
HT_ENABLED_STR			="Mode HT"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Incompatible avec canaux de 40 MHz"
LOWEST_STR			="Min."
MEDIUM_LOW_STR			="Faible"
MEDIUM_STR			="Moyenne"
MEDIUM_HIGH_STR			="Élevée"
HIGHEST_STR			="Max."
DISABLED_STR			="Désactivé(e)"
ENABLED_STR 			="Activé(e)"
CTS_TO_SELF_ENABLED_STR     	="Auto-CTS activée"
RTS_CTS_ENABLED_STR         	="RTS/CTS activée"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM désactivée"
WMM_ENABLED_STR             	="WMM activée"
NO_PREFERECE_STR            	="Aucune préférence"
PREFER_24_BAND_STR          	="Préférer bande 2,4 GHz"
PREFER_52_BAND_STR          	="Préférer bande 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Correspondance au modèle WOL"
PM_WIFI_REKEY_OFFLOAD	    	="Régénération des clés GTK pour WoWLAN"
PM_ARP_OFFLOAD			="Délestage ARP pour WoWLAN"
PM_NS_OFFLOAD			="Délestage NS pour WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Veille à la déconnexion WoWLAN"
PACKET_COALESCING               ="Fusion des paquets"
U_APSD_SUPPORT			="Assistance U-APSD"
THROUGHPUTBOOSTER_STR   	="Multiplicateur de débit"

SOURCEDISK1                     ="Disque d'installation de Intel(R) Wireless"

[Strings.040D] ; Hebrew (Israel)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="מנהל התקן של מתאם Intel(R) Wireless עבור Windows 8.1 32 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="ערוץ אד הוק 802.11b/g"
IBSS_TX_POWER_STR           	="עוצמת שידור"
ROAMING_AGGRESSIVENESS_STR	="תוקפנות נדידה"
ADHOC_QOS_MODE_STR          	="מצב QoS אד-הוק"
MIXED_MODE_PROTECTION_STR   	="הגנת מצב מעורב"
WIRELESS_MODE_STR           	="מצב אלחוטי"
PREFERRED_BAND_STR          	="פס מועדף"
CHANNELWIDTH52              	="רוחב ערוץ 802.11n עבור 5.2 GHz"
CHANNELWIDTH24              	="רוחב ערוץ 802.11n עבור 2.4 GHz"
TGnMode                     	="מצב HT"
VHT_ENABLED_STR			="מצב VHT"
HT_ENABLED_STR			="מצב HT"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="לא תואם לערוץ 40Mhz"
LOWEST_STR			="נמוך ביותר"
MEDIUM_LOW_STR			="בינוני-נמוך"
MEDIUM_STR			="בינוני"
MEDIUM_HIGH_STR			="בינוני-גבוה"
HIGHEST_STR			="גבוה ביותר"
DISABLED_STR			="מנוטרל"
ENABLED_STR 			="זמין"
CTS_TO_SELF_ENABLED_STR     	="מאופשר CTS-אל-עצמו"
RTS_CTS_ENABLED_STR         	="מאופשר RTS/CTS"
CHANNELWIDTH20ONLY          	="‎20 MHz"
CHANNELWIDTHAUTO            	="אוטומטי"
WMM_DISABLED_STR            	="WMM מנוטרל"
WMM_ENABLED_STR             	="WMM זמין"
NO_PREFERECE_STR            	="אין העדפה"
PREFER_24_BAND_STR          	="העדפת פס ‎2.4 GHz"
PREFER_52_BAND_STR          	="העדפת פס ‎5.2 GHz"
WAKE_ON_MAGIC_PACKET        	="התעורר בעת מנת Magic"
WAKE_ON_PATTERN_MATCH       	="התעורר בעת התאמת תבנית"
PM_WIFI_REKEY_OFFLOAD	    	="החלפת מפתחות GTK עבור WoWLAN"
PM_ARP_OFFLOAD			="העברת ARP עבור WoWLAN"
PM_NS_OFFLOAD			="העברת NS עבור WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="כניסה למצב שינה עם ניתוק WoWLAN"
PACKET_COALESCING               ="מיזוג מנה"
U_APSD_SUPPORT			="תמיכה ב- U-APSD"
THROUGHPUTBOOSTER_STR   	="הגברת תפוקה"

SOURCEDISK1                     ="דיסק התקנה של Intel(R) Wireless"

[Strings.040E] ; Hungarian (Hungary)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Intel(R) Wireless adapter illesztőprogram 32 bites Windows 8.1"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Alkalmi csatorna 802.11b/g"
IBSS_TX_POWER_STR           	="Sugárzási teljesítmény"
ROAMING_AGGRESSIVENESS_STR	="A barangolás intenzitása"
ADHOC_QOS_MODE_STR          	="Alkalmi QoS üzemmód"
MIXED_MODE_PROTECTION_STR   	="Vegyes üzemmódú védelem"
WIRELESS_MODE_STR           	="Vezeték nélküli üzemmód"
PREFERRED_BAND_STR          	="Preferált frekvenciasáv"
CHANNELWIDTH52              	="802.11n csatornaszélesség a 5,2 GHz"
CHANNELWIDTH24              	="802.11n csatornaszélesség a 2,4GHz"
TGnMode                     	="HT üzemmód"
VHT_ENABLED_STR			="VHT üzemmód"
HT_ENABLED_STR			="HT üzemmód"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Csökkentett sávszélességen működik"
LOWEST_STR			="Legalacsonyabb"
MEDIUM_LOW_STR			="Közepes - alacsony"
MEDIUM_STR			="Közepes"
MEDIUM_HIGH_STR			="Közepes - magas"
HIGHEST_STR			="Legmagasabb"
DISABLED_STR			="Letiltva"
ENABLED_STR 			="Engedélyezve"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self engedélyezve"
RTS_CTS_ENABLED_STR         	="RTS/CTS engedélyezve"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM letiltva"
WMM_ENABLED_STR             	="WMM engedélyezve"
NO_PREFERECE_STR            	="Nincs preferencia"
PREFER_24_BAND_STR          	="2,4 GHz-es sáv preferálása"
PREFER_52_BAND_STR          	="5,2 GHz-es sáv preferálása"
WAKE_ON_MAGIC_PACKET        	="Ébresztés magic-csomaggal"
WAKE_ON_PATTERN_MATCH       	="Ébresztés mintaegyezésre"
PM_WIFI_REKEY_OFFLOAD	    	="GTK újrakulcsolás WoWLAN hálózathoz"
PM_ARP_OFFLOAD			="ARP tehermentesítés WoWLAN hálózathoz"
PM_NS_OFFLOAD			="NS tehermentesítés WoWLAN hálózathoz"
DEVICE_SLEEP_ON_DISCONNECT	="Alvó állapot WoWLAN hálózati szétkapcsolás esetén"
PACKET_COALESCING               ="Csomagegyesítés"
U_APSD_SUPPORT			="U-APSD támogatás"
THROUGHPUTBOOSTER_STR   	="Átviteli sebesség növelés "

SOURCEDISK1                     ="Intel(R) Wireless telepítő lemez"

[Strings.0410] ; Italian (Italy)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Driver scheda Intel(R) Wireless per Windows 8.1 32 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Canale Ad Hoc 802.11b/g"
IBSS_TX_POWER_STR           	="Potenza di trasmissione"
ROAMING_AGGRESSIVENESS_STR	="Efficacia roaming"
ADHOC_QOS_MODE_STR          	="Modalità Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   	="Protezione a modalità mista"
WIRELESS_MODE_STR           	="Modalità wireless"
PREFERRED_BAND_STR          	="Banda preferita"
CHANNELWIDTH52              	="Larg. canale 802.11n per 5,2 GHz"
CHANNELWIDTH24              	="Larg. canale 802.11n per 2,4 GHz"
TGnMode                     	="Modalità HT"
VHT_ENABLED_STR			="Modalità VHT"
HT_ENABLED_STR			="Modalità HT"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Fat Channel incompatibile"
LOWEST_STR			="Minimo"
MEDIUM_LOW_STR			="Medio-basso"
MEDIUM_STR			="Medio"
MEDIUM_HIGH_STR			="Medio-alto"
HIGHEST_STR			="Massimo"
DISABLED_STR			="Disattivata"
ENABLED_STR 			="Attivata"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self attivato"
RTS_CTS_ENABLED_STR         	="Attivato RTS/CTS"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM disattivata"
WMM_ENABLED_STR             	="WMM attivata"
NO_PREFERECE_STR            	="Nessuna preferenza"
PREFER_24_BAND_STR          	="Preferenza a banda a 2,4 GHz"
PREFER_52_BAND_STR          	="Preferenza a banda a 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Magic Packet per riattivazione"
WAKE_ON_PATTERN_MATCH       	="Corrispondenza motivo per riattivazione"
PM_WIFI_REKEY_OFFLOAD	    	="Rigenerazione delle chiavi GTK per WoWLAN"
PM_ARP_OFFLOAD			="Offload ARP per WoWLAN"
PM_NS_OFFLOAD			="Offload NS per WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Sospensione attiva alla disconnessione da WoWLAN"
PACKET_COALESCING               ="Unione pacchetti"
U_APSD_SUPPORT			="Supporto U-APSD"
THROUGHPUTBOOSTER_STR   	="Incremento del throughput"

SOURCEDISK1                     ="Disco di installazione per Intel(R) Wireless"

[Strings.0411] ; Japanese (Japan)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Windows 8.1 32 ビット用 Intel(R) Wireless アダプタードライバー"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="アドホック チャネル 802.11b/g "
IBSS_TX_POWER_STR           	="送信パワー"
ROAMING_AGGRESSIVENESS_STR	="ローミングの積極性"
ADHOC_QOS_MODE_STR          	="アドホック QoS モード"
MIXED_MODE_PROTECTION_STR   	="混在モード保護"
WIRELESS_MODE_STR           	="ワイヤレス モード"
PREFERRED_BAND_STR          	="優先バンド"
CHANNELWIDTH52              	="5.2 GHz 用 802.11n チャネル幅"
CHANNELWIDTH24              	="2.4 GHz 用 802.11n チャネル幅"
TGnMode                     	="HT モード"
VHT_ENABLED_STR			="VHT モード"
HT_ENABLED_STR			="HT モード"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="40Mhz チャネル幅非互換"
LOWEST_STR			="最低"
MEDIUM_LOW_STR			="中低"
MEDIUM_STR			="中"
MEDIUM_HIGH_STR			="中高"
HIGHEST_STR			="最高"
DISABLED_STR			="無効"
ENABLED_STR 			="有効"
CTS_TO_SELF_ENABLED_STR     	="個別 CTS 有効"
RTS_CTS_ENABLED_STR         	="RTS/CTS 有効"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="自動"
WMM_DISABLED_STR            	="WMM 無効"
WMM_ENABLED_STR             	="WMM 有効"
NO_PREFERECE_STR            	="優先順位なし"
PREFER_24_BAND_STR          	="2.4 GHz バンドの優先"
PREFER_52_BAND_STR          	="5.2 GHz バンドの優先"
WAKE_ON_MAGIC_PACKET        	="Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Wake on Pattern Match"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN の GTK Rekey"
PM_ARP_OFFLOAD			="WoWLAN の ARP オフロード"
PM_NS_OFFLOAD			="WoWLAN の NS オフロード"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN のスリープ状態の解除"
PACKET_COALESCING               ="パケット結合"
U_APSD_SUPPORT			="U-APSD 対応"
THROUGHPUTBOOSTER_STR   	="スループット・ブースター"

SOURCEDISK1                     ="Intel(R) Wireless インストール・ディスク"

[Strings.0412] ; Korean (Korea)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Windows 8.1 32비트용 Intel(R) Wireless 어댑터 드라이버"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad Hoc 채널 802.11b/g"
IBSS_TX_POWER_STR           	="전송 전원"
ROAMING_AGGRESSIVENESS_STR	="로밍의 주동성"
ADHOC_QOS_MODE_STR          	="Ad Hoc QoS 모드"
MIXED_MODE_PROTECTION_STR   	="혼합 모드 보호"
WIRELESS_MODE_STR           	="무선 모드"
PREFERRED_BAND_STR          	="기본 설정 밴드"
CHANNELWIDTH52              	="5.2 GHz에 대한 802.11n 채널 폭"
CHANNELWIDTH24              	="2.4 GHz에 대한 802.11n 채널 폭"
TGnMode                     	="HT 모드"
VHT_ENABLED_STR			="VHT 모드"
HT_ENABLED_STR			="HT 모드"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="과부하 채널 비지원"
LOWEST_STR			="최하"
MEDIUM_LOW_STR			="보통-낮음"
MEDIUM_STR			="보통"
MEDIUM_HIGH_STR			="보통-높음"
HIGHEST_STR			="최고"
DISABLED_STR			="비활성화함"
ENABLED_STR 			="활성화함"
CTS_TO_SELF_ENABLED_STR     	="자체 CTS 활성화함"
RTS_CTS_ENABLED_STR         	="RTS/CTS 활성화함"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="자동"
WMM_DISABLED_STR            	="WMM 비활성화함"
WMM_ENABLED_STR             	="WMM 활성화함"
NO_PREFERECE_STR            	="기본 설정 없음"
PREFER_24_BAND_STR          	="2.4 GHz 밴드 선택"
PREFER_52_BAND_STR          	="5.2 GHz 밴드 선택"
WAKE_ON_MAGIC_PACKET        	="Wake on 매직 패킷"
WAKE_ON_PATTERN_MATCH       	="Wake on 패턴 일치"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN에 대한 GTK 키 재입력"
PM_ARP_OFFLOAD			="WoWLAN에 대한 ARP 오프로드"
PM_NS_OFFLOAD			="WoWLAN에 대한 NS 오프로드"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN 연결 해제 시 절전 상태"
PACKET_COALESCING               ="패킷 통합"
U_APSD_SUPPORT			="U-APSD 지원"
THROUGHPUTBOOSTER_STR   	="처리량 부스터"

SOURCEDISK1                     ="Intel(R) Wireless 시리즈 설치 디스크"

[Strings.0413] ; Dutch (Netherlands)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Intel(R) Wireless adapter stuurprogramma onder Windows 8.1 32 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad-hockanaal 802.11b/g"
IBSS_TX_POWER_STR           	="Verzendenergie"
ROAMING_AGGRESSIVENESS_STR	="Agressiviteit bij roamen"
ADHOC_QOS_MODE_STR          	="Ad-hoc QoS-modus"
MIXED_MODE_PROTECTION_STR   	="Beveiliging van gemengde modus"
WIRELESS_MODE_STR           	="Draadloze modus"
PREFERRED_BAND_STR          	="Voorkeursband"
CHANNELWIDTH52              	="802.11n-kanaalbreedte voor 5.2 GHz"
CHANNELWIDTH24              	="802.11n-kanaalbreedte voor 2.4 GHz"
TGnMode                     	="HT-modus"
VHT_ENABLED_STR			="VHT-modus"
HT_ENABLED_STR			="HT-modus"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Niet compatibel met 40-Mhz kanaal"
LOWEST_STR			="Laagste"
MEDIUM_LOW_STR			="Laag"
MEDIUM_STR			="Normaal"
MEDIUM_HIGH_STR			="Hoog"
HIGHEST_STR			="Hoogste"
DISABLED_STR			="Uitgeschakeld"
ENABLED_STR 			="Ingeschakeld"
CTS_TO_SELF_ENABLED_STR     	="CTS-naar-zelf ingeschakeld"
RTS_CTS_ENABLED_STR         	="RTS/CTS ingeschakeld"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automatisch"
WMM_DISABLED_STR            	="WMM uitgeschakeld"
WMM_ENABLED_STR             	="WMM ingeschakeld"
NO_PREFERECE_STR            	="Geen voorkeur"
PREFER_24_BAND_STR          	="Voorkeur voor 2,4-GHz band"
PREFER_52_BAND_STR          	="Voorkeur voor 5,2-GHz band"
WAKE_ON_MAGIC_PACKET        	="Activeren na Magic-pakket"
WAKE_ON_PATTERN_MATCH       	="patroonovereenkomst"
PM_WIFI_REKEY_OFFLOAD	    	="GTK opnieuw versleutelen voor WoWLAN"
PM_ARP_OFFLOAD			="ARP-offload voor WoWLAN"
PM_NS_OFFLOAD			="NS-offload voor WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Slapen bij verbroken WoWLAN-verbinding"
PACKET_COALESCING               ="Pakketsamenvoeging"
U_APSD_SUPPORT			="U-APSD ondersteuning"
THROUGHPUTBOOSTER_STR   	="Throughput booster"

SOURCEDISK1                     ="Installatieschijf voor Intel(R) Wireless"

[Strings.0414] ; Norwegian (Bokmål) (Norway)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Intel(R) Wireless kortdriver for Windows 8.1 32-bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad Hoc-kanal 802.11b/g"
IBSS_TX_POWER_STR           	="Overføringsstrøm"
ROAMING_AGGRESSIVENESS_STR	="Streifingsaggresjon"
ADHOC_QOS_MODE_STR          	="Ad Hoc QoS modus"
MIXED_MODE_PROTECTION_STR   	="Blandet modus-beskyttelse"
WIRELESS_MODE_STR           	="Trådløsmodus"
PREFERRED_BAND_STR          	="Foretrukket bånd"
CHANNELWIDTH52              	="802.11n-kanalbredde for 5.2 GHz"
CHANNELWIDTH24              	="802.11n-kanalbredde for 2.4 GHz"
TGnMode                     	="HT-modus"
VHT_ENABLED_STR			="VHT-modus"
HT_ENABLED_STR			="HT-modus"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Intolerant for kanal"
LOWEST_STR			="Laveste"
MEDIUM_LOW_STR			="Middels-lav"
MEDIUM_STR			="Middels"
MEDIUM_HIGH_STR			="Middels-høy"
HIGHEST_STR			="Høyeste"
DISABLED_STR			="Deaktivert"
ENABLED_STR 			="Aktivert"
CTS_TO_SELF_ENABLED_STR     	="CTS-til-selv aktivert"
RTS_CTS_ENABLED_STR         	="RTS/CTS-aktivert"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automatisk"
WMM_DISABLED_STR            	="WMM deaktivert"
WMM_ENABLED_STR             	="WMM aktivert"
NO_PREFERECE_STR            	="Ingen preferanser"
PREFER_24_BAND_STR          	="Foretrekk 2,4 GHz-bånd"
PREFER_52_BAND_STR          	="Foretrekk 5,2 GHz-bånd"
WAKE_ON_MAGIC_PACKET        	="Reaktivert etter magisk pakke"
WAKE_ON_PATTERN_MATCH       	="Reaktivert etter samsvarende mønster"
PM_WIFI_REKEY_OFFLOAD	    	="GTK-omnøkling for WoWLAN"
PM_ARP_OFFLOAD			="ARP-avlastning for WoWLAN"
PM_NS_OFFLOAD			="NS-avlastning for WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Hvilemodus ved WoWLAN-frakobling"
PACKET_COALESCING               ="Pakkeoppsamling"
U_APSD_SUPPORT			="Støtte for U-APSD:"
THROUGHPUTBOOSTER_STR   	="Gjennomstrømmings-Booster"

SOURCEDISK1                     ="Installasjonsplate for Intel(R) Wireless"

[Strings.0415] ; Polish (Poland)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Sterownik karty Intel(R) Wireless dla systemu Windows 8.1 32 Bit"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Kanał Ad Hoc 802.11b/g"
IBSS_TX_POWER_STR           	="Moc transmisji"
ROAMING_AGGRESSIVENESS_STR	="Agresywność mobilności"
ADHOC_QOS_MODE_STR          	="Tryb Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   	="Ochrona trybu mieszanego"
WIRELESS_MODE_STR           	="Tryb bezprzewodowy"
PREFERRED_BAND_STR          	="Pasmo preferowane"
CHANNELWIDTH52              	="Szerokoœæ kana³u 802.11n dla 5,2 GHz"
CHANNELWIDTH24              	="Szerokoœæ kana³u 802.11n dla 2,4 GHz"
TGnMode                     	="Tryb HT"
VHT_ENABLED_STR			="Tryb VHT"
HT_ENABLED_STR			="Tryb HT"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Brak tolerancji dla kanału 40 MHz"
LOWEST_STR			="Najniższa"
MEDIUM_LOW_STR			="Średnio-niska"
MEDIUM_STR			="Średnia"
MEDIUM_HIGH_STR			="Średnio-wysoka"
HIGHEST_STR			="Najwyższa"
DISABLED_STR			="Wyłączono"
ENABLED_STR 			="Włączono"
CTS_TO_SELF_ENABLED_STR     	="Włączony zwrotny CTS"
RTS_CTS_ENABLED_STR         	="Włączony RTS/CTS"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Automatyczny"
WMM_DISABLED_STR            	="Wyłączono WMM"
WMM_ENABLED_STR             	="Włączono WMM"
NO_PREFERECE_STR            	="Bez preferencji"
PREFER_24_BAND_STR          	="Preferowany pasmo 2,4 GHz"
PREFER_52_BAND_STR          	="Preferowany pasmo 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Wznawianie na podstawie pakietu Magic"
WAKE_ON_PATTERN_MATCH       	="Wznawianie na podstawie dopasowania do wzorca"
PM_WIFI_REKEY_OFFLOAD	    	="GTK tworzy klucze ponowne dla WoWLAN"
PM_ARP_OFFLOAD			="Odciążanie ARP dla WoWLAN"
PM_NS_OFFLOAD			="Odciążanie NS dla WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Uśpienie WoWLAN Disconnect"
PACKET_COALESCING               ="Łączenie pakietów"
U_APSD_SUPPORT			="Obsługa funkcji U-APSD"
THROUGHPUTBOOSTER_STR   	="Przyśpieszacz przepustowości"

SOURCEDISK1                     ="Dysk instalacyjny Intel(R) Wireless"

[Strings.0416] ; Portuguese (Brazil)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Driver do adaptador Intel(R) Wireless para Windows 8.1 32 bits"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Canal ad-hoc 802.11b/g"
IBSS_TX_POWER_STR           	="Potência de transmissão"
ROAMING_AGGRESSIVENESS_STR	="Agressividade de roaming"
ADHOC_QOS_MODE_STR          	="Modo QoS Ad-hoc"
MIXED_MODE_PROTECTION_STR   	="Proteção de modo misto"
WIRELESS_MODE_STR           	="Modo sem fio"
PREFERRED_BAND_STR          	="Banda preferencial"
CHANNELWIDTH52              	="Largura do canal 802.11n - 5.2 GHz"
CHANNELWIDTH24              	="Largura do canal 802.11n - 2.4 GHz"
TGnMode                     	="Modo HT"
VHT_ENABLED_STR			="Modo VHT"
HT_ENABLED_STR			="Modo HT"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Sem tolerância a canal FAT"
LOWEST_STR			="Mais baixo"
MEDIUM_LOW_STR			="Média a baixa"
MEDIUM_STR			="Média"
MEDIUM_HIGH_STR			="Média a alta"
HIGHEST_STR			="Mais alto"
DISABLED_STR			="Desabilitado"
ENABLED_STR 			="Habilitado"
CTS_TO_SELF_ENABLED_STR     	="CTS auto-ativação ativado"
RTS_CTS_ENABLED_STR         	="RTS/CTS ativado"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM Desativado"
WMM_ENABLED_STR             	="WMM Ativado"
NO_PREFERECE_STR            	="Sem preferência"
PREFER_24_BAND_STR          	="Preferir banda de 2,4 GHz"
PREFER_52_BAND_STR          	="Preferir banda de 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Pacote Mágico do Wake on"
WAKE_ON_PATTERN_MATCH       	="Correspondência de padrão do Wake on"
PM_WIFI_REKEY_OFFLOAD	    	="Nova geração de chaves GTK para WoWLAN"
PM_ARP_OFFLOAD			="Descarregamento ARP para WoWLAN"
PM_NS_OFFLOAD			="Descarregamento NS para WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Suspender desconexão de WoWLAN"
PACKET_COALESCING               ="União de pacote"
U_APSD_SUPPORT			="Suporte para U-APSD"
THROUGHPUTBOOSTER_STR   	="Impulsionador do throughput"

SOURCEDISK1                     ="Disco da instalação do Intel(R) Wireless"

[Strings.0816] ; Portuguese (Portugal)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Controlador da placa Intel(R) Wireless para Windows 8.1 32 Bits"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Canal ad hoc 802.11b/g"
IBSS_TX_POWER_STR           	="Potência de transmissão"
ROAMING_AGGRESSIVENESS_STR	="Agressividade do roaming"
ADHOC_QOS_MODE_STR          	="Modo Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   	="Protecção do modo misto"
WIRELESS_MODE_STR           	="Modo sem fios"
PREFERRED_BAND_STR          	="Banda preferida"
CHANNELWIDTH52              	="Largura do canal 802.11n - 5.2 GHz"
CHANNELWIDTH24              	="Largura do canal 802.11n - 2.4 GHz"
TGnMode                     	="Modo HT"
VHT_ENABLED_STR			="Modo VHT"
HT_ENABLED_STR			="Modo HT"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Canal de grandes volumes incompatível"
LOWEST_STR			="Menor"
MEDIUM_LOW_STR			="Média-baixa"
MEDIUM_STR			="Média"
MEDIUM_HIGH_STR			="Média-Elevada"
HIGHEST_STR			="Maior"
DISABLED_STR			="Desactivado"
ENABLED_STR 			="Activado"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self activado"
RTS_CTS_ENABLED_STR         	="RTS/CTS Activado"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM desactivado"
WMM_ENABLED_STR             	="WMM activado"
NO_PREFERECE_STR            	="Sem Preferência"
PREFER_24_BAND_STR          	="Preferir banda de 2,4 GHz"
PREFER_52_BAND_STR          	="Preferir banda de 5,2 GHz"
WAKE_ON_MAGIC_PACKET        	="Reactivação por Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Correspondência de padrão do Wake on"
PM_WIFI_REKEY_OFFLOAD	    	="Regeração de chaves GTK para WoWLAN"
PM_ARP_OFFLOAD			="Descarga ARP para WoWLAN"
PM_NS_OFFLOAD			="Descarga NS para WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Suspender quando a WoWLAN estiver desligada"
PACKET_COALESCING               ="União de pacote"
U_APSD_SUPPORT			="Suporte de U-APSD"
THROUGHPUTBOOSTER_STR   	="Otimizador do rendimento"

SOURCEDISK1                     ="Disco de Instalação da Intel(R) Wireless"

[Strings.0419] ; Russian (Russia)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Драйвер адаптера Intel(R) Wireless для Windows 8.1 32 Bit "

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Канал Ad Hoc 802.11b/g"
IBSS_TX_POWER_STR           	="Мощность передачи"
ROAMING_AGGRESSIVENESS_STR	="Агрессивность роуминга"
ADHOC_QOS_MODE_STR          	="Режим Ad Hoc QoS"
MIXED_MODE_PROTECTION_STR   	="Защита в смешанном режиме"
WIRELESS_MODE_STR           	="Режим беспроводной сети"
PREFERRED_BAND_STR          	="Предпочитаемая частота"
CHANNELWIDTH52              	="Ширина канала 802.11n (5,2 ГГц)"
CHANNELWIDTH24              	="Ширина канала 802.11n (2,4&nbsp;ГГц)"
TGnMode                     	="Режим HT"
VHT_ENABLED_STR			="Режим VHT"
HT_ENABLED_STR			="Режим HT"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Несовместимость с каналом"
LOWEST_STR			="Мин."
MEDIUM_LOW_STR			="Средн.-мин."
MEDIUM_STR			="Средн."
MEDIUM_HIGH_STR			="Средн.-макс."
HIGHEST_STR			="Макс."
DISABLED_STR			="Выключено"
ENABLED_STR 			="Включено"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self включено"
RTS_CTS_ENABLED_STR         	="RTS/CTS включено"
CHANNELWIDTH20ONLY          	="20 МГц"
CHANNELWIDTHAUTO            	="Авто"
WMM_DISABLED_STR            	="WMM Выключено"
WMM_ENABLED_STR             	="WMM Включено"
NO_PREFERECE_STR            	="Нет предпочтений"
PREFER_24_BAND_STR          	="Предпочитать частоту 2,4 ГГц"
PREFER_52_BAND_STR          	="Предпочитать частоту 5,2 ГГц"
WAKE_ON_MAGIC_PACKET        	="Пробуждение пакетом Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Пробуждение при соответствии шаблону"
PM_WIFI_REKEY_OFFLOAD	    	="Повторный ввод ключа GTK для режима пробуждения Wake on Wireless LAN"
PM_ARP_OFFLOAD			="Выгрузка ARP для режима пробуждения Wake on Wireless LAN"
PM_NS_OFFLOAD			="Выгрузка NS для режима пробуждения Wake on Wireless LAN"
DEVICE_SLEEP_ON_DISCONNECT	="Переход в состояние сна при отключении режима пробуждения Wake on Wireless LAN"
PACKET_COALESCING               ="Объединение пакетов"
U_APSD_SUPPORT			="Поддержка U-APSD"
THROUGHPUTBOOSTER_STR   	="Увеличение пропускной способности"

SOURCEDISK1                     ="Установочный диск адаптера Intel(R) Wireless"

[Strings.041D] ; Swedish (Sweden)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Kortdrivrutin för Windows 8.1 32-bitars Intel(R) Wireless"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Ad hoc-kanal 802.11b/g"
IBSS_TX_POWER_STR           	="Överföringsenergi"
ROAMING_AGGRESSIVENESS_STR	="Roaming-aggressivitet"
ADHOC_QOS_MODE_STR          	="Ad Hoc QoS-läge"
MIXED_MODE_PROTECTION_STR   	="Skydd för blandat läge"
WIRELESS_MODE_STR           	="Trådlöst läge"
PREFERRED_BAND_STR          	="Förvalt band"
CHANNELWIDTH52              	="802.11n-kanalbredd för 5,2 GHz"
CHANNELWIDTH24              	="802.11n-kanalbredd för 2,4 GHz"
TGnMode                     	="HT-läge"
VHT_ENABLED_STR			="VHT-läge"
HT_ENABLED_STR			="HT-läge"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Inkompatibel med 40 MHz-kanal"
LOWEST_STR			="Lägsta"
MEDIUM_LOW_STR			="Medel-låg"
MEDIUM_STR			="Medel"
MEDIUM_HIGH_STR			="Medel-hög"
HIGHEST_STR			="Högsta"
DISABLED_STR			="Inaktiverad"
ENABLED_STR 			="Aktiverad"
CTS_TO_SELF_ENABLED_STR     	="CTS-till-själv aktiverat"
RTS_CTS_ENABLED_STR         	="RTS/CTS aktiverat"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Auto"
WMM_DISABLED_STR            	="WMM inaktiverad"
WMM_ENABLED_STR             	="WMM aktiverad"
NO_PREFERECE_STR            	="Ingen inställning"
PREFER_24_BAND_STR          	="Föredra 2,4 GHz-bandet"
PREFER_52_BAND_STR          	="Föredra 5,2 GHz-bandet"
WAKE_ON_MAGIC_PACKET        	="Aktivera vid Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Aktivering vid mönstermatchning"
PM_WIFI_REKEY_OFFLOAD	    	="GTK-nyckeluppdatering för WoWLAN"
PM_ARP_OFFLOAD			="ARP-avbelastning för WoWLAN"
PM_NS_OFFLOAD			="NS-avbelastning för WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="Viloläge vid WoWLAN-frånkoppling"
PACKET_COALESCING               ="Paketsammanslagning"
U_APSD_SUPPORT			="Support för U-APSD"
THROUGHPUTBOOSTER_STR   	="Genomflödesbooster"

SOURCEDISK1                     ="Installationsdisk Intel(R) Wireless"

[Strings.041E] ; Thai (Thailand)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="ไดรเวอร์อแด็ปเตอร์ Intel(R) Wireless สำหรับ Windows 8.1 32 บิต"

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="แชนแนลเฉพาะกิจ 802.11b/g"
IBSS_TX_POWER_STR           	="การส่งผ่านพลังงาน"
ROAMING_AGGRESSIVENESS_STR	="ความแรงในการใช้งานข้ามเขต"
ADHOC_QOS_MODE_STR          	="โหมด QoS เฉพาะกิจ"
MIXED_MODE_PROTECTION_STR   	="การป้องกันโหมดผสม"
WIRELESS_MODE_STR           	="โหมดไร้สาย"
PREFERRED_BAND_STR          	="แบนด์ที่ต้องการ"
CHANNELWIDTH52              	="ขนาดแชนแนล 802.11n (5.2 GHz)"
CHANNELWIDTH24              	="ขนาดแชนแนล 802.11n (2.4 GHz)"
TGnMode                     	="โหมด HT"
VHT_ENABLED_STR			="โหมด VHT"
HT_ENABLED_STR			="โหมด HT"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="ไม่สามารถใช้กับแชนแนลขนาดใหญ่"
LOWEST_STR			="ต่ำสุด"
MEDIUM_LOW_STR			="ปานกลาง-ต่ำ"
MEDIUM_STR			="ปานกลาง"
MEDIUM_HIGH_STR			="ปานกลาง-สูง"
HIGHEST_STR			="สูงสุด"
DISABLED_STR			="ยกเลิกใช้งาน"
ENABLED_STR 			="เปิดการใช้งาน"
CTS_TO_SELF_ENABLED_STR     	="ใช้งาน CTS-to-self แล้ว"
RTS_CTS_ENABLED_STR         	="ใช้งาน RTS/CTS"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="อัตโนมัติ"
WMM_DISABLED_STR            	="ยกเลิกการใช้งาน WMM"
WMM_ENABLED_STR             	="เปิดการใช้งาน WMM"
NO_PREFERECE_STR            	="ไม่มีการกำหนด"
PREFER_24_BAND_STR          	="แบนด์ 2.4 GHz"
PREFER_52_BAND_STR          	="แบนด์ 5.2 GHz"
WAKE_ON_MAGIC_PACKET        	="Wake on Magic Packet"
WAKE_ON_PATTERN_MATCH       	="Wake on Pattern Match"
PM_WIFI_REKEY_OFFLOAD	    	="GTK กำลังกำหนดคีย์ใหม่สำหรับ WoWLAN"
PM_ARP_OFFLOAD			="ARP ออฟโหลดสำหรับ WoWLAN"
PM_NS_OFFLOAD			="NS ออฟโหลดสำหรับ WoWLAN"
DEVICE_SLEEP_ON_DISCONNECT	="ยกเลิกการเชื่อมต่อสลีปบน WoWLAN"
PACKET_COALESCING               ="การรวมแพคเก็ต"
U_APSD_SUPPORT			="การสนับสนุน U-APSD"
THROUGHPUTBOOSTER_STR   	="ตัวเพิ่มอัตรารับส่ง"

SOURCEDISK1                     ="ดิสก์ติดตั้ง Intel(R) Wireless"

[Strings.041F] ; Turkish (Turkey)
PROVIDER_NAME              		="Intel"
COMPANY_NAME               		="Intel Corporation"

NIC_7260AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7260" 
NIC_7260AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7260" 
NIC_7260BGN_2x2_HMC  		="Intel(R) Wireless-N 7260"

NIC_7265AC_2x2_HMC   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_7265AGN_2x2_HMC  		="Intel(R) Dual Band Wireless-N 7265"
NIC_7265BGN_2x2_HMC  		="Intel(R) Wireless-N 7265"

NIC_3160AC_HMC 			="Intel(R) Dual Band Wireless-AC 3160" 
NIC_3160AGN_HMC 			="Intel(R) Dual Band Wireless-N 3160" 
NIC_3160BGN_HMC 			="Intel(R) Wireless-N 3160" 

NIC_3165AC_HMC 			="Intel(R) Dual Band Wireless-AC 3165" 

NIC_AdapterModel_7260AC_2x2   	="Intel(R) Dual Band Wireless-AC 7260" 
NIC_AdapterModel_7260AGN_2x2  	="Intel(R) Dual Band Wireless-N 7260" 
NIC_AdapterModel_7260BGN_2x2  	="Intel(R) Wireless-N 7260"

NIC_AdapterModel_7265AC_2x2   	="Intel(R) Dual Band Wireless-AC 7265"
NIC_AdapterModel_7265AGN_2x2  	="Intel(R) Dual Band Wireless-N 7265"
NIC_AdapterModel_7265BGN_2x2  	="Intel(R) Wireless-N 7265"

NIC_AdapterModel_3160AC_HMC   	="Intel(R) Dual Band Wireless-AC 3160" 
NIC_AdapterModel_3160AGN_HMC  	="Intel(R) Dual Band Wireless-N 3160"  
NIC_AdapterModel_3160BGN_HMC  	="Intel(R) Wireless-N 3160"  

NIC_AdapterModel_3165AC_HMC   	="Intel(R) Dual Band Wireless-AC 3165" 

NIC_DriverDesc_7260AC_2x2  	     	="Intel(R) Dual Band Wireless-AC 7260"
NIC_DriverDesc_7260AGN_2x2 	     	="Intel(R) Dual Band Wireless-N 7260"
NIC_DriverDesc_7260BGN_2x2 	     	="Intel(R) Wireless-N 7260"

NIC_DriverDesc_7265AC_2x2   		="Intel(R) Dual Band Wireless-AC 7265"
NIC_DriverDesc_7265AGN_2x2  		="Intel(R) Dual Band Wireless-N 7265"
NIC_DriverDesc_7265BGN_2x2  		="Intel(R) Wireless-N 7265"

NIC_DriverDesc_3160AC_HMC   		="Intel(R) Dual Band Wireless-AC 3160" 
NIC_DriverDesc_3160AGN_HMC  		="Intel(R) Dual Band Wireless-N 3160"  
NIC_DriverDesc_3160BGN_HMC  		="Intel(R) Wireless-N 3160"  

NIC_DriverDesc_3165AC_HMC   		="Intel(R) Dual Band Wireless-AC 3165" 

NIC_Service_DispName_WINB	 	="Windows 8.1 32 Bit için Intel(R) Wireless Bağdaştırıcı Sürücüsü "

; following are Advanced Tab Properties (NDI) strings. need to be localized.
RECOMMENDED_CHANNEL24_STR 	="Aygıttan Aygıta Kanal 802.11b/g"
IBSS_TX_POWER_STR           	="Yayın gücü"
ROAMING_AGGRESSIVENESS_STR	="Gezinme Zorlaması"
ADHOC_QOS_MODE_STR          	="Aygıttan Aygıta QoS Modu"
MIXED_MODE_PROTECTION_STR   	="Karışık mod koruması"
WIRELESS_MODE_STR           	="Kablosuz Mod"
PREFERRED_BAND_STR          	="Yeğlenen Bant"
CHANNELWIDTH52              	="5.2 GHz için 802.11n Kanal Genişliği"
CHANNELWIDTH24              	="2.4 GHz için 802.11n Kanal Genişliği"
TGnMode                     	="HT Modu"
VHT_ENABLED_STR			="VHT Modu"
HT_ENABLED_STR			="HT Modu"
BTHSMode                    	="Bluetooth(R) AMP"
FAT_CHANNEL_TOLERANT		="Geniş Kanal için Uyumsuz"
LOWEST_STR			="En düşük"
MEDIUM_LOW_STR			="Düşük"
MEDIUM_STR			="Orta"
MEDIUM_HIGH_STR			="Yüksek"
HIGHEST_STR			="En yüksek"
DISABLED_STR			="Devre dışı"
ENABLED_STR 			="Etkin"
CTS_TO_SELF_ENABLED_STR     	="CTS-to-self etkin"
RTS_CTS_ENABLED_STR         	="RTS/CTS etkin"
CHANNELWIDTH20ONLY          	="20 MHz"
CHANNELWIDTHAUTO            	="Otomatik"
WMM_DISABLED_STR            	="WMM devre dışı"
WMM_ENABLED_STR             	="WMM etkin"
NO_PREFERECE_STR            	="Tercih yok"
PREFER_24_BAND_STR          	="2,4 GHz bant Tercih Et"
PREFER_52_BAND_STR          	="5,2 GHz bant Tercih Et"
WAKE_ON_MAGIC_PACKET        	="Sihirli Paket Uyanması"
WAKE_ON_PATTERN_MATCH       	="Desen eşleştirme uyanması"
PM_WIFI_REKEY_OFFLOAD	    	="WoWLAN için GTK yeniden anahtarlama"
PM_ARP_OFFLOAD			="WoWLAN için ARP yük boşaltma"
PM_NS_OFFLOAD			="WoWLAN için NS yük boşaltma"
DEVICE_SLEEP_ON_DISCONNECT	="WoWLAN Bağlantı Kesintisinde uyku durumuna geç"
PACKET_COALESCING               ="Paket Birleştirme"
U_APSD_SUPPORT			="U-APSD Desteği"
THROUGHPUTBOOSTER_STR   	="Verimlilik Arttırıcı"

SOURCEDISK1                     ="Intel(R) Wireless Yükleme Diski"
