;/****************************************************************************
; * Copyright 2009 Atheros Communications Inc., all rights reserved.          *
; *                                                                           *
; * Copyright (c) 2011 Qualcomm Atheros, Inc.                                 *
; * All Rights Reserved.                                                      *
; * Qualcomm Atheros Confidential and Proprietary.                            *
; *                                                                           *
; * INF file for Qualcomm Atheros reference designs                                    *
; ****************************************************************************/

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %ATHEROS%
CatalogFile = athuw8x.cat
DriverVer   = 10/15/2012,10.0.0.20


[Manufacturer]
%ATHEROS%     = Atheros, NTamd64
%NETGEAR%     = NETGEAR, NTamd64
%DLINK%       = DLINK, NTamd64
%AZUREWAVE%   = AZUREWAVE, NTamd64
%LITEON%      = LITEON, NTamd64
%SMC%         = SMC, NTamd64
%VIA%         = VIA, NTamd64
%VERIZON%     = Verizon, NTamd64
%ACTIONTEC%   = Actiontec, NTamd64
%CENTURYLINK% = Centurylink, NTamd64
[ControlFlags]
ExcludeFromSelect = *

[Atheros.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ATHER.DeviceDesc.9271% = ATHER_DEV_9271.ndi,     USB\VID_0CF3&PID_9271
%ATHER.DeviceDesc.9271% = ATHER_DEV_9271_SS.ndi,  USB\VID_0CF3&PID_9271&REV_0108&SS
%ATHER.DeviceDesc.7010% = ATHER_DEV_7010.ndi,     USB\VID_0CF3&PID_7010
%ATHER.DeviceDesc.7015% = ATHER_DEV_7015.ndi,     USB\VID_0CF3&PID_7015
%ATHER.DeviceDesc.1006% = ATHER_DEV_1006.ndi,     USB\VID_0CF3&PID_1006

[NETGEAR.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%NTGR.DeviceDesc.9030%  = NTGR_DEV_9030.ndi,      USB\VID_0846&PID_9030
%NTGR.DeviceDesc.9018%  = NTGR_DEV_9018.ndi,      USB\VID_0846&PID_9018

[DLINK.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%DLINK.DeviceDesc.3A10%  = DLINK_DEV_3A10.ndi,    USB\VID_07D1&PID_3A10

[AZUREWAVE.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%AZWV.DeviceDesc.3327%  = AZWV_DEV_3327.ndi,      USB\VID_13D3&PID_3327
%AZWV.DeviceDesc.3328%  = AZWV_DEV_3328.ndi,      USB\VID_13D3&PID_3328
%AZWV.DeviceDesc.3346%  = AZWV_DEV_3346.ndi,      USB\VID_13D3&PID_3346
%AZWV.DeviceDesc.3348%  = AZWV_DEV_3348.ndi,      USB\VID_13D3&PID_3348
%AZWV.DeviceDesc.3349%  = AZWV_DEV_3349.ndi,      USB\VID_13D3&PID_3349
%AZWV.DeviceDesc.3350%  = AZWV_DEV_3350.ndi,      USB\VID_13D3&PID_3350
%AZWV.DeviceDesc.3390%  = AZWV_DEV_33XX.ndi,      USB\VID_13D3&PID_3390
%AZWV.DeviceDesc.3391%  = AZWV_DEV_33XX.ndi,      USB\VID_13D3&PID_3391

[LITEON.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%ATHER.DeviceDesc.9271% = ATHER_DEV_9271.ndi,     USB\VID_04CA&PID_4605
%LITEON.DeviceDesc.9271% = LITEON_9271.ndi,       USB\VID_04CA&PID_9271

[SMC.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%SMC.DeviceDesc.A704%   = SMC_DEV_A704.ndi,       USB\VID_083A&PID_A704

[VIA.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%VIA.DeviceDesc.3801%   = ATHER_DEV_9271.ndi,     USB\VID_040D&PID_3801

[VERIZON.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
%VRZN.DeviceDesc.1200%  = ATHER_DEV_7015.ndi,     USB\VID_1668&PID_1200

[ACTIONTEC.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
; Actiontec
%ACTION.DeviceDesc.4500% = ATHER_DEV_7015.ndi,    USB\VID_1668&PID_4500

[CENTURYLINK.NTamd64]
; DisplayName               Section                 DeviceID
; -----------               -------                 --------
; Centurylink
%CENT.DeviceDesc.4700%   = ATHER_DEV_7015.ndi,    USB\VID_1668&PID_4700

[ATHER_DEV_9271.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, 9271.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHER_DEV_9271.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[ATHER_DEV_9271.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[ATHER_DEV_9271_SS.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, 9271.reg, usbSelectiveSuspend.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHER_DEV_9271_SS.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[ATHER_DEV_9271_SS.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[ATHER_DEV_7010.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, 7010.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHER_DEV_7010.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[ATHER_DEV_7010.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[ATHER_DEV_1006.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, 5416.bgub.reg, 9271.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHER_DEV_1006.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[ATHER_DEV_1006.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[ATHER_DEV_7015.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, 7015.reg, htDisableWepTkip.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[ATHER_DEV_7015.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[ATHER_DEV_7015.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[NTGR_DEV_9030.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, NTGR.reg, 9271.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[NTGR_DEV_9030.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[NTGR_DEV_9030.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[NTGR_DEV_9018.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, NTGR_9018.reg, htDisableWepTkip.reg, uapsd_VO.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[NTGR_DEV_9018.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[NTGR_DEV_9018.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[DLINK_DEV_3A10.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, DLINK.reg, 9271.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[DLINK_DEV_3A10.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[DLINK_DEV_3A10.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[AZWV_DEV_3327.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, 9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[AZWV_DEV_3327.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[AZWV_DEV_3327.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[AZWV_DEV_3328.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, 9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[AZWV_DEV_3328.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[AZWV_DEV_3328.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[AZWV_DEV_3346.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, 9271.reg, htDisableWepTkip.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[AZWV_DEV_3346.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[AZWV_DEV_3346.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[AZWV_DEV_3348.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, 9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[AZWV_DEV_3348.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[AZWV_DEV_3348.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[AZWV_DEV_3349.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, 9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[AZWV_DEV_3349.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[AZWV_DEV_3349.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[AZWV_DEV_3350.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, 9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[AZWV_DEV_3350.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[AZWV_DEV_3350.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[AZWV_DEV_33XX.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, 9271.reg, htDisableWepTkip.reg, surpriseRemovalOk.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[AZWV_DEV_33XX.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[AZWV_DEV_33XX.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[LITEON_9271.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, 9271.reg, htDisableWepTkip.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[LITEON_9271.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[LITEON_9271.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

[SMC_DEV_A704.ndi.NTamd64]
Characteristics = 0x84
BusType         = 15
AddReg          = atheros.reg, 7015.reg, htDisableWepTkip.reg
DelReg          = atheros.DelReg
CopyFiles       = atheros.CopyFiles
*IfType         = 71		; IF_TYPE_IEEE80211
*MediaType      = 16		; NdisMediumNative802_11
*PhysicalMediaType = 9		; NdisPhysicalMediumNative802_11

[SMC_DEV_A704.ndi.NTamd64.Services]
AddService = athur, 2, atheros.Service, atheros.EventLog

[SMC_DEV_A704.ndi.NTamd64.HW]
AddReg = atheros_os61.vwifi.reg

;;End of Others Section

[atheros.reg]
HKR, Ndi,                           Service,    0, "athur"
HKR, Ndi\Interfaces,                UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,                LowerRange, 0, "wlan,ethernet,vwifi"
HKR, Ndi\params\*ReceiveBuffers,    ParamDesc,  0, "%ReceiveBuffers%"
HKR, Ndi\params\*ReceiveBuffers,    default,    0, "256"
HKR, Ndi\params\*ReceiveBuffers,    min,        0, "1"
HKR, Ndi\params\*ReceiveBuffers,    max,        0, "00000512"
HKR, Ndi\params\*ReceiveBuffers,    step,       0, "1"
HKR, Ndi\params\*ReceiveBuffers,    Base,       0, "10"
HKR, Ndi\params\*ReceiveBuffers,    type,       0, "int"
HKR, Ndi\params\*TransmitBuffers,   ParamDesc,  0, "%TransmitBuffers%"
HKR, Ndi\params\*TransmitBuffers,   default,    0, "256"
HKR, Ndi\params\*TransmitBuffers,   min,        0, "1"
HKR, Ndi\params\*TransmitBuffers,   max,        0, "00000512"
HKR, Ndi\params\*TransmitBuffers,   step,       0, "1"
HKR, Ndi\params\*TransmitBuffers,   Base,       0, "10"
HKR, Ndi\params\*TransmitBuffers,   type,       0, "int"
HKR, Ndi\params\NetworkAddress,     ParamDesc,  0,  %NetworkAddress%
HKR, Ndi\params\NetworkAddress,     default,    0,  ""
HKR, Ndi\params\NetworkAddress,     LimitText,  0,  "12"
HKR, Ndi\params\NetworkAddress,     UpperCase,  0,  "1"
HKR, Ndi\params\NetworkAddress,     optional,   0,  "1"
HKR, Ndi\params\NetworkAddress,     type,       0,  "edit"
HKR, Ndi\params\shortPreamble,      ParamDesc,  0,  %shortPreamble%
HKR, Ndi\params\shortPreamble,      Base,       0,  "10"
HKR, Ndi\params\shortPreamble,      default,    0,  "1"
HKR, Ndi\params\shortPreamble,      type,       0,  "enum"
HKR, Ndi\params\shortPreamble\enum, "1",        0,  %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0",        0,  %shortPreambleDisable%
HKR, Ndi\params\scanTimeValid,      ParamDesc,  0,  %scanTimeValid%
HKR, Ndi\params\scanTimeValid,      default,    0,  "60"
HKR, Ndi\params\scanTimeValid,      min,        0,  "20"
HKR, Ndi\params\scanTimeValid,      max,        0,  "120"
HKR, Ndi\params\scanTimeValid,      step,       0,  "5"
HKR, Ndi\params\scanTimeValid,      base,       0,  "10"
HKR, Ndi\params\scanTimeValid,      type,       0,  "int"

HKR, Ndi\params\*SelectiveSuspend,  ParamDesc,  0,  %SelectiveSuspend%
HKR, Ndi\params\*SelectiveSuspend,  Base,       0,  "10"
HKR, Ndi\params\*SelectiveSuspend,  default,    0,  "1"
HKR, Ndi\params\*SelectiveSuspend,  type,       0,  "enum"
HKR, Ndi\params\*SelectiveSuspend\enum, "0",    0,  %Disabled%
HKR, Ndi\params\*SelectiveSuspend\enum, "1",    0,  %Enabled%

HKR, Ndi\params\*SSIdleTimeout,     ParamDesc,  0,  %SSIdleTimeout%
HKR, Ndi\params\*SSIdleTimeout,     default,    0,  "5"
HKR, Ndi\params\*SSIdleTimeout,     min,        0,  "1"
HKR, Ndi\params\*SSIdleTimeout,     max,        0,  "60"
HKR, Ndi\params\*SSIdleTimeout,     step,       0,  "1"
HKR, Ndi\params\*SSIdleTimeout,     base,       0,  "10"
HKR, Ndi\params\*SSIdleTimeout,     type,       0,  "int"

;/* Enable these if VLAN or 802.1p is to be enabled */
;HKR, Ndi\Params\*PriorityVLANTag,  ParamDesc,  , %PriorityVLAN%
;HKR, Ndi\Params\*PriorityVLANTag,  default,    , "3"
;HKR, Ndi\Params\*PriorityVLANTag,  type,       , "enum"
;HKR, Ndi\Params\*PriorityVLANTag\enum, 0,      , %PriorityVLANDisabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 1,      , %PriorityEnabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 2,      , %VLANEnabled%
;HKR, Ndi\Params\*PriorityVLANTag\enum, 3,      , %PriorityVLANEnabled%

HKR, ,                                  forceNormalSlotMrvl,             0x00002,  "1"
HKR, ,                                  htAdhocEnable,                   0x00002,  "0"
HKR, ,                                  ampEnable,                       0x00002,  "0"
HKR, ,                                  halusbForceWake,                 0x00002,  "0"
HKR, ,                                  usbForceWake,                    0x00002,  "0"
HKR, ,                                  disabletidqueue,                 0x00002,  "1"
HKR, ,                                  WowEnablePME,                    0x00002,  "0"

[atheros.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
HKR,Ndi\Params\tpc
HKR,,tpc
HKR,Ndi\Params\authTypeUseOnly
HKR,,authTypeUseOnly
HKR,,AdHocBand
HKR,,AwakeTimePerf
HKR,,beaconInterval
HKR,,bkScanEnable
HKR,,bssType
HKR,,ccode
HKR,,clist
HKR,,defaultKey
HKR,,EncryptionAlg
HKR,,FragThreshold
HKR,,HwTxRetries
HKR,,privacyInvoked
HKR,,QoS
HKR,,rateCtrlEnable
HKR,,RTSThreshold
HKR,,scanType
HKR,,SwTxRetryScale
HKR,,SmeEnable
HKR,,aifs
HKR,,cwmin
HKR,Ndi\params,MapRegisters,0x2000
HKR,,MapRegisters
HKR,Ndi\params,radioEnable,0x2000
HKR,Ndi\params,sleepMode,0x2000
HKR,,sleepMode
HKR,,transmitRateMax
HKR, Ndi\params\*TransmitBuffers
HKR,,*TransmitBuffers
HKR,,rxChainMask
HKR,,txChainMaskLegacy
HKR,,rxChainMaskLegacy
HKR,,rxChainDetect
HKR,,rxChainDetectRef
HKR,,rxChainDetectThreshA
HKR,,rxChainDetectThreshG
HKR,,rxChainDetectDeltaA
HKR,,rxChainDetectDeltaG
HKR,,usbSSuspendEnable

[7010.reg]
HKR, , isMagpie,                        0x00002, "1"
HKR, , htEnableWepTkip,                 0x00002, "0"
HKR, , gpioLedCustom,                   0x00002, "1"
HKR, , gpioPinFunc0,                    0x00002, "12"
HKR, , gpioPinFunc1,                    0x00002, "10"
HKR, , LowerHTTxGain,                   0x00002, "1"
HKR, , xpblevel5,                       0x00002, "256"
;HKR, , GreenTx,                               0, "0"
HKR, , wpsButtonGpio,                   0x00002, "13"

[7015.reg]
HKR, , isMagpie,                        0x00002, "1"
HKR, , gpioLedCustom,                   0x00002, "1"
HKR, , gpioPinFunc0,                    0x00002, "12"
HKR, , gpioPinFunc1,                    0x00002, "10"
HKR, , stbcEnable,                      0x00002, "1"
HKR, , wpsButtonGpio,                   0x00002, "4"

[htDisableWepTkip.reg]
HKR, , htEnableWepTkip,                 0x00002, "0"

[surpriseRemovalOk.reg]
HKR, , surpriseRemovalOk,               0x10003, 1

[9271.reg]
;HKR, , GreenTx,                        0, "0"
HKR, , btPriorityGpioSelect,            0, 6
HKR, , btActiveGpioSelect,              0, 7
HKR, , wlanActiveGpioSelect,            0, 8
HKR, , btCoexEnable,                    0, 0
HKR, , btCoexAgent,                     0, 0
HKR, , wpsButtonGpio,                   0x00002, "13"
HKR, , K2ScanPartialReset,              0x00002,  "0"

[usbSelectiveSuspend.reg]
HKR, , usbSSuspendEnable,               0x00002, "1"

;-----------------------------------------------------------------------------
;;Customized Section
[bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,        %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,        "10"
HKR, Ndi\params\NetBand,                default,                        0,        "1647"
HKR, Ndi\params\NetBand,                type,                           0,        "enum"
HKR, Ndi\params\NetBand\enum,           "1647",                         0,        %Auto%
HKR, Ndi\params\NetBand\enum,           "1603",                         0,        %5GOnly%
HKR, Ndi\params\NetBand\enum,           "44",                           0,        %2GOnly%
[adhocchannelselect.reg]
HKR, Ndi\params\defaultIbssChannel,     ParamDesc,                      0,        %adhocchannel%
HKR, Ndi\params\defaultIbssChannel,     default,                        0,        "10"
HKR, Ndi\params\defaultIbssChannel,     min,                            0,        "1"
HKR, Ndi\params\defaultIbssChannel,     max,                            0,        "11"
HKR, Ndi\params\defaultIbssChannel,     step,                           0,        "1"
HKR, Ndi\params\defaultIbssChannel,     base,                           0,        "10"
HKR, Ndi\params\defaultIbssChannel,     type,                           0,        "int"

[5416.bgub.reg]
HKR, ,                                  NetBand,                        0x00002,  "12"

[5416.bgnxb.reg]
HKR, ,                                  NetBand,                        0x00002,  "26636"
HKR, ,                                  wmodeselect,                    0x00002,  "26636"

[5416.bandselect.reg]
HKR, Ndi\params\NetBand,                ParamDesc,                      0,  %WirelessMode%
HKR, Ndi\params\NetBand,                Base,                           0,  "10"
HKR, Ndi\params\NetBand,                default,                        0,  "130671"
HKR, Ndi\params\NetBand,                type,                           0,  "enum"
HKR, Ndi\params\NetBand\enum,           "130671",                       0,  %Auto%
HKR, Ndi\params\NetBand\enum,           "104003",                       0,  %5GOnly%
HKR, Ndi\params\NetBand\enum,           "26668",                        0,  %2GOnly%
[NTGR.reg]
HKR, ,                                  ignore11dBeacon,                0, 1
HKR, ,                                  gpioLedCustom,                  0, 8
HKR, ,                                  gpioPinFunc0,                   0, 15
HKR, ,                                  swapDefaultLED,                 0, 1
HKR, ,                                  GreenTx,                        0, 31
HKR, ,                                  htEnableWepTkip,          0x00002, "3"
HKR, ,                                  htEnableWepTkipAgg,       0x00002, "0"
HKR, ,                                  usbWmiRetry,              0x00002, "0"

[NTGR_9018.reg]
HKR, ,                                  isMagpie,                 0x00002, "1"
HKR, ,                                  gpioLedCustom,            0x00002, "9"
HKR, ,                                  gpioPinFunc0,             0x00002, "12"
HKR, ,                                  gpioPinFunc1,             0x00002, "10"
HKR, ,                                  GreenTx,                        0, 0
HKR, ,                                  updatelinkspeed,                0, 1
HKR, ,                                  stbcEnable,               0x00002, "1"
HKR, ,                                  halPciePowerSaveEnable,         0, 2
HKR, ,                                  wpsButtonGpio,            0x00002, "13"
HKR, ,                                  usbWmiRetry,              0x00002, "0"

[DLINK.reg]
HKR, ,                                  gpioLedCustom,   0, 1
HKR, ,                                  gpioPinFunc0,    0, 15
HKR, ,                                  swapDefaultLED,  0, 1

[uapsd_VO.reg]
HKR, Ndi\params\uapsdEnabledBE,            ParamDesc,                      0,  %uapsdEnabledBE%
HKR, Ndi\params\uapsdEnabledBE,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledBE,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledBE,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledBE\enum,       "1",                            0,  %uapsdEnabledBEOn%
HKR, Ndi\params\uapsdEnabledBE\enum,       "0",                            0,  %uapsdEnabledBEOff%

HKR, Ndi\params\uapsdEnabledBK,            ParamDesc,                      0,  %uapsdEnabledBK%
HKR, Ndi\params\uapsdEnabledBK,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledBK,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledBK,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledBK\enum,       "1",                            0,  %uapsdEnabledBKOn%
HKR, Ndi\params\uapsdEnabledBK\enum,       "0",                            0,  %uapsdEnabledBKOff%

HKR, Ndi\params\uapsdEnabledVI,            ParamDesc,                      0,  %uapsdEnabledVI%
HKR, Ndi\params\uapsdEnabledVI,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledVI,            default,                        0,  "0"
HKR, Ndi\params\uapsdEnabledVI,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledVI\enum,       "1",                            0,  %uapsdEnabledVIOn%
HKR, Ndi\params\uapsdEnabledVI\enum,       "0",                            0,  %uapsdEnabledVIOff%

HKR, Ndi\params\uapsdEnabledVO,            ParamDesc,                      0,  %uapsdEnabledVO%
HKR, Ndi\params\uapsdEnabledVO,            Base,                           0,  "10"
HKR, Ndi\params\uapsdEnabledVO,            default,                        0,  "1"
HKR, Ndi\params\uapsdEnabledVO,            type,                           0,  "enum"
HKR, Ndi\params\uapsdEnabledVO\enum,       "1",                            0,  %uapsdEnabledVOOn%
HKR, Ndi\params\uapsdEnabledVO\enum,       "0",                            0,  %uapsdEnabledVOOff%

HKR, Ndi\params\psPollEnabled,            ParamDesc,                      0,  %psPoll%
HKR, Ndi\params\psPollEnabled,            Base,                           0,  "10"
HKR, Ndi\params\psPollEnabled,            default,                        0,  "1"
HKR, Ndi\params\psPollEnabled,            type,                           0,  "enum"
HKR, Ndi\params\psPollEnabled\enum,       "1",                            0,  %psPollEnable%
HKR, Ndi\params\psPollEnabled\enum,       "0",                            0,  %psPollDisable%

;;End of Customized Section

[atheros.Service]
DisplayName     = %ATHR.Service.DispName%
ServiceType     = 1         ;SERVICE_KERNEL_DRIVER
StartType       = 3         ;SERVICE_DEMAND_START
ErrorControl    = 1         ;SERVICE_ERROR_NORMAL
ServiceBinary   = %12%\athuw8x.sys
LoadOrderGroup  = NDIS

[atheros.EventLog]
AddReg = atheros.AddEventLog.reg

[atheros.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7


[atheros.CopyFiles]
athuw8x.sys,,,2

[SourceDisksNames]
1 = %DiskDescription%,athuw8x.sys,,

[SourceDisksFiles]
athuw8x.sys = 1,,

[DestinationDirs]
atheros.CopyFiles            = 12
DefaultDestDirs              = 11

;-------------- WDF Coinstaller installation
[DestinationDirs]
CoInstaller_CopyFiles = 11

[athurx.Dev.NT.CoInstallers]
AddReg=CoInstaller_AddReg
CopyFiles=CoInstaller_CopyFiles

[CoInstaller_CopyFiles]
wdfcoinstaller01005.dll

[SourceDisksFiles]
wdfcoinstaller01005.dll=1 ; make sure the number matches with SourceDisksNames

[CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "wdfcoinstaller01005.dll,WdfCoInstaller"

[athurx.Dev.NT.Wdf]
KmdfService = athurx, athurx_wdfsect

[athurx_wdfsect]
KmdfLibraryVersion = 1.5

;; Adds the VWiFi PNP filter
[atheros_os61.vwifi.reg]
HKR,,"UpperFilters",0x00010000,"vwifibus"

[Strings]
Msft                         = "Microsoft"
Atheros                      = "Qualcomm Atheros Communications Inc."
NETGEAR                      = "Netgear Inc."
DLINK                        = "D-Link"
AZUREWAVE                    = "AzureWave Technologies, Inc."
LITEON                       = "Lite-On"
SMC                          = "SMC Networks, Inc." 
VIA                          = "VIA"
VERIZON                      = "Verizon"
ACTIONTEC                    = "Actiontec"
CENTURYLINK                  = "Centurylink"
ATHR.Service.DispName        = "Qualcomm Atheros AR9271 Wireless Network Adapter Service"
ATHR7010.Service.DispName    = "Qualcomm Atheros AR7010 Wireless Network Adapter Service"
DiskDescription              = "Qualcomm Atheros Sample Driver Disk 1"
TransmitBuffers              = "Transmit Buffers"
ReceiveBuffers               = "Receive Buffers"
NetworkAddress               = "Network Address"
scanTimeValid                = "Scan Valid Interval"
shortPreamble                = "802.11b Preamble"
shortPreambleEnable          = "Long and Short"
shortPreambleDisable         = "Long only"
SelectiveSuspend             = "Selective Suspend"
SSIdleTimeout                = "Selective suspend idle time-out in units of seconds"
rssiThrHigh                  = "RSSI Threshold"
rssiThrHighNormal            = "Normal"
rssiThrHighMin               = "Min"
;radioEnable                  = "Radio On/Off"
;radioEnableOn                = "On"
;radioEnableOff               = "Off"
scanTime                     = "Roam Time (sec)"
roamRssiA                    = "Roam Time Threshold (db)"
WirelessMode                 = "Wireless Mode Selection"
adhocchannel                 = "Adhoc channel Selection"
bkScanEnable                 = "BackgroundScan On/Off"
bkScanEnableOn               = "On"
bkScanEnableOff              = "Off"
radioEnable                  = "Radio On/Off"
radioEnableOn                = "On"
radioEnableOff               = "Off"
roamRssi11A                  = "roamRssiA"
roamRssi11B                  = "roamRssiB"
roamRssi11BOnly              = "roamRssiBOnly"
roamRateA                    = "roamRateA"
roamRateA6M                  = " 6Mbps"
roamRateA9M                  = " 9Mbps"
roamRateA12M                 = "12Mbps"
roamRateA18M                 = "18Mbps"
roamRateA24M                 = "24Mbps"
roamRateA36M                 = "36Mbps"
roamRateA48M                 = "48Mbps"
roamRateA54M                 = "54Mbps"
roamRateBOnly                = "roamRateBOnly"
roamRateBOnly1M              = " 1Mbps"
roamRateBOnly2M              = " 2Mbps"
roamRateBOnly5M              = " 5Mbps"
roamRateBOnly11M             = "11Mbps"
roamRateB                    = "roamRateB"
roamRateB1M                  = " 1Mbps"
roamRateB2M                  = " 2Mbps"
roamRateB5M                  = " 5Mbps"
roamRateB6M                  = " 6Mbps"
roamRateB9M                  = " 9Mbps"
roamRateB11M                 = "11Mbps"
pcieAspm                     = "pcieAspm"
pcieAspmOff                  = "L0s Off, L1 Off"
pcieAspmL0sOn                = "L0s On,  L1 Off"
pcieAspmL1On                 = "L0s Off, L1 On"
pcieAspmL0sandL1On           = "L0s On,  L1 On"
wModeSelect                  = "Wireless Mode"
wModeSelect11bonly           = "11b only"
wModeSelect11nbg             = "11n(2.4GHz) and g and b"
wModeSelect11na              = "11n(5GHz) and a"
wModeSelect11abgn            = "11abgn"
wModeLegacy11a               = "11a only"
wModeLegacy11bonly           = "11b only"
wModeLegacy11bg              = "11g and 11b"
wModeLegacy11abg             = "11abg"
antennaSwitch                = "AntennaSwitch"
antennaSwitchAuto            = "Auto"
antennaSwitchA               = "Antenna A"
antennaSwitchB               = "Antenna B"
Auto                         = "Auto"
5GOnly	                     = "5Ghz Only"
2GOnly	                     = "2Ghz Only"
11DModeSwitch                = "11d Mode Switch"
Enable                       = "Enable"
Enabled                      = "Enabled"
Disable                      = "Disable"
Disabled                     = "Disabled"
PowerSaveMode                = "Power Save Mode"
Off                          = "Off"
Maximum                      = "Maximum"
Normal                       = "Normal"
802_11d                      = "802.11d"
uapsdEnabledBE               = "Power Save Policy (Best Effort)"
uapsdEnabledBEOn             = "WMM Power Save (UAPSD)"
uapsdEnabledBEOff            = "Legacy Power Save"
uapsdEnabledBK               = "Power Save Policy (Background)"
uapsdEnabledBKOn             = "WMM Power Save (UAPSD)"
uapsdEnabledBKOff            = "Legacy Power Save"
uapsdEnabledVI               = "Power Save Policy (Video)"
uapsdEnabledVIOn             = "WMM Power Save (UAPSD)"
uapsdEnabledVIOff            = "Legacy Power Save"
uapsdEnabledVO               = "Power Save Policy (Voice)"
uapsdEnabledVOOn             = "WMM Power Save (UAPSD)"
uapsdEnabledVOOff            = "Legacy Power Save"
psPoll                       = "Power Save Legacy Algorithm"
psPollEnable                 = "PS Poll"
psPollDisable                = "PS non Poll"
ATHER.DeviceDesc.9271        = "Qualcomm Atheros AR9271 Wireless Network Adapter"
ATHER.DeviceDesc.7010        = "Qualcomm Atheros AR7010 Wireless Network Adapter"
ATHER.DeviceDesc.7015        = "Qualcomm Atheros AR7015 Wireless Network Adapter"
ATHER.DeviceDesc.1006        = "Qualcomm Atheros 11G USB Wireless Network Adapter"
NTGR.DeviceDesc.9030         = "NETGEAR WNA1100 N150 Wireless USB Adapter"
NTGR.DeviceDesc.9018         = "NETGEAR WNDA3200 Wireless 11N Dual-band USB Adapter"
DLINK.DeviceDesc.3A10        = "High-Power Wireless 150 USB adapter"
AZWV.DeviceDesc.3327         = "Qualcomm Atheros AR9271 Wireless Network Adapter"
AZWV.DeviceDesc.3328         = "Qualcomm Atheros AR9271 Wireless Network Adapter"
AZWV.DeviceDesc.3346         = "Qualcomm Atheros AR9271 Wireless Network Adapter"
AZWV.DeviceDesc.3348         = "Qualcomm Atheros AR9271 Wireless Network Adapter"
AZWV.DeviceDesc.3349         = "Qualcomm Atheros AR9271 Wireless Network Adapter"
AZWV.DeviceDesc.3350         = "Qualcomm Atheros AR9271 Wireless Network Adapter"
AZWV.DeviceDesc.3390         = "Qualcomm Atheros AR9271 Wireless Network Adapter"
AZWV.DeviceDesc.3391         = "Qualcomm Atheros AR9271 Wireless Network Adapter"
SMC.DeviceDesc.A704          = "SMC Networks EZ Connect N 802.11n Wireless USB 2.0 Adapter"
VIA.DeviceDesc.3801          = "VIA 802.11b/g/n USB Wireless Network Adapter"
VRZN.DeviceDesc.1200         = "Verizon Wireless N 300 USB Adapter"
ACTION.DeviceDesc.4500       = "Actiontec Wireless N 300 USB Adapter"
LITEON.DeviceDesc.9271       = "Qualcomm Atheros AR9271 Wireless Network Adapter"
CENT.DeviceDesc.4700         = "Centurylink Wireless N 300 USB Adapter"
